{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":40,"n_cols":12,"rows_kept":40,"merged":[[0,0,0,11],[1,0,1,11],[36,0,36,8],[37,0,37,8],[38,0,38,8],[39,0,39,8]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2023年9月电气备件采购项目                    项目编号：HGJY-G2023155"]
["序号","资材编号","资材名称","规格描述","技术参数","执行标准","单位","数量","申请部门","交货期","含税单价（元）","生产厂家"]
[1,5300100406,"控制变压器","BK-4000VA380/220V",null,"GB/T18494.1-2001","台",2,"物流中心","2023-12-11"]
[2,6100100224,"中频炉变压器","ZP-300-BYQ","功率300千瓦，变比20：2  电压1200伏，中频谐振电流1500安  尺寸800x500x450mm 水压≥0.3MPa","GB/T18494.1-2001","台",1,"219厂部","2023-12-11"]
[3,4100400292,"电缆桥架","50*50*1.0  宽*高*厚   单位：mm","材质：镀锌钢板，线槽与盖板同长，配相应数量的连接板和螺丝","GB/T 5117-1995","米",100,"219厂部","2023-12-11"]
[4,4100400293,"电缆桥架","100*75*1.0   宽*高*厚  单位：mm","材质：镀锌钢板，线槽与盖板同长，配相应数量的连接板和螺丝","GB/T 5117-1995","米",100,"219厂部","2023-12-11"]
[5,6400600554,"激光测距传感器","O1D100-O1DLF3KG","18...30 DC，量程10 m   2 个开关输出；可将其中一个编程为4-20mA输出，使用寿命 [h]50000   安装附件：M12 5Pins输出插头或者插头线","IEC 61131-2","只",1,"219厂部","2023-12-11"]
[6,6100500418,"固态继电器","GJH25-W-3P","负载电流25A，负载电压380V/AV，控制电压3-32V/DC","GB/T 36640-2018","个",3,"检验检测中心","2023-12-11"]
[7,6400400173,"编码器","A860-2005-T301","A860-2005-T301T321；适用于αiF系列电机","MIL-STD-1835","个",1,"检验检测中心","2023-12-11"]
[8,6100500419,"继电器","LY4N-J","DC24V，带底座","IEC255","套",3,"检验检测中心","2023-12-11"]
[9,6100500420,"功率继电器","G2RL-1-CN","DC24V","IEC61810  GB/T 21711.1","个",5,"检验检测中心","2023-12-11"]
[10,6400200107,"光电开关（面积传感器）","A90-4N-R/E","检测区域:80mm 最小检测目标：直径12mm 接收器与发射器之间安装距离：0.3--6米  响应时间：20ms  输出：NPN  PNP各一  电源：DC24V  带极性保护  环境温度：-10--50℃  电缆线长5米","Q/3204BCK010-2013","套",5,"219厂部","2023-12-11"]
[11,6400600559,"液位传感器","G-NS-AM-K10","翻板式液位计NS10/25 AM-K10-SK166/1200配套液位传感器","GB/T14048","件",2,"89热轧","2023-12-11"]
[12,6400600079,"内置式位移传感器","BTL5-S172-M0500-B-KA05","检测长度500mm 配磁环","GB/T28857-2012","只",2,"炼钢厂部","2023-12-11"]
[13,6100900081,"平车电动机控制箱","XKP-2/5Kw","控制单相电容起动电动机；电机功率最大：5Kw; 输入电压：交流380V；配套电机型号：单相电容电动机;YDYP-21-6;5Kw;380V;40uF;17.7A;负载持续率40%;F级","JB14048.6","箱",1,"340热轧","2023-12-11"]
[14,6100200007,"电动隔离开关 合闸机构","3DC1026-5E 德国IEC947","额定工作电压36KV 额定电流2000A 控制电压AC220V 辅助触点4NO+4NC","德国IEC947","套",1,"炼钢厂部","2023-12-13"]
[15,6300700072,"综合显示大屏","BCD4P-AN2P-176","VOITAGE:100-240VAC/50-60HZ","Q/IBRF7-2013","台",1,"炼钢厂部","2023-12-11"]
[16,6300700077,"高压变频触摸屏控制器","PECS41-L","电源24VDC、500mA;通讯卡ABS-ETN10/100;冷却方式;风冷","T/SCSKJQYLHH 08-2021","台",1,"炼钢厂部","2023-12-11"]
[17,6500400228,"开关电源","LM350-10B05 5V","输入：200-220V~4A 50/60Hz  输出：5V 60A 功率(W): 300","GB/T9813-2000","个",5,"炼铁厂部","2023-12-11"]
[18,6100900161,"防爆电气控制箱","600*800*250；380V；铸铝材质","380V","JB14048.6","台",2,"炼铁厂部","2023-12-11"]
[19,6200200942,"水处理人机界面","HMIGXU3500","DC24V 5.4W Class2;带操作画面内容","GB50252-2010","台",1,"能源厂部","2023-12-11"]
[20,6200300110,"变频器整流模块","KBPC3510","Vrrp:1000VIf:35A","DL/T2033-2019","块",1,"炼钢厂部","2023-12-11"]
[21,6300200196,"profinet远程IO模块","VM3209C","16路AI;AI信号输入范围0-20mA","GB/T25105","块",1,"炼钢厂部","2023-12-11"]
[22,6300200197,"分布式总线IO模块","HJ5207","2DI数字量输入;支持Profinet协议;Modubs TCP;外带2路光电隔离485转profinet;额定电压DC24V","GB/T25105","块",1,"炼钢厂部","2023-12-11"]
[23,7502500112,"风机","HD9F-FAN-560-560","输入3PAC380V","GB/T22712-2008","台",1,"炼钢厂部","2023-12-11"]
[24,7502500113,"风机","HD9FS-FAN-400A-400","输入3PAC380V","GB/T22712-2008","台",1,"炼钢厂部","2023-12-11"]
[25,6200200918,"功率单元","HD9MS-A069-0061-500000","输入3PAC690V;输出2PAC690V/0-50HZ;输出电流61A","DL/T2033-2019","台",1,"炼钢厂部","2023-12-11"]
[26,6200200919,"功率单元","HD9M-A069-0340-50000CT03","输入3PAC690V;输出2PAC690V/0-50HZ;输出电流340A","DL/T2033-2019","台",1,"炼钢厂部","2023-12-11"]
[27,6200200886,"数字式（可控硅换向）调压调速装置","THYROMAT 10BCCH1200A 380BNZ-A","供电电压380-415V;3相50Hz;控制电压220V;单相50Hz;额定电流1200A;起升机构应用","GB/T3235-1999","台",1,"炼钢厂部","2023-12-11"]
[28,4100700169,"工业语音声光报警器","TGSG--110","AC220V，LED频闪发光，警灯颜色为红色，110分贝，防护等级：IP54，报警音调：定制（机车正在作业，禁止其他作业）循环播放","GB14048.5-2008","台",5,"340热轧","2023-12-11"]
[29,6400600556,"连接器","423 99 5621 00 06 公头","6针;5.0A;250V AC/DC;IP67;binder","QB/T 2442.1-2007","个",10,"180热轧","2023-12-11"]
[30,6400600557,"连接器","423 99 5622 00 06 母头","6孔;5.0A;250V AC/DC;IP67;binder","QB/T 2442.1-2007","个",10,"180热轧","2023-12-11"]
[31,6000300266,"冷却风机","G132-1734 ;60W","电压380V; 转速2800r/min; 50HZ; NO.11020502","GB14711-2006","台",2,"180热轧","2023-12-11"]
[32,4000200371,"AC36V工业插头","插头;CEE-012 ；电压等级36VAC，",null,"GBT 11918-2014","个",20,"219厂部","2023-12-11"]
[33,4000200372,"AC36V工业插座","插座：CEE-312；16A；电压等级36VAC",null,"GBT 11918-2014","个",5,"219厂部","2023-12-11"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2023年9月电气备件采购项目         项目编号：HGJY-G2023155"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}