{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":41,"n_cols":13,"rows_kept":41,"merged":[[0,0,0,8],[1,0,1,12],[37,0,37,8],[38,0,38,8],[39,0,39,8],[40,0,40,8]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2023年9月机械备件采购项目                     项目编号：HGJY-G2023157"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,7101800139,"气动球阀","DN80 ANSI 300 ASMEB16.5","铸钢 F30，CL300，AIR TO CLOSE，ASTM A479，TYPE316，TFM-1600","只",2,null,"高辅工段","2023-11-26"]
[2,5500500034,"离心通风机","NGP300A","540m3/h,全压2156Pa;电机0.75Kw;2900r/min","台",1,"GB/T14048","高辅工段","2023-11-26"]
[3,7001200011,"高压泵 除磷环喷嘴紫铜垫","*",null,"只",50,"JB/T9872-2000","340热轧","2023-11-26"]
[4,5100100425,"离心水泵六爪弹性圈","IS100-65-200","外径110，内径50，六爪弹性水泵弹性体","只",10,"JB/T7511-1994","能源厂部","2023-11-26"]
[5,5501400036,"烧结;A1筛筛板(一)","HBS2050(TTHBS-450-1)-a","上层棒条直径16mm，长度270mm，间距16mm；下层棒条直径13mm，长度320mm，间距12mm；棒条材质HBZL-5CrSiV；棒条布置角度18°","件",1,null,"烧结","2023-11-26"]
[6,5501000054,"碎焦振动筛","XHSZ1530","含激振器激振器ZDS6-6，箱体材质20g，滚动轴承采用哈、瓦、洛原厂正品，衬板采用耐磨陶瓷衬板，焊接部件不允许有漏焊、夹渣、咬边、气孔现象","台",1,"审核图纸","高辅工段","2023-11-26"]
[7,5501000065,"焦炭筛聚氨酯筛板","GY20220127-CX","介质：焦炭，材质：聚氨酯，使用寿命3个月处理能力300吨/小时。包含整套焦炭筛所用聚氨酯HW筛板和聚氨酯HW筛板托架。槽下全套筛板由16块高弹悬浮面小筛板","套",1,"审核图纸","高辅工段","2023-11-26"]
[8,7102200003,"遥控浮球阀用浮球和导阀","G1/2",null,"台",2,"QB/T1199-1991","180管加工热处理","2023-11-26"]
[9,7001200344,"高压柱塞泵;TJ03-01加TJ03K.02.00","TJ03-01加TJ03K.02.00，包含整套联轴器，流量415 立方米/H",null,"台",2,null,"340热轧","2023-11-26"]
[10,7101800130,"气动球阀","DN150 ANSI 300 ASMEB16.5","铸钢 F30，CLASS ANSI300，ASTMA216WCB，A351 CF8M，STAINLESS316，ANSI 300 ASMEB16.5","只",1,null,"高辅工段","2023-11-26"]
[11,5502000011,"低压脉冲袋式除尘器;骨架","直径124*5930","标准件 GB13871-1992","只",200,null,"高辅工段","2023-11-26"]
[12,7101800256,"气动球阀","Q641H-25P-65","PN25;DN65;介质:蒸汽;带DC24V气动电磁换向阀及回迅器","只",2,"GB12237-1989","炼钢厂部","2023-11-26"]
[13,5722600120,"锯床导向臂","导向臂长535，上宽110，下宽75","G4240/50锯床专用","台",2,"JB/T 4318.4-2002","180管加工热处理","2023-11-26"]
[14,5400300008,"煤气冷凝水排水器","SDLT-4000-100","Q235 GB6222","台",5,"GB6222","能源厂部","2023-11-26"]
[15,7501300118,"波纹补偿器","SDZ21810I-1000","通径：DN1810，总长1000，钢管壁厚12，双层波纹管，内层材质254SMO外层材质316L不锈钢，单层波纹管厚度0.8mm；工作温度：250℃；工作压力：0.25MPa；补偿量：轴向 50mm，横向50mm；介质：高炉煤气，两端开焊接式坡口","只",1,"GB/T12777-1999","能源厂部","2023-11-26"]
[16,7102100012,"气动控制阀门","D376XE71",null,"只",5,"ISO5211","720厂部","2023-11-11"]
[17,7502500111,"热风炉助燃风机调节门","ST0108.12，左旋","重量：186Kg","套",1,"审核图纸","高炉","2023-10-12"]
[18,7101900074,"中型常闭气控保压阀","60-11HF9-MPO","316SS不锈钢材质，最大驱动空气压力：100psi; 最大工作压力:60000psi;气源接头尺寸：1/8 NPT；阀座用于连接9/16'' 高压钢管","件",1,"EN/TEC60947-4-2(2020)","检验检测中心","2023-11-26"]
[19,5900100017,"车床中拖板丝杆铜螺母","BK10","长*宽：67mm*43mm 槽宽：16mm ;材质为：铅黄铜，已适配安装打孔;适用CYPMU660/3000车床","套",1,"JB/T3241-2005","检验检测中心","2023-10-12"]
[20,5900100015,"英思特朗150吨拉伸机夹具抗磨板","英思特朗拉伸机专用夹具抗磨板225906-1","一套共上下左右四块;1500MDX-G7B英思特朗1500KN万能试验机夹具抗磨板","套",1,"ASTM A370","检验检测中心","2023-10-27"]
[21,5900100016,"英思特朗150吨拉伸机夹具底座","英思特朗拉伸机专用夹具底座222712-3","1500MDX-G7B英思特朗1500KN万能试验机夹具底座；一套共上下左右四块","套",1,"ASTM A370","检验检测中心","2023-10-27"]
[22,5800100037,"碟形弹簧","φ63×φ31×4.9","D63(φ63×φ31×4.9 )，材质：弹簧钢60Si2MnA；A型","件",200,"GB/T1972-92","炼钢厂部","2023-11-26"]
[23,5500400112,"渣浆泵;后泵体","100YTZX-560","HT200 带配套螺栓","件",1,"JB/T8096-2013","高炉","2023-10-07"]
[24,7501300122,"膨胀节","DN442X14-300/F","补偿量30mm，长度300mm，双层波纹管：内层材质254SMo、外层材质316L不锈钢，厚度均为0.8mm；导流管材质：316L不锈钢，厚度5mm；工作温度：250℃；工作压力：250KPa；介质：高炉煤气；一端带法兰另外一端焊接式接头；带配套金属包覆垫","套",1,"GB/T12777-1999","高炉","2023-10-12"]
[25,7501300123,"膨胀节","DN752X16-400/F","补偿量30mm，长度400mm，双层波纹管：内层材质254SMo、外层材质316L不锈钢，厚度均为0.8mm；导流管材质：316L不锈钢，厚度5mm；工作温度：250℃；工作压力：250KPa；介质：高炉煤气；一端带法兰另外一端焊接式接头；带配套金属包覆垫","套",2,"GB/T12777-1999","高炉","2023-10-12"]
[26,7500300017,"板式换热器","BR0.1-5","法兰DN25，换热面积5㎡，压力1.6MPa","台",1,null,"高辅工段","2023-10-12"]
[27,4201300047,"滚珠丝杆","TDB-U-8020-9-6-2600-3583-ISO3",null,"套",1,"ISO 9001:2015","180热轧","2023-11-26"]
[28,4201300048,"滚珠丝杆","TDB-S-6310-6-6-1200-1672-ISO3",null,"套",1,"ISO9001:2015","180热轧","2023-11-26"]
[29,5722100063,"排气密封座","PT340.80HL-09.03","材质40CrNi2Mo，  重4240kg","件",1,"审核图纸","340管加工热处理","2023-11-26"]
[30,7502300038,"500~600足辊水喷嘴","1/4PZ3195B6","材质:黄铜;最大喷射角度95°;等效孔径1.8mm","只",200,"JB/T 12492-2015","炼钢厂部","2023-10-12"]
[31,7502300039,"700~800足辊水喷嘴","1/4PZ3110B6","材质:黄铜;最大喷射角度110°;等效孔径2.4mm","只",200,"JB/T 12492-2015","炼钢厂部","2023-10-12"]
[32,5602600066,"单倍尺割嘴","GKSD5-16","天然气;割嘴螺纹M36*2;喉径5.8;切割速度50-600mm/min;割缝宽度12~25mm;切割厚度≤1200mm","只",20,"GB5108-1985","炼钢厂部","2023-10-12"]
[33,7001500012,"罗茨真空泵","DDR4500","\"额定能力4500m3/h(50HZ);极限真空0.05 Pa;冷却形式;整体式夹套水冷;配套西门子变频电机;电机功率22Kw;转速2935r/min;入口连接DN200/PN16/RF\n出口连接DN200/PN16/R\"","台",1,"Q/SOEU17-2007","炼钢厂部","2023-10-27"]
[34,5601700034,"列管式热交换器","DSN039458","材质:304SS管","件",1,"审核图纸","炼钢厂部","2023-10-27"]
["注：1、投标报价含税，税率13%                                                                                     \n2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2023年9月机械备件采购项目           项目编号：HGJY-G2023157"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]