{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":43,"n_cols":12,"rows_kept":43,"merged":[[0,0,0,11],[1,0,1,11],[39,0,39,8],[40,0,40,8],[41,0,41,8],[42,0,42,8]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2023年10月电气备件采购项目                    项目编号：HGJY-G2023170"]
["序号","资材编号","资材名称","规格描述","技术参数","执行标准","单位","数量","申请部门","交货期","含税单价（元）","生产厂家"]
[1,6400200107,"光电开关（面积传感器）","A90-4N-R/E","检测区域:80mm 最小检测目标：直径12mm 接收器与发射器之间安装距离：0.3--6米  响应时间：20ms  输出：NPN  PNP各一  电源：DC24V  带极性保护  环境温度：-10--50℃  电缆线长5米","Q/3204BCK010-2013","套",5,"219厂部","2023-12-27"]
[2,6400600559,"液位传感器","G-NS-AM-K10","翻板式液位计NS10/25 AM-K10-SK166/1200配套液位传感器","GB/T14048","件",2,"89热轧","2023-12-27"]
[3,6100200007,"电动隔离开关 合闸机构","3DC1026-5E 德国IEC947","额定工作电压36KV 额定电流2000A 控制电压AC220V 辅助触点4NO+4NC","德国IEC947","套",1,"炼钢厂部","2023-12-27"]
[4,6100300302,"固定式断路器","HD4s-40.5MX-1600A-25kA","额定电压40.5KV;额定频率50Hz;额定电流1600A;3秒热稳定电流（有效值）25kA;额定动稳定电流（峰值）63kA;额定短路开断电流25kA;额定短路关合电流63kA;辅助电源电压;控制回路DC220V;储能电机DC220V;合闸时间55-67ms;分闸时间33-45ms;燃弧时间＜15ms;合闸弹跳时间≤2mS;机械循环寿命10000次;电气循环寿命符合E2级规定;ABB","GB1984-2001","台",1,"炼钢厂部","2023-12-27"]
[5,6200200942,"水处理人机界面","HMIGXU3500","DC24V 5.4W Class2;带操作画面内容","GB50252-2010","台",1,"能源厂部","2023-12-27"]
[6,7502500112,"风机","HD9F-FAN-560-560","输入3PAC380V","GB/T22712-2008","台",1,"炼钢厂部","2023-12-27"]
[7,7502500113,"风机","HD9FS-FAN-400A-400","输入3PAC380V","GB/T22712-2008","台",1,"炼钢厂部","2023-12-27"]
[8,6200200918,"功率单元","HD9MS-A069-0061-500000","输入3PAC690V;输出2PAC690V/0-50HZ;输出电流61A","DL/T2033-2019","台",1,"炼钢厂部","2023-12-27"]
[9,6200200919,"功率单元","HD9M-A069-0340-50000CT03","输入3PAC690V;输出2PAC690V/0-50HZ;输出电流340A","DL/T2033-2019","台",1,"炼钢厂部","2023-12-27"]
[10,6100300267,"真空断路器手车","3AH4305-2Z/1250-31.5","额定电压40.5KV;额定电流1250A;额定短路开断电流31.5KA;额定短时耐受电流4S:31.5KA;1分钟工频耐受电压95KV;重量170kg;tk;3S;MADE IN GERMANY","德国IEC947","台",1,"炼钢厂部","2023-12-27"]
[11,6400400174,"SSI隔离器","HXEC-1002-SSI","供电电源18-32VDC;100mA;输入输出型号类型SSI;信号保护：防雷、过流保护，信号箝位保护; 500Kbps; iCoupler磁隔离; 绝缘强度1500V AC/1min","EC1002","个",10,"180热轧","2023-11-27"]
[12,6400200024,"光电开关","WL24-2B240",null,"GB/T 18901.1-2002","只",5,"89油管车丝委外","2023-12-27"]
[13,4000200371,"AC36V工业插头","插头;CEE-012 ；电压等级36VAC，",null,"GBT 11918-2014","个",15,"720厂部","2023-10-28"]
[14,4000200372,"AC36V工业插座","插座：CEE-312；16A；电压等级36VAC",null,"GBT 11918-2014","个",50,"720厂部","2023-10-28"]
[15,4100400297,"电缆中间接头铜连接管","35mm2","T2紫铜,?铜接管长度67mm","JB/T7435","个",20,"能源厂部","2023-11-27"]
[16,4100500405,"薄膜按键","YX-WK/HFD 4*4","长11.2cm 宽8cm；PET银浆印刷线路；触点抖动时间小于5ms；金属弹片型；使用寿命50万次；","JB/T5405-91","个",2,"检验检测中心","2023-11-12"]
[17,4100700196,"晶闸管","MTC110A/2200V","额定电流110A;耐压2200V","GB/T17761-2018","个",10,"炼钢厂部","2023-11-12"]
[18,6100200056,"电动机操动机构","CJ2-C","主轴转角90度;电机功率0.37Kw;控制电压AC220V;操作时间4S;电机电压AC/DC220V;额定电流2.6A","JB/DQ2553-1989","台",1,"炼钢厂部","2023-11-27"]
[19,6100200057,"电动机操作机构","CJ6BW","主轴转角90°;电机功率0.37Kw;控制电压DC220V;操作时间4S;电机电压AC380V;额定电流1.3A","GB755-2008","台",1,"炼钢厂部","2023-11-27"]
[20,6100200058,"隔离开关","GN2-35D/1250-31.5","额定电压35KV;额定电流1250A;热稳定电流31.5KA","GB/T6170-2000","台",1,"炼钢厂部","2023-11-27"]
[21,6100300308,"真空断路器手车","3AH4305-2/1250-31.5","额定电压40.5KV;额定电流1250A;额定短路开断电流31.5KA;额定短时耐受电流3S:31.5KA;1分钟;Ud/Up95/195KV;额定操作顺序O-0.3S-CO-3min-CO","IEC62271-100","台",1,"炼钢厂部","2023-11-27"]
[22,6100400407,"行车用（一体化无触点）正反转装置","TDE-300A-3PJ-2N","电源AC380V；无触点通断；正反转延时保护，缺相、过流保护；智能风扇散热，电流实时显示。","GB14048.4-2003","只",1,"物流中心","2023-11-27"]
[23,6100500423,"继电器","DRI424024LD","线圈电压DC24V","EN60204-1","只",20,"炼钢厂部","2023-11-27"]
[24,6100500424,"继电器","DRI424730LT","线圈电压AC230V","EN60204-1","只",20,"炼钢厂部","2023-11-27"]
[25,6100800021,"复合绝缘金属氧化物避雷器","YH5WZ-51/134","系统额定电压35KV（rms）; 避雷器额定电压51KV（rms）; 标称放电电流5KA;下残压不大于134KV","GB11032","组",1,"炼钢厂部","2023-11-27"]
[26,6100800023,"三相组合式过电压保护器","RTB-Z-12.7KV/130","持续运行电压 12.7KV;出厂编号11020252","JB/DQ2553-1989","台",1,"180热轧","2023-11-27"]
[27,6200200944,"软启动器","ATS48C17Q","电源电压230-415V;额定功率90Kw;额定电流170A;防护等级IP00","EN/IEC60947-4-2","台",1,"炼钢厂部","2023-11-27"]
[28,6300500277,"双电源自动转换开关","WATSG400/3M","Ue;AC50Hz;400V;Ie;400A;Uimp;8KV,Ui;1000V;Icw;17kA/ms;Icm;24kA","GB/T14048.11","只",1,"炼钢厂部","2023-11-27"]
[29,6300600071,"手持式喷标机","DRA280","字符高度：20 mm─48 mm，字符点阵：16点，标记颜色： 白色涂料，喷印字符种类：英文、汉文、数字等计算机能编辑的任意字符和图形，喷印大小写字母可直接喷印无须将其制作成特殊字符，标号方式： 点阵式  ７×５，1０×８、1２×８、1４×1０、1６×1２等多种，采用标准字体(GB标准)，字体（符）和大小可自由选择编辑。一组喷印内容字符个数不低于200个。能内存1000条，不同的喷印内容，能方便调出。字体美观、清楚。每组(条) 喷印内容的间距、位置和组数能任意选择，","SGS","台",1,"89包装","2023-11-27"]
[30,6300700079,"喷标控制柜电源","C-16 P 25","INPUT:176-264V/3.5A max,50/60Hz;OUTPUT:+250V,1.2A","JB/T8679-1998","个",4,"340热轧","2023-10-28"]
[31,6400400176,"编码器","8.5821.1531.1024.9083","8~30VDC;40mA;S.Nr1116706011;kübler","DIN32878-1993","个",1,"180热轧","2023-11-27"]
[32,6400500924,"交流电压变送器","YDD-U","input;AC0V-100V;output;DC0V-10V;POWER;DC20V-60V","GB/T13978-1992","台",1,"炼钢厂部","2023-11-27"]
[33,6400600561,"工业级激光测距传感器","XW-DD3-E30-A","信号4-20mA/RS232;量程0.05-30m","Q/RG2003-2013","台",1,"炼钢厂部","2023-11-27"]
[34,6400600562,"位移传感器","RHM2200S1PU02A01","\"内置式;有效行程2200mm;螺纹M18*1.5;航\n空插头出线带2米欧标电缆;信号4-20毫安\"","GB/T14048","台",1,"炼钢厂部","2023-11-27"]
[35,6400600563,"位移传感器","RHM0260S1DU02A01","\"内置式;有效行程260mm;螺纹M18*1.5;航\n空插头出线带2米欧标电缆;信号4-20毫安\"","GB/T14048","台",1,"炼钢厂部","2023-11-27"]
[36,6600300168,"电动执行机构","M8320","电机功率：0.46KW,额定电流：1.42A，电源电压：380V/3PH 50HZ,防护等级：IP67，力矩120NM，行程/速度：36rpm，连接F10","JB/T8219-1999","台",1,"能源厂部","2023-11-27"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2023年10月电气备件采购项目      项目编号：HGJY-G2023170"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}