{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":54,"n_cols":12,"rows_kept":54,"merged":[[0,0,0,11],[1,0,1,11],[50,0,50,8],[51,0,51,8],[52,0,52,8],[53,0,53,8]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2023年11月电气备件采购项目                    项目编号：HGJY-G2023182"]
["序号","资材编号","资材名称","规格描述","技术参数","执行标准","单位","数量","申请部门","交货期","含税单价（元）","生产厂家"]
[1,6200200376,"逆变器","20DH500NOENNBNANE AB","输入电压：540V直流 输入电流：589A 输出电压：0-400V 输出电流：500A 输出频率：三相，0-320HZ 一般负载:250KW Frame:10",null,"台",1,"219厂部","2023-12-27"]
[2,6200200206,"变频器","20G11NC104JA0NNNNN 55Kw PowerFIex755","进线电压：3相 380V-480VAC 额定功率55KW 重载功率45KW 额定电流104A",null,"台",1,"219厂部","2023-12-27"]
[3,6300500226,"POINT I/O模块底座","1734-RTB+1734-TB;AB","导轨安装","IEC 60068-2-1","套",10,"219厂部","2023-12-27"]
[4,6300400003,"Piont I/0 SSI电源模块","1734-EP24DC AB","直流24V 标准IEC61508",null,"块",5,"219厂部","2023-12-27"]
[5,6300300040,"通讯模块","1734-AND AB","标准IEC61508",null,"块",5,"219厂部","2023-12-27"]
[6,6300300037,"控制网SSI通讯模块","1734-ACNR DC24V AB 60068-2-1","标准IEC 60068-2-1",null,"块",5,"219厂部","2023-12-27"]
[7,6300300017,"Piont I/O SSI计数模块","1734-SSI AB","绝对值计数，SSI输入 标准IEC 60068-2-1","IEC 60068-2-1","块",10,"219厂部","2023-12-27"]
[8,6200200216,"变频器","20BC085A0AYNANC0 E0.967X","45Kw 85A 400VAC","E0.967X","台",2,"219厂部","2023-12-27"]
[9,6200100093,"变频器","MD480T37GB","37KW","EN61800-3","台",5,"219厂部","2023-12-27"]
[10,6300100129,"CPU模块","1756-L81E","1756-L81E","IEC61508","块",2,"219厂部","2023-12-27"]
[11,4100500405,"薄膜按键","YX-WK/HFD 4*4","长11.2cm 宽8cm；PET银浆印刷线路；触点抖动时间小于5ms；金属弹片型；使用寿命50万次；","JB/T5405-91","个",2,"检验检测中心","2023-12-27"]
[12,6200300076,"电热电容器","RFM 0.751000-1S","CN 283UF UN750V FN 1000HZ  IN1333A   水流量6L/MIN","JB/T 7110-1993","台",2,"89油管车丝委外","2024-01-26"]
[13,6200300113,"感应加热电源","HXKPS-300KW/1-2.5KHZ","进线电源630V,50HZ,中频频率1-2.5KHZ，中频电压0-1275KV可调,功率300KW,可控硅垂直安装，外配谐振电容与300KW加热器一套，柜体尺寸1200*950*2000。","GB/T7676.1-9","套",1,"89油管车丝委外","2023-12-27"]
[14,6200300114,"感应加热炉","GTR-90-Ⅰ","孔径Φ90，300Kw，2500HZ ，1275V，水冷 ，600*400*600 ，分左右接线","审核图纸","台",3,"89油管车丝委外","2023-12-27"]
[15,6200300116,"感应加热炉","GTR-100-Ⅰ","孔径φ100，300Kw，2500Hz ，1275V，水冷，600*400*600，分左右接线","审核图纸","台",3,"89油管车丝委外","2023-12-27"]
[16,6200300115,"感应加热炉","GTR-130-Ⅰ","孔径φ130，300Kw，2500Hz ，1275V，水冷，600*400*600，分左右接线","审核图纸","台",3,"89油管车丝委外","2023-12-27"]
[17,6400600177,"温度继电器","ETS388-5-150+TFP100+S.S+ZBE08+ZBM300","测量范围0-100℃ 精度等级正负1% 4个开关量输出带换向触点，1个模拟输出4-20mA 耐振，耐冲击",null,"只",2,"180厂部","2023-12-27"]
[18,6200200899,"制动电阻","3kW/18R","配CS710-4T30GB变频器，电阻值:18R,制动功率:3kW","IEC61800","台",2,"炼铁厂部","2023-12-27"]
[19,8700800023,"PMC机床 定心臂轮子","*",null,"JB/T3588-2007","件",12,"340管加工车丝","2023-12-27"]
[20,6000201084,"高频电源冷却风机","W2E250—HL06-01","AC 230V  50Hz  0.66A  127W","JB/T10391-2002","台",10,"炼铁厂部","2023-12-27"]
[21,5100300084,"抱闸电控箱","EXE800一2E","输入交流380V；\n输出直流65V；启动12V;维持\n瞬间启动电流36A,功率2500W;\n维持电流6.7A,功率100W\"","JB14048.11","台",1,"340热轧","2023-12-27"]
[22,6400600555,"传感器7针插头","No.560701+530029 D70  带25米线","No.560701+530029 带线25米线; MTS 灰数据（-） 粉红数据（+） 黄时钟（-） 绿时钟（-） 棕+24VDC(-15/+20%) 白电源地 M16mm连接器接口。","IEC60176-2-106-2011","根",5,"180热轧","2023-12-27"]
[23,4000300255,"电缆桥架盖板","2000mm*100mm*1.5mm（长*宽*厚）","材质：镀锌钢板","GB/T 5117-1995","米",40,"180热轧","2023-12-27"]
[24,4000300256,"电缆桥架盖板","2000mm*200mm*1.5mm（长*宽*厚）","材质：镀锌钢板","GB/T 5117-1995","米",40,"180热轧","2023-12-27"]
[25,6000300265,"电机抱闸整流器","RH555","555V ;2A;输入380V,输出直流220V；UHT","GB3859-93","个",3,"180热轧","2023-12-27"]
[26,7502500112,"风机","HD9F-FAN-560-560","输入3PAC380V","GB/T22712-2008","台",1,"炼钢厂部","2023-12-27"]
[27,7502500113,"风机","HD9FS-FAN-400A-400","输入3PAC380V","GB/T22712-2008","台",1,"炼钢厂部","2023-12-27"]
[28,6200200918,"功率单元","HD9MS-A069-0061-500000","输入3PAC690V;输出2PAC690V/0-50HZ;输出电流61A","DL/T2033-2019","台",1,"炼钢厂部","2023-12-27"]
[29,6200200919,"功率单元","HD9M-A069-0340-50000CT03","输入3PAC690V;输出2PAC690V/0-50HZ;输出电流340A","DL/T2033-2019","台",1,"炼钢厂部","2023-12-27"]
[30,4000200309,"电源滑线导杆","800A；345205；橙色",null,"GB/T 14966-1994","根",30,"炼铁厂部","2023-12-27"]
[31,6400600562,"位移传感器","RHM2200S1PU02A01","\"内置式;有效行程2200mm;螺纹M18*1.5;航\n空插头出线带2米欧标电缆;信号4-20毫安\"","GB/T14048","台",1,"炼钢厂部","2023-12-27"]
[32,6400600563,"位移传感器","RHM0260S1DU02A01","\"内置式;有效行程260mm;螺纹M18*1.5;航\n空插头出线带2米欧标电缆;信号4-20毫安\"","GB/T14048","台",1,"炼钢厂部","2023-12-27"]
[33,6100300261,"高压断路器","VS1-ZN63A 2500A","短路持续时间4S，短路断开电流31.5KA；电压等级10KV,操作电压DC220V",null,"台",1,"炼铁厂部","2023-12-27"]
[34,6400600177,"温度继电器","ETS388-5-150+TFP100+S.S+ZBE08+ZBM300","测量范围0-100℃ 精度等级正负1% 4个开关量输出带换向触点，1个模拟输出4-20mA 耐振，耐冲击",null,"只",1,"340管加工热处理","2024-01-11"]
[35,7101500108,"电动隔离装置","ADE-LDRX-DZGL","高温型,DN80，快开型6S，电源：220VAC；干接点输出","GB/T21385-2008","台",1,"炼铁厂部","2023-12-27"]
[36,6400400177,"编码器","XHI 803, part no:770594-01","supply:9-30Vdc, Output:1024 ppr HCHTL,Connection type:Cable gland,Connecting direction:Adjustable,leine linde","IEC 61010","个",1,"720厂部","2024-01-26"]
[37,6100100230,"出线电抗器","YFSDK-5A/5V","额定电流5A;额定电压5V","GB10229-88","台",1,"炼钢厂部","2023-12-27"]
[38,6100100231,"出线电抗器","MC0-18/1","电流18A;电感710uH;频率50Hz","GB10229-88","台",1,"炼钢厂部","2023-12-27"]
[39,6100100232,"出线电抗器","MC1-15/2","电流15A;电感939uH;频率50Hz","GB10229-88","台",1,"炼钢厂部","2023-12-27"]
[40,6000300254,"多合一智能电动机转子控制器","RSC1-M1-160R1-3","转子额定开路电压≤AC500v;用于三相交流电动机3段转子电阻器的控制","GB/T3235-1999","台",1,"炼钢厂部","2023-12-27"]
[41,6200200887,"数字式（可控硅换向）调压调速装置","THYROMAT 10BCCH200A 380BNZ-A","供电电压380-415V;3相50Hz;控制电压220V;单相50Hz;额定电流200A;电机定子电流143A-181A;升机构应用","GB/T3235-1999","台",1,"炼钢厂部","2023-12-27"]
[42,6100900083,"BCM数字式吸盘控制装置","BCM 140A 220BS","140A  220V","GB/T3235-1999","台",1,"炼钢厂部","2023-12-27"]
[43,6100900171,"弧形辊道一段成套电气变频柜","辊道成套变频柜MD480T5.5GB-PLUS-10","柜体尺寸800*2200*800?仿威图；内含汇川变频器MD480T5.5GB-PLUS?10台；交流塑壳断路器NSX160F?TMD?160?3P3D?F?总开关1个；iC65N-D16A/3P?10个；输入/出电抗器ACL-15/OCL-15各10个；柜内元器件接线配好到端子排，附图纸。","GB/T12668.2-1989","套",1,"340热轧","2023-12-27"]
[44,6000300275,"车床风机","RF22P-2DK.3F.5R","ZEHL-ABEC；131510\t07222412；- 400V ±10% Y 50Hz P10 0.80A DI=0% 2320/MIN COSY；- 400V ±10% Y 60Mz P10.1,1A DI=0% 2230/MIN COSY.D PeF min.470PA；-480V ±10% Y 50Mz P10,1.1A Dl=0% 2550MIN COSY 020 PSF min.620PA1P54 THCL155","IEC97-1991","台",2,"340热轧","2023-12-27"]
[45,6200200953,"制动单元","BKBU4075N","75KW，额定电流25A，最大150A； 配11只5KW电阻 ，型号：BKRX20-5KW110RJH，电阻值9.1Ω","GB/T12668.2-1989","套",1,"340管加工热处理","2024-01-27"]
[46,6400200109,"冷探","HS18L-D1G5AA","2080954；10-30V;out<100mA+55C;品牌：SICK","EN 60947-5-2:2007","只",2,"340热轧","2023-12-28"]
[47,6400200110,"冷探","HS18-P1G7BA","2078054；10-30V;out<100mA+70C;品牌：SICK","EN 60947-5-2:2007","只",2,"340热轧","2023-12-28"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2023年11月电气备件采购项目         项目编号：HGJY-G2023182"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]