{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":57,"n_cols":12,"rows_kept":57,"merged":[[0,0,0,11],[1,0,1,11],[53,0,53,11],[54,0,54,11],[55,0,55,11],[56,0,56,11]],"flags":["formulas_cached_only"]}
["    （一）开标一览表"]
["项目名称：2024年1月电动机招标采购项目                    项目编号：HGJY-G2024007"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","交货时间","使用部门","含税单价(元)","生产厂家\n","备注   "]
[1,"5720500046","4#线炉内辊电动机成套","DLR04-179YPG132M-4-4KW-M1-L","电机型号：YPG132m-4;电机额定功率4KW；输出转速179r/min;防护等级IP54","套","3","2024-03-30","180管加工热处理"]
[2,"6000100008","齿轮减速电动机","SK02050-80L/4 0.75Kw 带变频电机","变频电机0.75kw","台","1","2024-03-30","炼钢厂部"]
[3,"6000200389","异步交流电动机","Y90L-2B5","2.2Kw","台","2","2024-03-30","720厂部"]
[4,"6000200631","冶金起重电动机","YZR160M2-6","7.5Kw 双轴","台","2","2024-03-30","炼钢厂部"]
[5,"6000201023","起重及冶金用绕线转子三相异步电动机","YZR355L1-10C;110Kw","定子电压380V;223A;转子电压362V;189A ;S3-40%;H级绝缘;IP54;接法Y;转速586r/min;带超速开关","台","1","2024-03-30","炼钢厂部"]
[6,"6000201073","轧钢辊道电动机","YE4-112M-4E；配DSZR87-60","配DSZR87-60,带小齿轮，功率：4KW;8.7A;额定转速:1445rpm;防护等级:IP55;频率:50HZ;出厂编号：1100027834/4-003;厂家:宁波东力","台","5","2024-03-30","340热轧"]
[7,"6000201115","交流伺服电机","130SJT-M050D(A4II)","输入电压AC220V三相, 额定功率1.5Kw; 额定电流6A ; 额定转矩6NM ; 额定转速2500rpm ; 最高转速3000rpm","台","1","2024-03-30","检验检测中心"]
[8,"6000201116","交流异步电动机","BPYXKK500-6W","功率1250Kw;额定电压6000V;额定电流146A;额定频率50Hz;绝缘等级F级;防护等级IP54;转速990r/min;S1工作制;Y型接法;冷却方式IC616","台","1","2024-03-30","炼钢厂部"]
[9,"6000201129","三相异步电动机","YE4-225S-4","功率37Kw;额定电压380;额定电流69.5A;频率50Hz;额定转速1480r/min;三角形接线方式;防护等级IP55;安装方式B3;S1工作制","台","1","2024-03-30","炼钢厂部"]
[10,"6000201130","三相异步电动机","YE4-280S-4/B35","功率75Kw;额定电压380V;额定电流139.3A;额定转速1480r/min;安装方式B35;防护等级IP55;绝缘等级F级;S1工作制","台","1","2024-03-30","炼钢厂部"]
[11,"6000201131","三相异步电动机","YE4-280M-4/B35","功率90Kw;额定电压380V;额定电流164A;额定转速1485r/min;安装方式B35;防护等级IP55;绝缘等级F级;S1工作制","台","1","2024-03-30","炼钢厂部"]
[12,"6000201132","三相异步电动机","YE4-315S-4/B35","功率110Kw;额定电压380V;额定电流196.3A;额定转速1485r/min;安装方式B35;防护等级IP55;绝缘等级F级;S1工作制","台","1","2024-03-30","炼钢厂部"]
[13,"6000201133","三相异步电动机","YE4-160L-4/B35","功率15Kw;额定电压380V;额定电流28.8A;额定转速1465r/min;安装方式B35;防护等级IP55;绝缘等级F级;S1工作制","台","1","2024-03-30","炼钢厂部"]
[14,"6000201134","高效率变频调速三相异步电动机","YPTX3-315L1-2","功率160Kw;额定电压380V;额定电流279.4A;额定转速2981r/min;安装方式B3;防护等级IP55;绝缘等级F级;S1工作制;频率30-50Hz","台","1","2024-03-30","炼钢厂部"]
[15,"6000201135","变频调速三相异步电动机","XDYSP180L-4","功率22Kw;额定电压380V;额定电流43.7A;额定转速1470r/min;安装方式B3;防护等级IP55;绝缘等级F级;S1工作制","台","1","2024-03-30","炼钢厂部"]
[16,"6000201135","变频调速三相异步电动机","XDYSP180L-4","功率22Kw;额定电压380V;额定电流43.7A;额定转速1470r/min;安装方式B3;防护等级IP55;绝缘等级F级;S1工作制","台","1","2024-03-30","炼钢厂部"]
[17,"6000201136","高效率变频调速三相异步电动机","YPTX3-200L2-2","功率160Kw;额定电压380V;额定电流67.4A;额定转速2961r/min;安装方式B3;防护等级IP55;绝缘等级F级;S1工作制，频率30-50Hz","台","1","2024-03-30","炼钢厂部"]
[18,"6000201137","高效率三相异步电动机","YE4-280S-4/B3;75Kw","功率75Kw;额定电压380V;额定电流136.4A;额定转速1492r/min;安装方式B3;防护等级IP55;绝缘等级F级;S1工作制","台","1","2024-03-30","炼钢厂部"]
[19,"6000201138","三相异步电动机","YE4-160L-2/B5","功率18.5Kw;额定电压380;额定电流34.2A;额定转速2945r/min;安装方式B5;防护等级IP55;绝缘等级F级","台","1","2024-03-30","炼钢厂部"]
[20,"6000201139","高效率隔爆型三相异步电动机","YBX3-160M1-2","功率11Kw;额定电压380V;额定电流20.6A;额定转速2955r/min;安装方式B3;防护等级IP55;绝缘等级F级;三角形接法","台","1","2024-03-30","炼钢厂部"]
[21,"6000201140","变频调速专用三相异步电动机","YVF2-315L2-6","功率132Kw;额定电压380V;额定电流246.5A;转矩1273.3Nm;安装方式B3;防护等级IP55;绝缘等级F级;三角形接法","台","1","2024-03-30","炼钢厂部"]
[22,"6000201141","三相异步电动机","YE4-315S-4V1","功率110Kw;额定电压380V;额定电流195A;额定转速1491r/min;安装方式B5;防护等级IP55;绝缘等级F级;三角形接法","台","1","2024-03-30","炼钢厂部"]
[23,"6000201142","三相异步电动机","YE4-315L1-4V1","功率160Kw;额定电压380V;额定电流279.6A;额定转速1491r/min;安装方式B5;防护等级IP55;绝缘等级F级;三角形接法","台","1","2024-03-30","炼钢厂部"]
[24,"6000201143","三相异步电动机","YE4-132S2-2","额定功率7.5Kw;额定电压380V;额定电流16.2A;额定转速2900r/min;三角型接法;防护等级IP55;绝缘等级F级;安装方式B5","台","1","2024-03-30","炼钢厂部"]
[25,"6000201154","变频调速三相异步电动机","YZPSL132M2-6","额定功率5.5Kw;额定电压380V;额定电流13A;防护等级IP55;绝缘等级H级;带抱闸;抱闸制动电压DC24V","台","1","2024-03-30","炼钢厂部"]
[26,"6000201155","变频调速三相异步电动机","YPT 315-4/200Kw","功率200Kw;额定电压6000V;频率50Hz;额定电流24.2A;额定转速1482r/min;防护等级IP23级;热分级155;S1工作制;安装方式B3;Y型接法;轴伸出端型号6220/C3;非轴伸出端型号6218/C3","台","1","2024-03-30","炼钢厂部"]
[27,"6000201156","变频调速三相异步电动机","YPT 400-6","功率710Kw;额定电压6000V;频率50Hz;额定电流84.6A;额定转速981r/min;防护等级IP23级;热分级155;S1工作制;安装方式B3;Y型接法;轴伸出端型号6224C3;非轴伸出端型号6222C3","台","1","2024-03-30","炼钢厂部"]
[28,"6000201158","变频调速三相异步电动机","YPT 315-4/220Kw","功率220Kw;额定电压6000V;频率50Hz;额定电流26.7A;额定转速1482r/min;防护等级IP23级;热分级155;S1工作制;安装方式B3;Y型接法;轴伸出端型号6220/C3;非轴伸出端型号6218/C3","台","1","2024-03-30","炼钢厂部"]
[29,"6000201159","高效率三相异步电动机","YE4 180L-4","功率22Kw;额定电压380V;频率50Hz;额定电流41.6A;绝缘等级F;防护等级IP55级;S1工作制安装方式B5","台","1","2024-03-30","炼钢厂部"]
[30,"6000201160","起重及冶金用变频调速三相异步电动机","YZP160L-6-E","额定功率11Kw;额定电压380V;额定电流24A;额定转速967r/min;接线盒在上面;防护等级IP55;绝缘等级H级;Y形接法;安装方式B3","台","1","2024-03-30","炼钢厂部"]
[31,"6000201161","YD低速电动机","YD 90","额定功率0.3Kw;额定电压380V;额定电流1.3A;额定转速1.2r/min;额定转矩650N.m;防护等级IP54;绝缘等级F级;安装方式B5;带抱闸","台","1","2024-03-30","炼钢厂部"]
[32,"6000201162","交流电动机","YS8024","额定功率0.75Kw;额定电压380V;额定电流2.01A;额定转速1400r/min;防护等级IP54;绝缘等级F级;安装方式B5;S1工作制;Y型接法","台","4","2024-03-30","炼钢厂部"]
[33,"6000201164","高效率三相异步电动机","YE4-132S-4/B5  5.5KW","额定电压380V ;额定电流11.4A;转速1440r/min;绝缘等级 F级; 防护等级IP54;安装方式 B5 ;接线方式Δ型;频率50HZ;电机轴伸处顶部钻孔攻丝φ10mm*35mm","台","3","2024-03-30","180热轧"]
[34,"6000201165","高效率三相异步电动机","YE4-112M-4/B3；4KW","4KW 电压:380VAC 绝缘等级:F 防护等级:IP54 安装方式:B3 接线方式:三角型接法 S1工作制","台","1","2024-03-30","180热轧"]
[35,"6000201167","三相异步电动机","1TL0001-3AD63-3AA4-Z;315L","额定功率110Kw;额定电压380/660V;额定电流220/127A;额定转速741r/min;绝缘等级:F级;防护等级IP55;安装方式B3;三角型接法","台","1","2024-03-30","炼钢厂部"]
[36,"6000201168","三相异步电动机","YPB160L-6;11Kw","额定功率11Kw;额定电压380V;额定电流23.3A;额定转速968r/min;绝缘等级:F级;防护等级IP54;安装方式B3;Y型接法","台","1","2024-03-30","炼钢厂部"]
[37,"6000201169","液压内轴电机","C05-43BO 5HP","额定电压：380VAC   额定电流：8.6A     额定转速：1420rpm  额定功率：3.75KW","台","1","2024-03-30","检验检测中心"]
[38,"6000201170","三相交流异步电动机","M2BAX 112MA4","额定功率：4KW      额定电流：8.46A    额定转速1433rpm IP55 卧式","台","1","2024-03-30","检验检测中心"]
[39,"6000201171","变频调速三相异步电动机","D1ZP160L-6","额定功率11Kw;额定电压380V;额定电流26A;转速970r/min;防护等级IP55;绝缘等级H级;Y型接法;S3工作制;安装方式B3","台","1","2024-03-30","炼钢厂部"]
[40,"6000201172","冷却塔三相异步电动机","YLT225M-10","额定功率15Kw;额定电压380V;额定频率50Hz;额定电流35.1A;防护等级IP55;S1工作制;绝缘等级F级;额定转速580r/min;三角接法;安装方式B5","台","2","2024-03-30","炼钢厂部"]
[41,"6000201173","三相异步电动机","YE4-160M-4","额定功率11Kw;额定电压380V;额定频率50Hz;额定电流21.5A;防护等级IP55;绝缘等级F级;额定转速1465r/min;三角接法;安装方式B5","台","1","2024-03-30","炼钢厂部"]
[42,"6000201174","三相异步电动机","YE4-160M-4/B3","额定功率11Kw;额定电压380V;额定频率50Hz;额定电流22A;防护等级IP55;绝缘等级F级;额定转速1460r/min;三角接法;安装方式B3","台","1","2024-03-30","炼钢厂部"]
[43,"6000201175","三相异步电动机","YE4-280S-6","额定功率45Kw;额定电压380V;额定频率50Hz;额定电流84.8A;防护等级IP55;绝缘等级F级;额定转速990r/min;安装方式B3","台","1","2024-03-30","炼钢厂部"]
[44,"6000201176","三相异步电动机","YE4-200L2-6","额定功率22Kw;额定电压380V;额定频率50Hz;额定电流43.9A;防护等级IP55;绝缘等级F级;额定转速985r/min;安装方式B3","台","1","2024-03-30","炼钢厂部"]
[45,"6000201177","变频调速三相异步电动机","YGP160S-4","额定功率5.5Kw;额定电压380V;额定频率50Hz;额定电流12.5A;防护等级IP55;绝缘等级H级;S1工作制;额定转速1475r/min;安装方式B5;Y型接法","台","10","2024-03-30","炼钢厂部"]
[46,"6000201178","三相异步电动机","YE4-280M-4/B35;90Kw","额定功率90Kw;额定电压380V;额定频率50Hz;额定电流162A;防护等级IP55;绝缘等级F级;S1工作制;额定转速1490r/min;安装方式B3;三角接法","台","1","2024-03-30","炼钢厂部"]
[47,"6000201179","三相异步电动机","YE4-160L-6","额定功率11Kw;额定电压380V;额定电流23.5A;转速970r/min;防护等级IP55;绝缘等级F级;S1工作制;安装方式B35;三角接法","台","1","2024-03-30","炼钢厂部"]
[48,"6000201186","DMP250M-4 55Kw;H级;带小齿轮","额定电压380V;额定电流106A;额定转速 1480r/min;绝缘等级 H级; 防护等级 IP55 ;安装方式 B5 ;△型接线方式; 出厂编号1100021652/18-1；带编码器支架，键槽宽14mm；小齿轮安装方式采用止动垫圈加锁紧螺母方式",null,"台","1","2024-03-30","180热轧"]
[49,"6000201190","交流电动机","YE3-90L-2","AC380V  2.2KW 4.6A 2840RPM 安装方式B5   定额S1 标准编号 GB18613-2012","台","4","2024-03-30","720厂部"]
[50,"6000300276","变频调速三相异步电动机","YTSZ315M2-10","功率：90KW;196A;额定转速:585rpm;防护等级:IP55;绝缘等级：H级;频率:50HZ;接线方式:三角形;厂家:大连第二电机厂","台","1","2024-03-30","340热轧"]
["注：1、投标报价含税，税率13% ；                                                                                                                2、生产厂家要求全称填写准确无误 ；                                                                                                               3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）；"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2024年1月电动机招标采购项目                    项目编号：HGJY-G2024007"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]