{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":58,"n_cols":12,"rows_kept":58,"merged":[[0,0,0,11],[1,0,1,11],[54,0,54,8],[55,0,55,8],[56,0,56,8],[57,0,57,8]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2024年1月电气备件采购项目                    项目编号：HGJY-G2024006"]
["序号","资材编号","资材名称","规格描述","技术参数","执行标准","单位","数量","申请部门","交货期","含税单价（元）","生产厂家"]
[1,6200200899,"制动电阻","3kW/18R","配CS710-4T30GB变频器，电阻值:18R,制动功率:3kW","IEC61800","台",2,"炼铁厂部","2024-02-26"]
[2,6400600177,"温度继电器","ETS388-5-150+TFP100+S.S+ZBE08+ZBM300","测量范围0-100℃ 精度等级正负1% 4个开关量输出带换向触点，1个模拟输出4-20mA 耐振，耐冲击",null,"只",2,"180厂部","2024-02-26"]
[3,6000300265,"电机抱闸整流器","RH555","555V ;2A;输入380V,输出直流220V；UHT","GB3859-93","个",3,"180热轧","2024-02-26"]
[4,7502500112,"风机","HD9F-FAN-560-560","输入3PAC380V","GB/T22712-2008","台",1,"炼钢厂部","2024-02-26"]
[5,7502500113,"风机","HD9FS-FAN-400A-400","输入3PAC380V","GB/T22712-2008","台",1,"炼钢厂部","2024-02-26"]
[6,4000200309,"电源滑线导杆","800A；345205；橙色",null,"GB/T 14966-1994","根",30,"炼铁厂部","2024-02-26"]
[7,6000300275,"车床风机","RF22P-2DK.3F.5R","ZEHL-ABEC；131510\t07222412；- 400V ±10% Y 50Hz P10 0.80A DI=0% 2320/MIN COSY；- 400V ±10% Y 60Mz P10.1,1A DI=0% 2230/MIN COSY.D PeF min.470PA；-480V ±10% Y 50Mz P10,1.1A Dl=0% 2550MIN COSY 020 PSF min.620PA1P54 THCL155","IEC97-1991","台",2,"340热轧","2024-02-26"]
[8,6100900171,"弧形辊道一段成套电气变频柜","辊道成套变频柜MD480T5.5GB-PLUS-10","柜体尺寸800*2200*800?仿威图；内含汇川变频器MD480T5.5GB-PLUS?10台；交流塑壳断路器NSX160F?TMD?160?3P3D?F?总开关1个；iC65N-D16A/3P?10个；输入/出电抗器ACL-15/OCL-15各10个；柜内元器件接线配好到端子排，附图纸。","GB/T12668.2-1989","套",1,"340热轧","2024-02-26"]
[9,6200200959,"变频器","VFD037E43A","INPUT:3PH 380-480V 50/60Hz;11.2A;OUTPUT:3PH00480V;8.5A;6.8KVA;3.7Kw","GB/T12668.2-2002","台",1,"炼钢厂部","2024-02-26"]
[10,6300700082,"MCGS智能物联网触摸屏","TPC1021Nt","10.2英寸高亮度TFT液晶显示屏（分辨率1024×600）;CPU A8 600MHz;内存128M;系统存储128M;串口1*RS232+1*RS485;USB口 1主1从;以太网口1*10/100M","GB4943.1","块",1,"炼钢厂部","2024-02-26"]
[11,6300700083,"触摸屏","FE7100WE","电源电压24VDC;功率＜10W","GBT 2828","块",1,"炼钢厂部","2024-02-26"]
[12,6100300309,"万能式断路器","CW3-1000","抽屉式;使用类别B;额定绝缘电压U1=1000V;额定冲击耐受电压12KV;Icu65KA,Ics50KA;Icw 1s42KA,分励脱扣器电压AC230V;电操机构AC230V;合闸电磁铁电压AC230V;电源模块电压AC230V;电压额定工作电压Ue=400V;额定电流800A","GB/T14048.2","台",1,"炼钢厂部","2024-02-26"]
[13,4100400293,"电缆桥架","100*75*1.0   宽*高*厚  单位：mm","材质：镀锌钢板，线槽与盖板同长，配相应数量的连接板和螺丝","GB/T 5117-1995","米",50,"720厂部","2024-02-26"]
[14,6100900097,"智能水泵控制器","XY-BC1-4000C","电压：380v，    功率：3KW","GB/T 15184-1994","只",17,"340管加工热处理","2024-03-27"]
[15,4000200152,"绝缘板","8.293543.A;","直径2280*直径710*40;BLT双马酰胺","审核图纸","件",3,"炼钢厂部","2024-02-26"]
[16,6200200216,"变频器","20BC085A0AYNANC0 E0.967X","45Kw 85A 400VAC","E0.967X","台",2,"219厂部","2024-02-26"]
[17,6300500226,"POINT I/O模块底座","1734-RTB+1734-TB;AB","导轨安装","IEC 60068-2-1","套",10,"219厂部","2024-02-26"]
[18,6400400137,"增量编码器","KOYO  TRD-J600-RZV","电源：5VDC； 脉冲数/转：600； 两相带原点输出； 主轴外径：8mm； 带弹性联轴器",null,"只",4,"219厂部","2024-02-26"]
[19,6300400011,"PLC 电源模块","1756-PA72","AB","GBT15969","块",1,"89油管车丝委外","2024-02-10"]
[20,6400400131,"光学编码器","H200808-100","Part NO.:60-0068（From MCCOY Global WinCatt 7 Technical & Operating Manual Parts&Assemblies)；Bei shaft encoder 100 count;100conuts/360°；供电电压 5V;提供原厂DYNAPAR的 Deckaratuib of EC-Conformity合格证书.","Dynaper","件",1,"检验检测中心","2024-02-26"]
[21,6400400180,"轴角编码器安装底座","1392-104A-R3","Part NO.:60-0001（From MCCOY Global WinCatt 7 Technical & Operating Manual Parts&Assemblies);配合H200808-100型光电编码器使用;","API RP 5C5:2018/ISO 13679:2019","套",1,"检验检测中心","2024-02-26"]
[22,6200100102,"无触点控制器","TSF-80A-3PQ","额定功率7.5KW,电源380V，无触点通断，故障报警可储存，通断无火花，实时电流监视。","IEC60947","台",1,"89油管车丝委外","2024-02-26"]
[23,6100300310,"高压断路器和避雷器小车","DQV-12/630-25KA","12kW,630A.机械寿命>30000次","GB/T 1984-2014","台",2,"89油管车丝委外","2024-02-26"]
[24,6400600580,"位移传感器","RWMS0250MLVL10SLG801","SSI输出的，有效行程250mm，最高分辨率0.001mm，带10米电缆","GB/T 28857-2012","根",3,"180热轧","2024-02-26"]
[25,7101500105,"阀门电动装置","Q90-0.5/Z-SZ","防护等级IP65;电机功率0.37Kw;输出转矩900N.m;电压380V;工作时间15-30S","JB/T8219-1999","台",1,"炼钢厂部","2024-02-26"]
[26,6100800024,"阻容过电压吸收器","ZR20-40.5-0.1/100-1(1.6KW)","额定电压40.5KV;额定电阻100Ω;额定电容0.1μF","JB/DQ2553-1989","台",3,"炼钢厂部","2024-02-11"]
[27,6100100238,"三相交流输出电抗器","OCL-0040-0M18-0.4SC","额定电流40A;电感值0.18mH;工作电压380V/50Hz;绝缘等级F级;抗电强度3000V","GB/T1094.6-2011","台",2,"炼钢厂部","2024-02-26"]
[28,6100100239,"三相交流输入电抗器","ACL-0040-0M18-0.4SC","额定电流40A;电感值0.36mH;工作电压380V/50Hz;绝缘等级F级;抗电强度3000V","GB/T1094.6-2011","台",2,"炼钢厂部","2024-02-26"]
[29,6200200963,"制动电阻","RXLG-5KW30R","R101-02202305127405;制动电阻30Ω/5Kw","JB6319-2010","台",2,"炼钢厂部","2024-02-26"]
[30,6100100240,"出线电抗器","MC0-130/1","额定电流130A;电感值97μH;额定频率50Hz","GB/T1094.6-2011","台",2,"炼钢厂部","2024-02-26"]
[31,6100100241,"出线电抗器","MC0-170/1","额定电流70A;电感值74μH;额定频率50Hz","GB/T1094.6-2011","台",2,"炼钢厂部","2024-02-26"]
[32,6100100242,"CSC-280测控保护装置","CSC-283S","工作电源DC220V;CT额定值1A","GB/T25840-2010","台",2,"炼钢厂部","2024-02-26"]
[33,6100100243,"CSC-280测控保护装置","CSC-287S","工作电源DC220V;CT额定值1A","GB/T25840-2010","台",2,"炼钢厂部","2024-02-26"]
[34,6100100244,"CSC-280测控保护装置","CSC-281S","工作电源DC220V;CT额定值1A","GB/T25840-2010","台",2,"炼钢厂部","2024-02-26"]
[35,6100900172,"手自一体降压硅链","GL3520-B2","电压;DC110-220V","DL/781-2001","台",1,"炼钢厂部","2024-02-26"]
[36,6100500427,"中间继电器","DRH275024LT","线圈电压DC24V","EN60204-1","个",5,"炼钢厂部","2024-02-26"]
[37,6100300311,"高压断路器","ZN-12/1250-31.5","额定频率50Hz;额定电压12KV;额定电流1250A;额定短路开断电流31.5KA;额定短路持续时间4S;额定短路关合电流80KA;1min工频耐受电压42KV;操作顺序;分-0.3S-合分-180S-合分;操作电压DC220V","JB/T3855-2008","台",1,"炼钢厂部","2024-03-27"]
[38,6100300312,"高压断路器","ZN-12/2500-31.5","额定频率50Hz;额定电压12KV;额定电流2500A;额定短路开断电流31.5KA;额定短路持续时间4S;额定短路关合电流80KA;1min工频耐受电压42KV;操作顺序;分-0.3S-合分-180S-合分;操作电压DC220V","JB/T3855-2008","台",1,"炼钢厂部","2024-03-27"]
[39,6600200959,"数字显示单元","DD3S-F31P-R","电源电压12-24VDC;正逻辑;标准10进制","IEC-60529","块",10,"炼钢厂部","2024-02-26"]
[40,6100400408,"交流接触器","GMC-800","线圈电压AC24-550V;额定频率50Hz或60Hz;额定绝缘电压为690-1000V;在AC-3使用类别下额定工作电压为380V时的额定工作电流800A","IEC60947-4-1","个",2,"炼钢厂部","2024-02-26"]
[41,6100100097,"整流控制柜变压器","ZSG-30KVA/170+190","GB/T18494.1-2001 30KVA 输入380V 输出170+190V","JB4315-1986","台",1,"炼钢厂部","2024-03-12"]
[42,6100100181,"整流变压器","ZSG-65KVA","输入3AC380V/50Hz;输出AC220V;容量65KVA;全铜绕组","GB/T18494.1-2014","台",2,"炼钢厂部","2024-02-26"]
[43,6300500283,"Profibus从站网关","PCTG-8016，ProfibusDP从站转ModbusTCP","将Profibus和ModbusTcp以太网总线连接的通讯协议转换，Profibus总线上工作在从站模式，在ModbusTcp总线上支持在服务器模式（ModbusTcp从站模式）和客户端模式（ModbusTcp主站模式）","profibusDP协议和modbusTCP协议","块",5,"720厂部","2024-03-27"]
[44,6200200961,"多通道智能滤波分支器","MULTIrep X5","供电电压: 24 VDC ±20%;供电电流: 0,3 A;连接方式: 2-7 x DB9接头;波特率: 9,6 kbps to 12 Mbps;防护等级: IP20;运行温度: +5 °C--+55 °C","GB/T29486-2013","台",1,"340热轧","2024-03-27"]
[45,6100400387,"无触点控制器","TDF-100A-5BH","电源AC380V,无触点通断，可带5路电阻切换，HMI编程面板  智能风扇散热，故障报警可储存，通断无火花，实时电流监视","GB14048.4","台",4,"物流中心","2024-02-26"]
[46,6100900173,"辊道开关箱","600*500*200","304不锈钢箱体，板厚不小于1.5mm,配GV2ME14C 6-10A电动机断路器20只","审核图纸","只",5,"89油管车丝委外","2024-02-26"]
[47,6200200966,"通讯卡","OPC-G1-PDP","FRENIC-MEGA变频器 选件 OPC-G1-PDP(PROFIBUS-DP)通信卡","GBT12668.2-2002","只",4,"89油管车丝委外","2024-02-26"]
[48,6100900174,"操作台","穿孔机P1\\P2\\P3步进炉B1台","4个非标操作台","审核图纸","套",1,"89油管车丝委外","2024-02-26"]
[49,6100500428,"断相与相序保护继电器","XJ3-G","工作电压：三相380V 圆8孔底座使用","GB/T14048.5-2017","个",1,"检验检测中心","2024-02-26"]
[50,6200200909,"高压变频器功率单元","1200G15N","输入电压3相690V/50HZ;输出电压0-690V","DL/T2033-2019","台",2,"炼钢厂部","2024-02-26"]
[51,6100500353,"时间继电器","SK4-220d；0.1～3S","通电延时型空气延时头；延时动作时间0.1～3S；触头额定电流：0.95A主触头触点形式：双断电；工作条件：周围空气温度-50℃—+40℃，24小时的平均值不超过+35℃；空气的相对湿度为不超过50%；安装地点海拔不超过2000M；","GB14048.4-2010","只",20,"340热轧","2024-02-26"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2024年1月电气备件采购项目         项目编号：HGJY-G2024006"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]