{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":46,"n_cols":12,"rows_kept":46,"merged":[[0,0,0,11],[1,0,1,11],[42,0,42,8],[43,0,43,8],[44,0,44,8],[45,0,45,8]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2024年2月电气备件采购项目                    项目编号：HGJY-G2024026"]
["序号","资材编号","资材名称","规格描述","技术参数","执行标准","单位","数量","申请部门","交货期","含税单价（元）","生产厂家"]
[1,6200200405,"变频器","20G14TC770JNONNNNN","输入直流电压范围：486-594V 电流：LD/ND/HD,957/886/739A 输出3相交流电压0-400V 频率0-400HZ 电流：LD/ND/HD，832/770/642 功率：LD/ND/HD，450/400/355kw 带ControlNet网络通讯适配器 带数字量I/O板 带增量型编码器速度反馈接口 带操控面板。标准EN 61800-3:2004 EN 61800-5-1:2007 IEC 61000-4-34。",null,"台",1,"219厂部","2024-06-11"]
[2,6200200216,"变频器","20BC085A0AYNANC0 E0.967X","45Kw 85A 400VAC","E0.967X","台",2,"219厂部","2024-06-11"]
[3,4100500074,"真空灭弧室","3AY1715-1L",null,"GB1984","个",3,"炼钢厂部","2024-06-11"]
[4,6200200683,"变频器","20BC043A0AYNANC0；AB","400V,22KW,43A","E0.967X","台",3,"219厂部","2024-06-11"]
[5,6300100046,"处理器","1756-L61 AB","标准IEC61508","IEC61508","块",4,"219厂部","2024-06-11"]
[6,6200200752,"变频器","PowerFlex 753；20F11NC043JA0NNNNN  AB","输入电压：400V交流 输入频率：三相，47-63HZ：输出电压：0-400V 输出电流：43A 输出频率：三相，0-400HZ 一般负载：22KW","IEC61800","台",2,"219厂部","2024-06-11"]
[7,6300200163,"输出模块","1756-OF8","供电电压;24VDC;   点数;继电器输出8点;   AB","IEC61508","块",2,"219厂部","2024-06-11"]
[8,6300200181,"模拟量输入模块 AB","1769-IF8","8 channel Current /Voltage Analog Input","IEC61508","块",1,"89管加工热处理","2024-06-11"]
[9,6300200182,"数字量输入模块 AB","1769-IQ32","供电电压;24VDC;32点输入模块  AB","IEC61508","块",1,"89管加工热处理","2024-06-11"]
[10,6400600177,"温度继电器","ETS388-5-150+TFP100+S.S+ZBE08+ZBM300","测量范围0-100℃ 精度等级正负1% 4个开关量输出带换向触点，1个模拟输出4-20mA 耐振，耐冲击",null,"只",2,"180厂部","2024-06-11"]
[11,6400600385,"流量开关","SI5010","工作电压19-36VDC,额定电流250mA，不锈钢，福门","EN61000-6-2","只",8,"炼钢厂部","2024-06-11"]
[12,4100400293,"电缆桥架","100*75*1.0   宽*高*厚  单位：mm","材质：镀锌钢板，线槽与盖板同长，配相应数量的连接板和螺丝","GB/T 5117-1995","米",150,"720厂部/180热轧/炼钢","2024-04-28"]
[13,6100800024,"阻容过电压吸收器","ZR20-40.5-0.1/100-1(1.6KW)","额定电压40.5KV;额定电阻100Ω;额定电容0.1μF","JB/DQ2553-1989","台",3,"炼钢厂部","2024-04-28"]
[14,6200200961,"多通道智能滤波分支器","MULTIrep X5","供电电压: 24 VDC ±20%;供电电流: 0,3 A;连接方式: 2-7 x DB9接头;波特率: 9,6 kbps to 12 Mbps;防护等级: IP20;运行温度: +5 °C--+55 °C","GB/T29486-2013","台",1,"340热轧","2024-04-28"]
[15,4100400298,"电缆快速连接头","KMDL-60/80w","额定电流;500A","GB/T19446-2004","套",6,"炼钢厂部","2024-04-28"]
[16,6200200967,"制动电阻","JEDRXLG-10KW7R1J","船型耐高温;阻值50Ω;精度5%","GB10963.1","台",1,"炼钢厂部","2024-04-28"]
[17,6200200913,"数字式（可控硅换向）调压调速装置","THYROMAT 10BCCH 150A 380BNZ-A","供电电压380-415V;3相50Hz;控制电压220V;单相50Hz;额定电流150A;起升机构应用","GB/T3235-1999","台",1,"炼钢厂部","2024-04-28"]
[18,4100400299,"圆形预绝缘端子","RV3.5-5","端子可接2.5-4mm2的线缆，安装螺丝孔为M5，黄铜内芯、阻燃护套、绝缘材料PVC ；欧式接线","GB/T 14315-2008","个",500,"340热轧","2024-04-28"]
[19,5400400034,"移动式工业冷气机","BGK1801-65R","电源220V/50HZ;制冷量6500W;额定功率3000W;最大功率3500W;额定电流13.5A;最大电流16A;出风量1200m3/h;吸/排侧工作压力2.5/4.5MPa;热交换器最大工作压力4.5MPa;使用环境18℃-45℃","GB/T22257-2008","台",1,"180热轧","2024-04-28"]
[20,6400400180,"轴角编码器安装底座","1392-104A-R3","Part NO.:60-0001（From MCCOY Global WinCatt 7 Technical & Operating Manual Parts&Assemblies);配合H200808-100型光电编码器使用;","API RP 5C5:2018/ISO 13679:2019","套",1,"检验检测中心","2024-04-28"]
[21,6100300310,"高压断路器和避雷器小车","DQV-12/630-25KA","12kW,630A.机械寿命>30000次","GB/T 1984-2014","台",2,"89油管车丝委外","2024-04-28"]
[22,6200200966,"通讯卡","OPC-G1-PDP","FRENIC-MEGA变频器 选件 OPC-G1-PDP(PROFIBUS-DP)通信卡","GBT12668.2-2002","只",4,"89油管车丝委外","2024-04-28"]
[23,6600200991,"LoRa无线透传模块","RS232/485-LoRa SX1278","双信号232/485单天线无线模块 3米天线 有效距离1000m","IEC 60947-5-1","对",2,"89管加工热处理","2024-06-11"]
[24,6100900175,"高频电源控制箱","EHC-CZX","容量1.4A，输入电压380V，带手操器接口、上位机接口，尺寸600mm*440mm,防护等级ip65","GB/T3797-2005","套",1,"炼铁厂部","2024-04-28"]
[25,7502500117,"高频电源主风机","DW.S0218-02-DF右旋","电机功率1.1KW/380V,流量1600m3/h ,风压1530pa","GB/T19232-2003","个",1,"炼铁厂部","2024-04-28"]
[26,7502500118,"高频电源主风机","DW.S0218-01-DF左旋","电机功率1.1KW/380V,流量1600m3/h ,风压1530pa","GB/T19232-2003","个",1,"炼铁厂部","2024-04-28"]
[27,6100100245,"开关柜智能操控装置","AB-6609","装置电压DC220V;温控电压AC220V;温湿控制2路;开关旋钮4个;带电显示","IEC255-22","台",3,"炼铁厂部","2024-04-28"]
[28,4100400305,"堵油铜接线鼻子","紫铜，DT-400","400mm2","GB/T 14315-2008","只",6,"能源厂部","2024-04-28"]
[29,6200200683,"变频器","20BC043A0AYNANC0；AB","400V,22KW,43A","E0.967X","台",1,"219厂部","2024-06-11"]
[30,6200200122,"变频器","20BC072A3AYNANCO AB E0.967X","输入电压：400V交流 输入电流：68.9A 输入频率：三相，50HZ：输出电压：0-400V 输出电流：72A 输出频率：三相，0-400HZ 一般负载：37KW","E0.967X","台",1,"219厂部","2024-06-11"]
[31,4100400299,"圆形预绝缘端子","RV3.5-5","端子可接2.5-4mm2的线缆，安装螺丝孔为M5，黄铜内芯、阻燃护套、绝缘材料PVC ；欧式接线","GB/T 14315-2008","个",500,"180热轧","2024-04-28"]
[32,6000400088,"周向磁轭","ZY-380-40A","790mm*450mm*200mm,线圈采用环氧浇注，防水绝缘处理，材质SUS304.","GB/T4249","套",1,"340管加工热处理","2024-04-28"]
[33,6100300329,"ME万能式空气断路器","ME-2500","\"抽屉式，额定电流2500A,过载长延时脱扣器整定电流调节范围\n1500-2000-2500A，短路短延时脱扣器整定电流调节范围8-10-12kA，短路瞬时脱扣器整定电流调节范围4-6-8，通断能力符合IEC60947-2,400-690V 50kA,接通能力400-690V 180kA,额定短时耐受电流80kA.选配欠压脱扣。\"","IEC60947-2","台",1,"89管加工热处理","2024-04-28"]
[34,6100300330,"ME万能式空气断路器","ME-1600","抽屉式，额定电流1600A，过载长延时脱扣器整定电流调节范围900-1200-1600A，短路短延时脱扣器整定电流调节范围5-6.5-8kA，短路瞬时脱扣器整定电流调节范围4-6-8kA，通断能力符合IEC60947-2,400-690V 50kA,接通能力400-690V 105kA,额定短时耐受电流50kA.选配欠压脱扣。","IEC60947-2","台",1,"89管加工热处理","2024-04-28"]
[35,6100900173,"辊道开关箱","600*500*200","304不锈钢箱体，板厚不小于1.5mm,配GV2ME14C 6-10A电动机断路器20只","审核图纸","只",3,"340热轧","2024-04-28"]
[36,6200200863,"变频器","MD480T220P-L;带制动单元及电抗器、制动电阻、485通讯卡","变频器220KW、输入电压380V 额定电流426A 、尺寸：W*H*D 300*1424*500；MD系列变频器制动单元，380V制动单元-标准机；11KW制动电阻；485通讯卡MD38TX1，带隔离的modbus通讯适配卡。","EN61800-3","台",1,"89管加工热处理","2024-04-28"]
[37,6300500285,"双电源自动转换开关","WATSNB-630/630.3CBS-F","Ue:AC50Hz400V:Ie:630A;Uimp;8KV;Ui;690V","GB/T14048.11","台",1,"炼钢厂部","2024-04-28"]
[38,6300700062,"触摸屏电脑","QY-P150-H/I7-7500U","I7-7500U/4G/2*RJ-45/4*USB/4*RS232+2*(RS232/422/485)/可选 9-36V；网口：2 个 intel 千兆以太网；串口： 6 个 RS232/2 个 RS(422/485)；类型：电容式；安装方式： 面板嵌入式，配合支架可 VESA 安装；电源输入：9～36V 直流电源；总体尺寸：390*300*50mm；功率：20W","IEC947","台",1,"89管加工热处理","2024-05-28"]
[39,6300700084,"嵌入式一体化触摸屏","TPC1071Nt","输入24V DC/300mA  max,环境温度0℃...50℃","Q/CP BLH003-2001","块",1,"炼钢厂部","2024-04-28"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2024年2月电气备件采购项目            项目编号：HGJY-G2024026"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}