{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":20,"n_cols":13,"rows_kept":20,"merged":[[0,0,0,12],[1,0,1,12],[16,0,16,8],[17,0,17,8],[18,0,18,8],[19,0,19,8]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2024年3月电磁备件采购项目                   项目编号：HGJY-G2024027"]
["标包号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,6000400007,"电磁吸盘","MW929-420400L/G",null,"台",1,"JB/T10577-2006","720厂部","2024-04-31"]
[2,4100400291,"电缆卷筒","62180.02","最大行程（55+45）m;电缆长度70m;行走速度3-30m/min;最大转堵力矩3000Nm;最大堵转电流25A;配带三相力矩电机YLEJ132-25/6及减速箱;力矩调节控制柜","套",1,"JT/T806.4-2011","炼钢厂部","2024-04-31"]
[3,4100400039,"电缆卷筒","DF100/20-45/35-8/8","容量100A 8通道 电缆长度20米","台",1,"JT/T806.4-2011","炼钢厂部","2024-04-31"]
[4,5300100249,"电缆卷筒","JTA170-15-2Ⅱ",null,"台",2,"JT/T806.4-2011","340管加工热处理","2024-04-31"]
[5,4100400041,"电缆卷筒","JTA100-20-2","容量100A 电缆长度20米2通道","台",1,"JT/T806.4-2011","720厂部","2024-04-31"]
[6,5300100906,"电磁吸吊吸盘链条","(10+10)TJ",null,"套",8,null,"炼钢厂部","2024-04-31"]
[7,6700400038,"永磁吸吊器","YX1-0.5G",null,"台",2,"CB/T3555-1994","180热轧","2024-04-31"]
[8,6000400085,"起重电磁铁","MW42-140140YL/2-75","额定电流55A;额定电压DC220V;功率12.1Kw 重量5000Kg","台",2,"JB4315-86","炼钢厂部","2024-04-31"]
[9,6100900166,"吸盘控制设备","ZKBP1-B-120A/C-N","输入电源AC380V 输出电源DC220V 输出电流DC120A;停电保磁时间30min","台",1,"JB4315-86","炼钢厂部","2024-04-31"]
[10,6000400089,"电磁搅拌器","DJMR-Φ60W","铸坯断面尺寸60cm;额定电压380V:电流500A;频率1～5Hz;视在功率329kVA;线圈采用独立循环水冷却;进水压力≤0.45MPa;外形尺寸Φ1510mm*Φ1010mm*600mm;重量3000Kg","台",1,"Q/JA001-1999","炼钢厂部","2024-04-31"]
[11,6000400090,"电磁搅拌器","DJMR-Φ80W","铸坯断面尺寸80cm;额定电压380V:电流500A;频率1～5Hz;视在功率329kVA;线圈采用独立循环水冷却;进水压力≤0.45MPa;外形尺寸Φ1720mm*Φ1170mm*630mm;重量3900Kg","台",1,"Q/JA001-1999","炼钢厂部","2024-04-31"]
[12,5300100525,"吸盘链条","MW5-250200",null,"付",4,"GB54a-1977","炼钢厂部","2024-05-13"]
[13,6000300125,"气管卷筒","QJDF-50F/20","带力矩电机及减速机","台",1,"JT/T806.4-2011","炼钢厂部","2024-05-13"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2024年3月电磁备件采购项目       项目编号：HGJY-G2024027"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]