{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":28,"n_cols":14,"rows_kept":28,"merged":[[0,0,0,8],[1,0,1,13],[24,0,24,8],[25,0,25,8],[26,0,26,8],[27,0,27,8]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2024年3月机械备件采购项目                       项目编号：HGJY-G2024028"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","标包合价（含税）","生产厂家","备注"]
[1,7100100219,"自力式压力调节阀","V230D01;DN100;PN1.6MPa;0.05-0.3MPa;<140℃","调压范围0.05-0.3MPa;使用温度<140℃","台",1,"SB/T11049-2010","高辅工段","2024-05-28"]
[2,6600300051,"压力调节阀","YCTJF",null,"只",3,"SB/T11049-2010","340热轧","2024-05-28"]
[3,5500300067,"电动执行机构","LSTJ-14000-Q","380VAC;输入信号4-20ma，输出信号4-20ma；自带开关到位及过力矩无源触点反馈；输出力矩14000NM","台",2,"GB/T28017-2011","高炉","2024-05-28"]
[4,5701600106,"离心风机;转子组总成","X4-73-11","No11C;740度;01080929;左旋；原装厂家：吉林四平东大风机工程有限公司","件",1,"JB/T8940-2014","89油管热处理","2024-05-28"]
[5,7101600253,"空气调节阀","电动调节（切断）碟阀，型号：HS4410，DN1100","公称直径：1100，流量系数：68000,公称压力：0.6MPa ，工作温度：-20℃～450℃ ，阀体铸钢件，阀杆、阀板、阀体密封面材质304不锈钢，执行机构防爆等级：ExiaⅡB T4，防护等级IP65，带电动装置及执行机构，全尺寸涡轮，涡轮蜗杆调质处理，蜗杆轴承处设计加油点，带不锈钢金属包覆垫2片及螺栓整套","台",1,"GB/T12238-2008","炼铁厂部","2024-05-28"]
[6,7001900060,"气动隔膜泵止回件","666270-EEB-C英格索兰气动隔膜泵止回配件","每套含4个阀球93358-A (山道橡胶)和4个球座94328-A(山道橡胶)","套",4,"JB/T8697-2014","能源厂部","2024-05-28"]
[7,5300300883,"电链锯","MIL-FF05-405","16寸，自动泵油，锯链长度405mm,净重4.3公斤，220V，50Hz,1900w,480m/min","台",1,"TB447-2004","物流中心","2024-05-28"]
[8,6600300035,"煤气调节阀","E75F/COS-11.17-AP/PDH","阀门口径 DN100 压力等级：ANSI150# 对夹式 流量特性：近似等百分比特性 行程90度 阀体WCB、阀板CF8M不锈钢、阀杆17-4PH不锈钢、阀座RPTFE：泄漏等级：ClassⅥ","只",1,"GB/T4213-2008","89油管车丝委外","2024-05-28"]
[9,6600300033,"煤气调节阀","E75B/WSO-11.15-AP/PSDH","阀门口径 DN150 压力等级：ANSI150# 对夹式 流量特性：近似等百分比特性 额定CV值：1350 行程90度 阀体WCB、阀板CF8M不锈钢、阀杆17-4PH不锈钢、阀座RPTFE：泄漏等级：ClassⅥ 执行机构型号 S93气动角行程，高温型≤120℃ 气源压力0.4~0.6Mpa 阀门定位器S67Y（高温型≤120℃），","只",1,"GB/T4213-1992","89油管车丝委外","2024-05-28"]
[10,6600300041,"气动调节蝶阀","E74B/ST3-13.18-AP/PD","阀门口径 DN125 压力等级：ANSI150# 对夹式 流量特性：近似等百分比特性 额定CV值：1350 行程90度 阀体WCB、阀板CF8M不锈钢、阀杆17-4PH不锈钢、阀座RPTFE：泄漏等级：ClassⅥ 执行机构型号 S93气动角行程，高温型≤120℃ 气源压力0.4~0.6Mpa 阀门定位器S67Y（高温型≤120℃），","只",1,"GBT3667.1-2005","89油管车丝委外","2024-05-28"]
[11,5716700068,"1号线淬火炉天燃气烧嘴（加热段）","型号：SCEM 140LN-100/35","450KW;","套",5,"GB/T 35073-2018","340管加工热处理","2024-05-28"]
[12,5601500002,"烘烤器熄火自动切断装置","含SZK-4火检仪.SJT-4火检探头.SBJQ声光报警器等",null,"套",15,null,"炼钢厂部","2024-05-28"]
[13,4200700079,"吸尘器吸尘扒","50mm，用于VKD-40吸尘器","内径：46mm；外径：50mm；宽：55mm；总长：530mm；宽：17mm；材质：铝合金","个",2,"GB4706.7-2004","340热轧","2024-05-28"]
[14,5400100153,"空压机散热器","LG167","长1240mm,宽1005mm;高度110mm，内螺纹，适配GL90-10正力精密螺杆空压机","套",1,"JB/T2785-2010","检验检测中心","2024-05-28"]
[15,7102000093,"液动阻尼缓冲止回阀","HH47X-10-DN400","压力:1.0MPa DN400 阀体长度310mm","只",2,"GB/T12233-2006","89管加工热处理","2024-05-28"]
[16,7102600090,"星型卸灰阀（含减速机）","YJD-300","300*300","台",2,"GB16490-1996","炼钢厂部","2024-05-28"]
[17,7500300035,"空-空冷却器","AAC130.32.2300","热交换容量13.0Kw;内风路出风温度60℃;外风路进风温度40℃","台",1,"JB/T2728.2-2008","炼钢厂部","2024-05-28"]
[18,null,"双级扒料机","螺旋外径600mm;螺旋扒料宽度3m;取料宽度3.4m;叶片厚度8mm;配用电机功率45KW;配用减速机ZQ400双输出;前输送带宽1000mm，长度10m，动力7.5KW电滚筒，细绊主架12#槽钢，输送带材料尼龙芯防滑橡胶带:后输送带宽1000mm，长度12m+5m(伸缩)，动力15KW电滚筒，刹车电机4KW，主架12#槽钢输送带材料尼龙芯防滑橡胶带《配皮带清扫器);卸料高度3-5米;小挖电机4KW;液压站配用电机15KW;履带底盘带宽400橡胶，履带型号00*90*68，有效长度2.9米，液压行走;后皮带机可左右180度摇摆，配置@1000回转支承，液压站11KW。","详见技术规格书","套",1,null,"炼铁厂热风炉烟气脱硫改造HG202337","2024-05-28"]
[19,7102600089,"管夹阀","SZTM-PF01.5A","DN10;GJH-2C","只",4,"GB12232-89","炼钢厂部","2024-05-28"]
[20,5501800024,"整套圆盘（不含减速机）","PDX25HLS","定量圆盘给料系统，盘面直径2500，硬齿面回转轴承QND900.25AZ，底架组装件,盘面及附属密封、管路螺栓等，不包括减速箱及减速箱润滑系统。","套",1,null,"烧结","2024-05-28"]
[21,6600300194,"蒸汽调节阀","型号：LSDF-P2-16KG","参数：压力：1.6MPa，口径：50mm，输入输出：4-20mA，介质：高温蒸汽，?电动执行器：LSP-210，流量特性：等百分比","台","1","JB/T7387","炼铁厂部","2024-05-28"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2024年3月机械备件采购项目          项目编号：HGJY-G2024028"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}