{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":24,"n_cols":14,"rows_kept":24,"merged":[[0,0,0,8],[1,0,1,13],[20,0,20,8],[21,0,21,8],[22,0,22,8],[23,0,23,8]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2024年4月机械备件采购项目                     项目编号：HG JY-G2024041"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","标包合价（含税）","生产厂家","备注"]
[1,5601500003,"自预热高速燃烧器","WD-GZYS-200H","1Cr18Ni9Ti和Cr25Ni20,85Kg;焊缝无夹杂、气孔等缺陷;法兰面不能有焊渣;保证法兰面平整;所有位置满焊;不能出现漏气的焊孔。","只",2,"JB/T10697-2007","炼钢厂部","2024-06-26"]
[2,7100100219,"自力式压力调节阀","V230D01;DN100;PN1.6MPa;0.05-0.3MPa;<140℃","调压范围0.05-0.3MPa;使用温度<140℃","台",1,"SB/T11049-2010","高辅工段","2024-06-26"]
[3,6600300051,"压力调节阀","YCTJF",null,"只",3,"SB/T11049-2010","340热轧","2024-06-26"]
[4,5400300008,"煤气冷凝水排水器","SDLT-4000-100","Q235 GB6222","台",1,"GB6222","高辅工段","2024-06-26"]
[5,5702400071,"空气预热器","90270116DR5005IS001-2","管径51*30 Cr18SiAl 插件0Cr13 7200Kg","台",1,"审核图纸","180热轧","2024-06-26"]
[6,5501800024,"整套圆盘（不含减速机）","PDX25HLS","定量圆盘给料系统，盘面直径2500，硬齿面回转轴承QND900.25AZ，底架组装件,盘面及附属密封、管路螺栓等，不包括减速箱及减速箱润滑系统。","套",1,null,"烧结","2024-06-26"]
[7,6600300051,"压力调节阀","YCTJF",null,"只",3,"SB/T11049-2010","340热轧","2024-06-26"]
[8,6600300051,"压力调节阀","YCTJF",null,"只",3,"SB/T11049-2010","340热轧","2024-06-26"]
[9,6200300117,"中频水水交换器","LSS-100-D","冷却容量≥100KW,纯水流量18T/H,不锈钢换热器，不锈钢泵组一用一备，电机功率4KW。","套",1,"JB/T5833-2013","89管加工热处理","2024-06-26"]
[10,7502300070,"喷嘴","PZ12.7-80-30HY","二冷水;螺纹连接;角度80*30o;流量12.7L/min","只",300,"YB4187-1992","炼钢厂部","2024-06-26"]
[11,7501300135,"膨胀节","DN50 L=200","材质304不锈钢;伸缩量30mm","个",4,"GB/T12777-2008","炼钢厂部","2024-06-26"]
[12,7101600256,"气动开关蝶阀","Z011-A-PN16-DN125","阀体材质;球墨铸铁GGG-40;阀板材质;不锈钢1.4408;阀杠材质;2Cr13;阀座密件;EPDM;连接方式;对夹;阀板工作压力;16bar","只",2,"GB/T8100-2006","炼钢厂部","2024-06-26"]
[13,7500300036,"列管式冷却器","GLC4-20","设计压力1.3Mpa.试压压力1.6Mpa;设计温度100度，冷却面积20平方米，内部换热管材质T2紫铜管。","只",1,"JB/T4715-1992","能源厂部","2024-06-26"]
[14,7502400150,"回转式栅格机 配件总成","格栅机型号:HQHF-600，珊条间隙：5mm","含轴1根、尼龙隔套25个、靶齿23片、连接片2个、挡板2块、小外卡环6个、大外卡环2个、小套2个、滚轮2个","套",20,"GB/T19001-2008","能源厂部","2024-06-26"]
[15,7501300137,"波纹膨胀节","SHCL300350F-PN25-380-1.4301","波纹管材质：不锈钢，规格：DN350，工作压力：PN2.5MPa，长度：380㎜；","件",3,"GB/T12777","180管加工热处理","2024-06-26"]
[16,4201700146,"容恩驾驶式工业洗扫一体机","R-QQ驾驶式洗地机","机器重量277kg；工作宽度700mm，续航3-4小时，吸水扒宽度960mm，清水箱容积90L，脏水箱容积100L，行驶速度0-6km/h，电源24V150AH可充电式，机器1330mm*800mm*1210mm。配置：电池一组、带三个吸水扒、刷盘配套；整机质保12个月，电池质保3年；","套",4,"EN60335-2-69","340热轧","2024-06-26"]
[17,null,"焦炭取样机","GY-JCY1000","详见技术规格书","套",1,null,"HG202360炼铁焦仓区无组织扬尘综合治理项目","2024-06-26"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2024年4月机械备件采购项目       项目编号：HG JY-G2024041"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]