{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["一、开标一览表","二、偏离表"],"read":"whole","date_system":"1900"}

{"sheet":"一、开标一览表","index":0,"n_rows":32,"n_cols":13,"rows_kept":32,"merged":[[0,0,0,12],[1,0,1,12],[27,0,27,12],[29,0,29,3],[30,0,30,3],[31,0,31,3]]}
["    （一）开标一览表"]
["项目名称：2024年4月份液压类备件公开招标项目                                      项目编号：HG JY-G2024043"]
["序号","资材编号","资材名称","规格型号","技术参数","单位","执行标准","数量","交货时间","使用部门","含税单价(元)","生产厂家","备注"]
[1,5900100006,"可移动夹紧虎钳油缸","90*400","90*400；用于G4240/50卧式带锯床","台","JB/T4318.3-1996",2,"2024-07-30","检验检测中心"]
[2,7200400111,"GB4280C带锯机升降油缸","G4280;直径120*880","G4280;直径120*880；适配雁荡山GB4280C锯床","台","JB/T11588-2013",2,"2024-07-30","检验检测中心"]
[3,7100300460,"电磁换向阀","DPHI-2710/E-X-24DC","two stage directional solenoid valve(双级电磁换向型）；由DHE-0713P DC 20铸件和PHE-2710/E 20阀组合而成；surface mounting(ISO 4401):size 16；最大流量为 300L/min；最高承压能力350bar；供电电压24 DC ；Atos solenoid directional valve","台","ISO 4401:2005/BS ISO 7368-2016",1,"2024-07-30","检验检测中心"]
[4,7100300461,"电磁换向阀","DHE-0714-X-24DC 20","surface mounting(ISO 4401):size 06；最大流量为 80L/min；最高承压能力350bar；供电电压24 DC ；Atos solenoid directional valve","台","ISO 4401:2005/BS ISO 7368-2016",1,"2024-07-30","检验检测中心"]
[5,7100300462,"电磁换向阀","DPHI-2614/E/FV-X-24DC","two stage directional solenoid valve(双级电磁换向型）；由PILOT DHE-0631/2P/F-X 24DC 20铸件和DPHE-2614/E/FV-X-24DC 20阀组合而成；surface mounting(ISO 4401):size 16；最大流量为 300L/min；最高承压能力350bar；供电电压24 DC ；Atos solenoid directional valve","台","ISO 4401:2005/BS ISO 7368-2016",1,"2024-07-30","检验检测中心"]
[6,7100300463,"电磁换向阀","DHE-0614/A/FV-X-24DC 20","surface mounting(ISO 4401):size 06；最大流量为 80L/min；最高承压能力350bar；供电电压24 DC ；Atos solenoid directional valve","台","ISO 4401:2005/BS ISO 7368-2016",1,"2024-07-30","检验检测中心"]
[7,7100500129,"阿托斯比例换向阀","DPZO-A-351-LS5   31/10","通径25，最大压力：350bar","台","ISO 4401标准",1,"2024-07-30","219厂部"]
[8,4200700109,"液压拉伸器","GT4.090541","额定工作压力1500bar;行程15mm;可以多台串联和并联使用;自动复位功能;拉杆和支撑桥可以快速拆卸、安装","台","EN-ISO 4413:2010",1,"2024-07-30","炼钢厂部"]
[9,4200700110,"液压拉伸器适配器","GT4PM-NRS05603","用于M56*3的螺栓;包含M56*3拉杆、支撑桥、拨圈、拨杆;适配器与拉伸器GT4.090541的液压缸匹配使用","台","EN-ISO 4413:2010",1,"2024-07-30","炼钢厂部"]
[10,7000300051,"气柜油泵站齿轮泵","KCB33.3","流量2.0m3/h、额定压力1.45MPa、功率2.2KW、转速1420r/min、进出口直径20mm 、带联轴器","台","JB/T7041-2006",4,"2024-07-30","能源厂部"]
[11,7200100177,"液压缸","UBJZD100-180度H","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台",null,1,"2024-07-30","219厂部"]
[12,7200100077,"液压缸","CD250D100/70-125A10/02CGDMA","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台","JB/T10205-2000",3,"2024-07-30","219厂部"]
[13,7200600162,"液压缸","HYZ02345","直径90/80-130","台","JB/T10205-2000",3,"2024-07-30","89热轧"]
[14,7200600220,"PG-140平衡油缸","GJ13021","140/70-20","台","审核图纸",2,"2024-07-30","89热轧"]
[15,7200600135,"引锭杆存放液压缸","125/70-490","96Kg","台","JB/T10205-2000",2,"2024-07-30","炼钢厂部"]
[16,7200600145,"中间包车升降液压缸","160/110-405","进口密封 带位移传感器型号:RHM0425MR021A01,并配配套磁环 油缸所配阀块分左、右两种,一台油缸配一块阀块,具体见图纸 工作介质聚酯抗燃液压油","台","JB/T10205-2000",3,"2024-07-30","炼钢厂部"]
[17,7200600292,"φ125电极升降缸","31120-2-3-4","柱塞直径125mm;举升行程3500mm;工作压力15Mpa;试验压力20Mpa;工作介质;水-乙二醇;采用V组密封;采用铜导向套","台","审核图纸",1,"2024-07-30","炼钢厂部"]
[18,7200200066,"液压缸","Z0745.05.02.04","额定压力25MPa JB/T 5000","台","审核图纸",3,"2024-07-30","180热轧"]
[19,7200600265,"管坯锯平衡液压缸","HYZ01945;32/20-25","缸径32mm，杆径20mm，行程25mm，方形，采用滑环式密封","台","审核图纸",3,"2024-07-30","180热轧"]
[20,5723000044,"快开缸装配","图号：19500701.3.11 ；总重量：1869.5㎏；","装配件；含：1.缸体：19500701.3.11-01，材质：45#；2.油口：19500701.3.11-02，材质：45#；3.活塞：19500701.3.11-03，材质：45#；4.缸盖，19500701.3.11-04，材质：45#；5.图纸中其相应的部件及密封件等；试验压力25MPa 工作环境温度-20℃~70℃；","台","审核图纸",1,"2024-07-30","180管加工热处理"]
[21,7200100035,"液压缸","CD250F63/36-100A10/02CGDMA","压力等级：25MPa 采用进口密封 连接螺栓12.9级","台",null,4,"2024-07-30","340热轧"]
[22,7200600120,"液压缸","PBA03DC00000 100/63-150","缸径Φ100,杆径Φ63,行程150 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞采用PG型组合密封 活塞杆采用RS+USH型组合密封","台","审核图纸",2,"2024-07-30","340热轧"]
[23,7200600099,"液压缸","HYZ138-45 160/140-450","缸径Φ160,杆径Φ140,行程450 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台","审核图纸",2,"2024-07-30","340热轧"]
[24,7200500073,"液压缸","EF02F0000;63/45-630","缸径Φ63,杆径Φ45,行程630,工作压力14MPa,试验压力16MPa,活塞及活塞杆采用V型组合",null,"JB/T10205-2000",2,"2024-07-30","340热轧"]
["注：1、投标报价含税，税率13% ；                                                                                                 \n2、生产厂家要求全称填写准确无误 ；                                                                                        \n3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）"]
[]
["投标人：                         （盖单位公章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日  期：      年      月      日                "]

{"sheet":"二、偏离表","index":1,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]]}
["   （二）商务/技术偏离表"]
["项目名称：2024年4月份液压类备件公开招标项目                                      \n项目编号：HG JY-G2024043"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位公章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日  期：      年      月      日                "]