{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":27,"n_cols":12,"rows_kept":27,"merged":[[0,0,0,11],[1,0,1,11],[23,0,23,8],[24,0,24,8],[25,0,25,8],[26,0,26,8]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2024年4月电气备件采购项目                    项目编号：HG JY-G2024047"]
["序号","资材编号","资材名称","规格描述","技术参数","执行标准","单位","数量","申请部门","交货期","含税单价（元）","生产厂家"]
[1,6200100100,"ACS6000去离子热交换器","GX-18PI","最大/最小工作压力10bar/-1bar；最大/最小工作温度100度/0度；空载重量213KG;满载重量239KG；品牌：tranter德国丹尼尔SERIAL:1923168/1:CONTROL:02813654/40:CONTROL:02813654/40","JB/T4715-1992","台",1,"340热轧","2024-06-11"]
[2,6400400182,"增量编码器","HS35AY1CX15","供电电压10-30VDC;1024PPR;信号输出方式;脉冲输出;孔径16mm;防护等级IP65","JB/T11505-2013","台",4,"炼钢厂部","2024-06-11"]
[3,6400600593,"MTS磁致伸缩位移传感器","RH5MA0050M01D701S1011G1","电源电压24VDC;输出类型SSI;数据长度25bit;数据格式;格雷码;分辨率5μm;标准行程50mm;连接类型;M16公接头（7针）;正向测量;异步模式;配201542-2磁环","JB/T10726-2007","台",2,"炼钢厂部","2024-06-11"]
[4,6400400007,"增量编码器","DGS60-G4B04096 德国IEC947","电源电压DC10-30V，脉冲数1024个/圈","德国IEC947","只",2,"炼钢厂部","2024-06-11"]
[5,6100500430,"大功率继电器","JQX-38F 3Z","线圈电压24VDC;辅助触点负载40A;辅助触点三开三闭","GB/T14048","只",20,"炼钢厂部","2024-06-11"]
[6,6100300284,"时控开关","SX102L","工作电压：3*380VAC±15%;50-60HZ;控制负载≤4KW三相（阻性）;控制电流：3*16A","GB/T14536.1","个",20,"炼钢厂部","2024-06-11"]
[7,4100400294,"工业航空插头","NTC1-563P6h/415V 插头","5芯:额定电流:63A,额定电压415V:防护等级：IP44;厂家:浙江正泰","GB/T 11918.1","个",1,"烧结","2024-06-11"]
[8,6100900131,"传动控制柜柜体","GGD改","高*宽*深2200*1200*800","审核图纸","台",3,"180热轧","2024-06-11"]
[9,6100300327,"万能式断路器","CW1-1600/1600A","CatB;额定绝缘电压Ui1000V;额定冲击耐受电压Uimp12KV;额定工作电压Ue400V;额定电流In1600A;Icu100kA;Ics80kA;Icw 1s 80kA;控制电压AC230V","GB14048.2","台",1,"340热轧","2024-06-11"]
[10,5501500023,"汇流板","300M-9F；4V310",null,"ISO9001-CE","件",2,"烧结","2024-06-11"]
[11,5501500024,"汇流板","300M-11F；4V310",null,"ISO9001-CE","件",2,"烧结","2024-06-11"]
[12,6100900179,"高频电源控制箱","EHC-NBX-600A","容量1.4A，输入电压AC380V，输出电压AC537v高频交流电，尺寸450mm*360mm,防护等级ip65","GB/T3797-2005","套",1,"炼铁厂部","2024-06-11"]
[13,5300700016,"铁水车加盖：地面控制柜","LC8921-II/型","交流380伏","JB/T2785-2010","个",2,"物流中心","2023-06-27"]
[14,4100400176,"端子排卡子","249-116",null,"IEC947-7-1","个",100,"219厂部","2024-06-11"]
[15,4000200305,"电阻器","RS54-355M-10/11D","配90Kw电机，要求4级切除，工作时带一部分软化电阻","JB/T11410-2013","组",1,"物流中心","2024-06-11"]
[16,6200300117,"中频水水交换器","LSS-100-D","冷却容量≥100KW,纯水流量18T/H,不锈钢换热器，不锈钢泵组一用一备，电机功率4KW。","JB/T5833-2013","套",1,"89管加工热处理","2024-06-11"]
[17,6200300113,"感应加热电源","HXKPS-300KW/1-2.5KHZ","进线电源630V,50HZ,中频频率1-2.5KHZ，中频电压0-1275KV可调,功率300KW,可控硅垂直安装，外配谐振电容与300KW加热器一套，柜体尺寸1200*950*2000。","GB/T7676.1-9","套",2,"89管加工热处理","2024-06-11"]
[18,6400600022,"安全开关","LX8-5",null,"GB/T5465.2-1996","只",10,"物流中心","2024-06-11"]
[19,6100900178,"操作台","800*780*1100mm","审核图纸","审核图纸","个",1,"89管加工热处理","2024-06-11"]
[20,6400300242,"振动传感器","CST51301-G03","4-20mA  7.87mV/μm   DC12V-35V  0-125μm","GB/T14048","个",1,"能源厂部","2024-06-11"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2024年4月电气备件采购项目          项目编号：HG JY-G2024047"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}