{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":20,"n_cols":13,"rows_kept":20,"merged":[[0,0,0,8],[1,0,1,12],[16,0,16,8],[17,0,17,8],[18,0,18,8],[19,0,19,8]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2024年5月机械备件采购项目                     项目编号：HG JY-G2024054"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,7502500043,"轴流风机","BSFT-300","AC220V;0.55Kw;配10米风管手提式；防爆","台",2,"GB/T11800-2008","720厂部","2024-07-12"]
[2,7001300005,"超高压热水清洗机","HMSJ-5022","最大压力500kg/cm2;最大流量22L/min;22kw;380V;最高出水温度90度","套",1,"GB/T26135-2010","89热轧","2024-07-28"]
[3,5601500003,"自预热高速燃烧器","WD-GZYS-200H","1Cr18Ni9Ti和Cr25Ni20,85Kg;焊缝无夹杂、气孔等缺陷;法兰面不能有焊渣;保证法兰面平整;所有位置满焊;不能出现漏气的焊孔。","只",2,"JB/T10697-2007","炼钢厂部","2024-07-28"]
[4,6600300051,"压力调节阀","YCTJF",null,"只",9,"SB/T11049-2010","340热轧","2024-07-28"]
[5,5502000041,"一极出灰刮板输送机","YD250G","输送物料:粉尘;输送长度:25.8m;输灰量:6.5立方/h;机槽宽度:25㎝;链条节距:15厘米;传动方式:链条传动;减速机型号:BWY3332-187-5.5-4;电机功率:5.5kw;电机防护等级:IP54;电源:380v;50HZ","套",1,"审核图纸","高辅工段","2024-07-28"]
[6,5501100056,"限矩型永磁耦合器","DYT-X75","结构形式AB-BA盘式对称结构设计；永磁转子部件烧结钕铁硼、铝、钢；导体转子部件钢、 铜；输入转速1480rpm；最高输出转速<1480rpm(电机额定转速的97%-99%）；工作效率≥97%；角度允许偏差＜1.5°；最大传递扭矩871 N.m；堵转保护转矩/电机额定转矩1.8倍；允许最低工作环境温度-40℃；允许最高工作环境温度3+180℃；轮毂类型剖分式轮毂（带平键）","套",1,"Q/320192MGNT001-2018","烧结","2024-07-28"]
[7,7502300037,"双介质气雾喷枪","621072303-03-00-2","P=0.6MP;Qmax3.7T/H;＜120°;￠3500;H~3000;枪长1600;开孔273;316L护板","把",2,"GB/T4213-1992","炼钢厂部","2024-07-28"]
[8,4201200045,"火焰清理枪","QLQ-2","总长2m;枪头长280mm;氧气接头螺纹M18*1.5;燃气接头螺纹M16*1.5反丝;材质;手柄铜（H59-1);枪头材质耐热钢","把",10,"GB5108-1985","炼钢厂部","2024-07-28"]
[9,4201200046,"清理嘴","QLZ-2","长度280mm;氧气接头螺纹M16*1.5;燃气接头螺纹M16*1","个",20,"GB5108-1985","炼钢厂部","2024-07-28"]
[10,7502500087,"离心通风机","225FLJ7F","380V/50Hz;170w","台",4,"JB/T2977-1992","89管加工热处理","2024-07-28"]
[11,4300500129,"废橡胶皮带","成捆","不得夹杂碎皮带及钢丝皮带","吨",60,"GB7984-2001-T","物流中心","2024-07-27"]
[12,5400100162,"离心式空压机 后冷却器","S050 1006","\"FS-ELLIOTT 260 传热面积：46.27㎡\n，外壳最大工作压力:0.6Mpa、最大工作温度：104℃，换热器最大工作压力：1.0Mpa、最大工作温度248℃\"","台",1,"GB151-1999","能源厂部","2024-08-26"]
[13,5800200112,"拖链","TL125-Ⅱ;200*420*3125","铝型材支撑板II型;两侧长孔70*100;中间长孔70*150","件",5,"JB/T6608-1993","炼钢厂部","2024-07-27"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2024年5月机械备件采购项目                     \n项目编号：HG JY-G2024054"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}