{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":26,"n_cols":14,"rows_kept":26,"merged":[[0,0,0,12],[1,0,1,12],[22,0,22,9],[23,0,23,9],[24,0,24,9],[25,0,25,9]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2024年10月电气备件采购项目                  项目编号：HG JY-G2024133"]
["序号","子项号","资材编号","资材名称","规格描述","技术参数","执行标准","单位","数量","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,"A2248000440005",6200200990,"数字式（可控硅换向）调压调速装置","THYROMAT 10BCCH 350A 380BSZ-A","供电电压380V;3相50Hz;控制电压220V;单相50Hz;额定电流350A;电机定子电流250A-318A;起升机构应用","GB/T3235-1999","台",1,"炼钢厂部","2024-10-27"]
[2,"A2249000390021",4000200382,"耐磨型集电器组件","PB31DD-NMX2000Z","包含全套精密铸造支架、D66材质合金电刷、铜导线、导电铜托盘、高强度绝缘子组件等;具备清灰功能;可连续使用30天","GB/T6391-2010","套",50,"炼钢厂部","2024-11-27"]
[3,"A2249000390022",4000200383,"耐磨型集电器组件电刷","PB31DD-NM2000-DS","D66材质;沁铜工艺和金电刷;200*80*35等;具备清灰功能;可连续使用30天","GB/T6391-2010","只",50,"炼钢厂部","2024-11-12"]
[4,"A1249000410091",4100500409,"APT带灯旋钮开关","PB1S-11CXD/G23","绿色;AC/DC24V;一开一闭;孔径22.5mm;防护等级IP65","IEC60947-5-1","只",50,"219厂部","2024-11-27"]
[5,"A1249000410104",4100600073,"行车防震高清投影灯","SBLJWB200W","输入电压220V，功率200W LED，色温8000-8500K,防护等级IP65","GB/T28037-2011","台",2,"219厂部","2024-11-27"]
[6,"A2249000680202",6100600312,"熔断器","ATDR6","6A;AC 200KA;IR600V;DC100KA IR300V","GB/T13539 IEC 60270","只",100,"180热轧","2024-11-27"]
[7,"A1249000360044",6100600313,"半导体设备保护用熔断器","RSK-500V/800A-07ALK","额定电压500V，电流800A","IEC60269-4","只",5,"89管加工热处理","2024-11-27"]
[8,"A2249000350029",6200100107,"电源板","EMS-Project-Power-1","通过集成电路和其他原器件将220VAC和580VDC转变成15VDC和24VDC","GB/T14048.10-2008","块",1,"炼钢厂部","2024-11-27"]
[9,"A2249000390016",6200200632,"调压调速装置","THYROMAT 10BCCT150A","380BSZ;容量150A;平移","GB/T3235-1999","台",1,"炼钢厂部","2024-11-27"]
[10,"A1249000360042",6200200654,"伺服控制器","IS580T100-R1","INPUT 3PH AC380-480V 106A OUTPUT AC 0-480V,112A 0－300HZ 55KW SUZHOU LNOUANCE","JB/T8219-1999","套",1,"89管加工热处理","2024-11-27"]
[11,"A2249000680182",6200200980,"行走变频器","S500-1.5G/2.2P","变频器品牌艾默生，输入：交流电3PH；额定电压380V±15%；额定频率50/60HZ  输出：额定电流3.8A；交流电3PH；额定电压0-380V；额定频率0-600HZ","GB/T12668.2-1989","套",1,"180热轧","2024-11-27"]
[12,"A2249000680183",6200200981,"滚轮变频器","S500-2.2G/4P","变频器品牌艾默生，输入：交流电3PH；额定电压380V±15%；额定频率50/60HZ  输出：额定电流5.1A；交流电3PH；额定电压0-380V；额定频率0-600HZ","GB/T12668.2-1989","套",1,"180热轧","2024-11-27"]
[13,"A2249000680184",6200200982,"主电机变频器","S500-G18.5/22P","变频器品牌艾默生输入：交流电3PH；额定电压380V±15%；额定频率50/60HZ  输出：额定电流37A；交流电3PH；额定电压0-380V；额定频率0-600HZ","GB/T12668.2-1989","套",1,"180热轧","2024-11-27"]
[14,"A2249000350025",6200200998,"IGBT功率模块","2MBI1400VXB-120P-54","容量1400A;耐压1200V;MYS","GB/T1404","块",1,"炼钢厂部","2024-11-27"]
[15,"A2249000350026",6200200999,"整流模块","MDC500A/1600V","容量5000A;耐压1600V","GB/T18904-2002","块",1,"炼钢厂部","2024-11-27"]
[16,"A2249000350027",6200201010,"控制板","EMS-Project-Control-1","电压24VDC;±15VDC;通过集成电路和其他原器件实现对变频电源柜的过程控制和数据采集;出厂编号ZK22120422;带程序","JB/T8680-2008","块",1,"炼钢厂部","2024-11-27"]
[17,"A2249000350028",6200201011,"驱动板","EMS-Project-IGBT Drive(1400A)-1","电压24VDC;15VDC;通过集成电路和其他原器件控制变频电源柜IGBT逆变输出;出厂编号ZK2103008;带程序","GB/T20079-2006","块",1,"炼钢厂部","2024-11-27"]
[18,"A1249000360043",6200300123,"抗干扰六脉冲控制板","KGPS-6D","控制电源AC18V, 频率0-2500HZ ，主回路进线电源AC380V","SJ/T10616-1995","块",2,"89管加工热处理","2024-11-27"]
[19,"A2249000350057",7502500113,"风机","HD9FS-FAN-400A-400","输入3PAC380V","GB/T22712-2008","台",1,"炼钢厂部","2024-11-12"]
["注：1、投标报价含税，税率13%                                                                                     \n2、生产厂家要求全称填写准确无误\n3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2024年10月电气备件采购项目     项目编号：HG JY-G2024133"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]