{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Macro1","附件1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"附件1","index":1,"n_rows":612,"n_cols":8,"rows_kept":612,"merged":[[0,0,0,7]],"flags":["formulas_cached_only"]}
["附件1"]
["序号","资材编码","资材名称","规格描述","技术要求","部门","单位","数量"]
[1,7402700007,"金属包覆垫片","直径780/直径730 厚度8mm","不锈钢 耐温1200度","炼铁厂","片",10]
[2,7402700065,"金属包覆垫片","直径915/直径820","厚度5mm 耐温1200度","炼铁厂","片",10]
[3,7402700002,"金属缠绕式垫片","直径575*直径485 厚度8mm 不锈钢 耐温1200度","不锈钢 GB/T4622.2-2003","炼铁厂","片",10]
[4,7402700055,"316不锈钢垫片","直径210*直径160*3","耐高温500℃；紫铜；压力2.5MPa 16Kg/cm2","能源分厂","片",10]
[5,7402600013,"316不锈钢石墨垫片","直径80*125*3","316不锈钢 耐温250℃，GB/T9877-2008","炼铁厂","片",100]
[6,7402700012,"金属包覆垫片","直径1780*1690*8","不锈钢 耐高温500℃，GB/T15601-1995","炼铁厂","片",4]
[7,7402700013,"金属包覆垫片","直径2180*2080*8","不锈钢 耐高温500℃，GB/T15601-1995","炼铁厂","片",2]
[8,7402700014,"金属包覆垫","直径1333*直径1230*8 304/石墨橡胶+石墨","304/石墨橡胶+石墨 GB/T15601-1995","炼铁厂","片",5]
[9,7402700027,"金属包式垫片","直径1255*30*10 304/石棉橡胶+石墨","304/石棉橡胶+石墨 GB/T15601-1995","炼铁厂","片",5]
[10,7402700028,"金属包式垫片","直径1290*30*10 304/石棉橡胶+石墨","304/石棉橡胶+石墨 GB/T15601-1995","炼铁厂","片",10]
[11,7402700063,"金属包覆垫片","CSCLBXG1800-355/10mm","耐高温1200度","炼铁厂","片",2]
[12,7402700044,"金属硬密封垫圈","Q37F-16C","DN400","炼铁厂","只",10]
[13,4000800946,"金属包式垫片","直径1400","不锈钢","炼铁厂","个",2]
[14,7402700062,"金属包覆垫片","315*705*375*8","耐温1200度","炼铁厂","片",10]
[15,7402700029,"金属包覆垫片","直径520*450*8","不锈钢 GB/T150601-1995","炼铁厂","只",10]
[16,7402700010,"金属包覆垫片","∮300*∮360*6","不锈钢 耐高温500℃，压实厚度6mm","炼铁厂","片",10]
[17,7402700011,"金属包覆垫","直径800*直径880*5","316不锈钢包石墨 . 耐温250℃","炼铁厂","片",10]
[18,7402700007,"金属包覆垫片","直径780/直径730 厚度8mm","不锈钢 耐温1200度","炼铁厂","片",10]
[19,7402700016,"金属包覆垫片","DN100，厚度4mm，外径154mm，内径100mm，耐温>500℃","碳钢 GB/T150601-1995","炼铁厂","片",100]
[20,7402700061,"不锈钢垫片","CPS357S-125*90*4","PTFE","管加工分厂","片",10]
[21,7402700062,"金属包覆垫片","315*705*375*8","耐温1200度","炼铁厂","片",10]
[22,7402700065,"金属包覆垫片","直径915/直径820","厚度5mm 耐温1200度","炼铁厂","片",10]
[23,7402700067,"316不锈钢高温专用垫片","DN300;","325/416;耐温>500℃","炼铁厂","片",10]
[24,7402700068,"金属垫圈","1600*1690*厚度5mm","适用于煤气出口主管道电动扇形阀;D943P-2.5;DN1600","炼铁厂","只",10]
[25,7402700069,"金属垫圈","1200*1290*厚度5mm","适用于加气出口金属碟形齿回阀;H47X-2.5;DN1200","炼铁厂","只",10]
[26,7402700070,"金属垫圈","1400*1490*厚度5mm","适用于煤气加压电动插板阀;DN1400;F944X","炼铁厂","只",5]
[27,4000800865,"金属包覆垫","680*600*6","不锈钢耐高温1200度","炼铁厂","个",10]
[28,7402700051,"金属包覆垫","1215*1300","压实厚度10mm;;耐温1200度;316不锈钢包石墨","炼铁厂","片",2]
[29,7402700052,"金属包覆垫","1220*1340","压实厚度10mm;;耐温1200度;316不锈钢包石墨","炼铁厂","片",2]
[30,7402700003,"金属缠绕式垫片","直径680*直径600 厚度6mm 不锈钢 耐高温1200度","不锈钢 GB/T4622.2-2003","炼铁厂","片",10]
[31,7402500042,"密封垫圈","?445*?360*3.5/1.5/1.0/0.75","石棉橡胶板","180分厂","个",10]
[32,7402500043,"密封垫圈","0109030-23.535","软木橡胶","180分厂","个",10]
[33,7402500055,"密封圈","HJC03-400-700",null,"89分厂","只",5]
[34,7402700032,"金属包覆垫片","直径670/630*8","316不锈钢包石墨 GB/T4622.2-2003耐高温1302℃","炼铁厂","片",10]
[35,7402700033,"金属包覆垫片","直径210/160*10","316不锈钢包石墨 GB/T4622.2-2003耐高温1303℃","炼铁厂","片",10]
[36,7402700034,"金属包覆垫片","直径1300/1240*10","316不锈钢包石墨 GB/T4622.2-2003耐高温1304℃","炼铁厂","片",5]
[37,7402700035,"金属包覆垫片","直径 695/635*10","316不锈钢包石墨 GB/T4622.2-2003耐高温1305℃","炼铁厂","片",10]
[38,7402700036,"金属包覆垫片","直径325/285*10","316不锈钢包石墨 GB/T4622.2-2003耐高温1306℃","炼铁厂","片",10]
[39,7402700015,"金属包覆垫片","直径1684*直径1624*6 304/石墨橡胶+石墨 耐温≤300℃","304/石墨橡胶+石墨 GB/T15601-1995","炼铁厂","片",2]
[40,7402700019,"金属包覆垫片","直径2086*直径2026*6 304/石墨橡胶+石墨 耐温≤300℃","304/石墨橡胶+石墨 GB/T15601-1995","炼铁厂","片",2]
[41,7402500061,"金属垫圈","1000*1090*厚度5mm","适用于金属硬密封碟阀;D943P-2.5;DN1000","炼铁厂","只",10]
[42,7402500065,"缠绕式密封垫圈","325*250*3.5","基本型","炼铁厂","只",10]
[43,7402700042,"316不锈钢高温专用垫片","DN400","426/544 耐温>500℃","340分厂","片",10]
[44,7402700024,"316不锈钢高温专用垫片","DN50 57/107 耐温>500℃",null,"炼铁厂","片",100]
[45,7402700025,"316不锈钢高温专用垫片","DN65 76/127 耐温>500℃",null,"炼铁厂","片",100]
[46,7402700030,"金属包覆垫片","直径1100/1000*10","316不锈钢包石墨 GB/T4622.2-2003耐高温1300℃","炼铁厂","片",10]
[47,7402700031,"金属包覆垫片","直径1360/1290*10","316不锈钢包石墨 GB/T4622.2-2003耐高温1301℃","炼铁厂","片",2]
[48,7402700040,"金属包履垫片","CSCL","DN200","340分厂","只",10]
[49,7402700041,"金属包覆垫片","DN350",null,"340分厂","片",10]
[50,7402700043,"316不锈钢高温专用垫片","DN500","530/622 耐温>500℃","340分厂","片",10]
[51,7402700045,"316不锈钢垫片","直径65*直径35*3","16Kg/cm2","340分厂","片",100]
[52,7402700067,"316不锈钢高温专用垫片","DN300;","325/416;耐温>500℃","炼铁厂","片",10]
[53,7402700074,"金属包覆垫片","直径1380*直径1310*8","304/石墨橡胶+石墨 耐高温≤300℃","340分厂","片",5]
[54,7402700050,"缠绕式密封垫圈","118*65*3.2","118*65*3.2","89分厂","个",100]
[55,7402700075,"316不锈钢高温专用垫片","DN700;720/846;耐温>500℃",null,"340分厂","片",10]
[56,7402700076,"金属缠绕式垫片","φ1030*φ1090*8；不锈钢 耐温1200度","不锈钢 GB/T4622.2-2003","340分厂","片",10]
[57,4000801170,"热风阀用高温组合垫片","HY8400","6.3MPa；工作温度：1200℃","炼铁厂","套",1]
[58,7402700053,"金属硬密封煤气除尘人孔密封垫圈","HZ60-180/B","规格890*800","能源分厂","只",5]
[59,7402700066,"金属硬密封进出孔密封垫圈","HB2810-16K",null,"炼铁厂","只",10]
[60,7402600024,"高温高压石墨垫片","CSCLS3000","耐高温500℃；不锈钢;厚3mm","能源分厂","片",10]
[61,7402600028,"石墨垫片","CPS-316","不锈钢;直径180*125*3.2","180分厂","片",100]
[62,7402600043,"石墨垫片","CPS-316","不锈钢 直径135*80*3.2","180分厂","片",100]
[63,7402600012,"石墨垫片","直径360*300*3.2","不锈钢 GB/T9877-2008","炼铁厂","片",5]
[64,7402600014,"视孔石墨成型环","直径35*20*5",null,"炼铁厂","只",100]
[65,7402600008,"煤枪石墨成型环","直径50*21*8",null,"炼铁厂","只",50]
[66,7402600017,"石墨垫片","CPS-316;直径84*40*3","不锈钢;直径84*40*3","炼铁厂","片",50]
[67,7402600041,"石墨垫片","CPS-316","不锈钢 直径350*320*3","180分厂","片",20]
[68,7402600026,"石墨垫片","CPS-316","CPS-316;不锈钢;直径100*50*3","180分厂","片",10]
[69,7402800017,"石墨盘根","2101；20*20","石墨","炼铁厂","Kg",10]
[70,7402600017,"石墨垫片","CPS-316;直径84*40*3","不锈钢;直径84*40*3","炼铁厂","片",100]
[71,7402600033,"石墨垫片","CPS-316","不锈钢；直径210*150*3.2","89分厂","片",10]
[72,7402600040,"石墨垫片","CPS-316","不锈钢 直径56*20*3","89分厂","片",100]
[73,7402900009,"高温密封填条","*","JN5050 12*10*10","炼钢厂","根",1]
[74,7402900010,"高温密封填条","*","JN5050 50*15*16.2","炼钢厂","根",1]
[75,7402900004,"仓门盖密封条","*","H=25mm B=20mm B=20mm b=6mm 槽宽4mm 槽高15mm","炼钢厂","米",10]
[76,7402900005,"仓门盖密封条","*","H=25mm B=25mm B=25mm 发泡橡胶","炼钢厂","米",10]
[77,5400100046,"离心式空压机 中冷橡胶密封条","FS-ELLIOTT 260","铸造 氟橡胶，耐温大于250℃","能源分厂","只",1]
[78,7402900013,"密封填条","*","CSCL25GJKD18-HD12","炼铁厂","米",10]
[79,7402900002,"O型密封条","*","直径45*15 硅橡胶","炼钢厂","Kg",10]
[80,7402900062,"煤气阀凹形专用密封填条","16GJ15-9-13",null,"炼铁厂","米",15]
[81,7402900011,"密封填条","*","CSCL19R5-2FJ-26B 耐高温400度","炼铁厂","米",30]
[82,7402900012,"密封填条","*","CSCL13B-2GJ.13B耐高温400度","炼铁厂","米",30]
[83,5712300020,"侧烧嘴与炉墙密封垫","5mm 620*565*475 φ24孔均布12个",null,"340分厂","片",10]
[84,5712300221,"步进炉加热段烧嘴内密封垫","直径225*268*305*3.2","8孔20均布;耐温500℃","340分厂","个",10]
[85,5712300164,"步进炉加热段烧嘴密封垫","*","耐温500℃","340分厂","只",10]
[86,5400300024,"煤气增压机 后端油封","AII850(M)型；NO.5101-02","锻件 材质：铝","炼铁厂","付",1]
[87,7402500035,"电动盲板阀密封","F943X-1.6C","DN500","能源分厂","套",2]
[88,7402500034,"电动盲板阀密封","F943X-1.6C","DN600","89分厂","个",2]
[89,7402400002,"碟阀密封圈","H0P1-DN80","BNR","180分厂","只",10]
[90,7402400003,"蝶阀特制密封圈","DN100","直径97.8*直径137.5*56 E704","340分厂","只",10]
[91,7402400004,"蝶阀特制密封圈","DN65","直径64*直径101.5*50 E704","340分厂","只",10]
[92,7402500037,"密封垫圈","BXGJS1103295","耐高温500℃；不锈钢","能源分厂","片",10]
[93,7402500038,"高压密封垫","GJLH20026045","耐高温500℃；不锈钢","能源分厂","片",10]
[94,5712300121,"煤气管道金属硬密封垫圈","*",null,"340分厂","只",10]
[95,7402700054,"煤气管道金属硬密封垫圈","DN500","不锈钢;直径560*500*3.2","能源分厂","片",10]
[96,7402500036,"高温密封圈","CLBF45420500","耐高温500℃；不锈钢;直径500*420*45*3.2","能源分厂","片",10]
[97,7402500059,"煤气加压电动敞开式盲板阀密封垫圈","DN1200;","F944X","炼铁厂","只",5]
[98,7402100040,"高压密封组件","A-36/20.02.01.02",null,"能源分厂","套",2]
[99,7502400054,"高压泵 密封组","L-YL95.01.02",null,"管加工分厂","套",2]
[100,7402400001,"碟阀密封","HPS030009",null,"180分厂","只",10]
[101,7401700001,"端盖密封套件","*","HPS30011","180分厂","套",10]
[102,7402400002,"碟阀密封圈","H0P1-DN80","BNR","180分厂","只",5]
[103,5500100007,"炉顶放散阀密封件","HJN0901-15D","DN500 氟硅橡胶 HJN0901-15D 氟硅橡胶，耐高温400℃","炼铁厂","只",1]
[104,5500100029,"眼睛阀密封圈","直径345*直径16","氟硅橡胶 氟硅橡胶，耐高温400℃","炼铁厂","只",10]
[105,5500100017,"上密轴密封外形圈/套环","M200-36/19","45# 钢调质 一套一个分油环 三个Yx密封 分油环尺寸：φ180*φ152*15","炼铁厂","套",1]
[106,7402000039,"机械密封","CPS-MTN55","直径55mm","炼钢厂","只",2]
[107,7402000044,"机械密封","CPS-MTN90","直径90mm","720分厂","只",1]
[108,7402000035,"机械密封","MTN-50","电机功率：15KW；电压：380V；流量22t/h;扬程40米;口径65mm","能源分厂","套",2]
[109,7001800264,"水泵机械密封","SBS250-370F",null,"180分厂","套",2]
[110,7402000040,"水泵机械密封","SLOW250-390A",null,"炼钢厂","套",1]
[111,7402000041,"水泵机械密封","SLOW250-610A",null,"炼钢厂","套",1]
[112,7402000042,"水泵机械密封","SLOW200-530",null,"炼钢厂","套",1]
[113,7402000043,"水泵机械密封","SLOW300-450(I)",null,"炼钢厂","套",2]
[114,7402000029,"水泵机械密封","SLOW200-660C",null,"能源分厂","套",2]
[115,7402000036,"水泵机械密封","40ZW20-15","电机功率：15KW；电压：380V；流量22t/h;扬程40米;口径50mm","能源分厂","套",2]
[116,7402000007,"离心水泵 机械密封","SBS150-605F/523",null,"能源分厂","套",1]
[117,7001800026,"水泵机械密封","SBS200-520E/486",null,"180分厂","套",1]
[118,7001800116,"离心水泵 机械密封","SBS200-420E/415",null,"能源分厂","套",1]
[119,7001800103,"离心水泵 机械密封","MTN-70",null,"能源分厂","套",1]
[120,7402000003,"离心水泵 机械密封","SBS150-360F",null,"能源分厂","套",2]
[121,7402000015,"离心水泵 机械密封","SBL150-250IA","(内径：45mm)","能源分厂","套",2]
[122,7402000016,"离心水泵 机械密封","SBL250-315A","（内径50）","能源分厂","套",2]
[123,7402000002,"离心水泵 机械密封","SBS125-230E",null,"能源分厂","套",1]
[124,7402000001,"离心水泵 机械密封","KQSN250-M6/410","离心水泵 机械密封 KQSN250-M6/410 MG1/80-G60","能源分厂","套",2]
[125,7402000024,"离心水泵 机械密封","KQSN200-M13/188",null,"炼铁厂","套",1]
[126,5500600054,"离心水泵 机械密封","KQSN350-M9/473","MG1/90-G60","炼铁厂","套",1]
[127,7402000010,"离心水泵 机械密封","SBS200-420E/415",null,"能源分厂","套",2]
[128,7402000013,"离心水泵 机械密封","SBS350-360E/357",null,"能源分厂","套",2]
[129,7402000011,"离心水泵 机械密封","SBS300-435F/450",null,"能源分厂","套",2]
[130,7402000009,"离心水泵 机械密封","SBS200-320E/314",null,"能源分厂","套",2]
[131,7001800301,"管道泵 机械密封","40GB-A",null,"能源分厂","套",5]
[132,7402000052,"机械密封","MN206-110","100YTZX-560，硬质合金","能源分厂","套",1]
[133,7001800031,"高压泵 填料","10*10J5-75IV","75*95*10","能源分厂","件",10]
[134,7502000003,"高压泵 柱塞填料","J5-80-Ⅳ-12.5*12.5",null,"能源分厂","件",10]
[135,7402000032,"机械密封","250YTZX-650","橡胶","炼铁厂","套",1]
[136,7402000033,"P302冲渣泵;机械密封","100YTZX-500","橡胶","炼铁厂","套",1]
[137,7402000034,"机械密封","MN206-110","150YTZ-560 橡胶","炼铁厂","套",1]
[138,5500400033,"水渣渣浆泵;机械密封","MN206-100","100YTZX-500, 硬质合金","炼铁厂","套",1]
[139,7402500039,"上锅筒密封圈","3.2542E+12","耐高温500℃；不锈钢","能源分厂","片",10]
[140,7402500040,"下锅筒密封圈","2.95395E+12","耐高温500℃；不锈钢","能源分厂","片",10]
[141,5702400098,"气缸内阀板密封件","HJ-HX22509 HJ-HX22509","直径274*直径291*3.5，配金属石墨垫","180分厂","只",10]
[142,5702400099,"气缸内阀板密封件","HJ-HX22509 HJ-HX22509","直径248*直径255*3.5，配金属石墨垫","180分厂","只",10]
[143,7402500042,"密封垫圈","?445*?360*3.5/1.5/1.0/0.75","石棉橡胶板","180分厂","个",10]
[144,7402700018,"送风管道金属密封垫圈","CSCLBFD530-630/10","耐高温1200度","炼铁厂","只",10]
[145,7402700037,"送风管道金属密封垫圈","CSCLBFD620-540/10","耐高温1200度","炼铁厂","只",10]
[146,7402500010,"硅胶密封圈","电动插板阀CCF944X-0.5","DN2000用 硅橡胶 硅橡胶，4根/套，Q/HT3-2009","炼铁厂","套",1]
[147,7502400054,"高压泵 密封组","L-YL95.01.02",null,"管加工分厂","套",2]
[148,7402000022,"离心水泵 机械密封","KQSN350-N4/693","P201","炼铁厂","套",1]
[149,7402000025,"离心水泵 机械密封","KQSN600-N27/466",null,"炼铁厂","套",1]
[150,7001200246,"五柱塞往复泵;填料环甲","5XND-315-0211-D",null,"能源分厂","个",5]
[151,7001200271,"五柱塞往复泵;填料环乙","5XND-315-0212-D","材质黄铜；重量0.1Kg","能源分厂","只",5]
[152,7001200277,"高压泵;高压密封组","L-NYL01.01.02","内径83；铜件+密封件","能源分厂","件",1]
[153,7402000039,"机械密封","CPS-MTN55","直径55mm","炼钢厂","只",2]
[154,7402000044,"机械密封","CPS-MTN90","直径90mm","720分厂","只",2]
[155,7402000035,"机械密封","MTN-50","电机功率：15KW；电压：380V；流量22t/h;扬程40米;口径65mm","能源分厂","套",2]
[156,7402400003,"蝶阀特制密封圈","DN100","直径97.8*直径137.5*56 E704","340分厂","只",5]
[157,5400100032,"离心式空压机 密封套件","FS-ELLIOTT 5件套","铸造 6\",8\"×2,10\",16\",氟橡胶，耐温大于250℃","能源分厂","套",1]
[158,7001200246,"五柱塞往复泵;填料环甲","5XND-315-0211-D",null,"能源分厂","个",2]
[159,7001200271,"五柱塞往复泵;填料环乙","5XND-315-0212-D","材质黄铜；重量0.1Kg","能源分厂","只",2]
[160,7001800078,"离心水泵 机械密封","KQS N200-N5/334",null,"180分厂","套",2]
[161,7400900083,"高压泵盘根组合密封","AIGI871;  60*76*30","3个高油四氟成型密封环、2个聚甲醛支撑环   AIGI","炼钢厂","套",10]
[162,5712200110,"机械密封","0109015-24.115","1.组合件配合良好 2.满足生产要求","340分厂","套",20]
[163,5712200111,"机械密封","0109015-25.115","1.组合件配合良好 2.满足生产要求","340分厂","套",3]
[164,7402400005,"阀门耐压密封垫","D343H400.10C-P","480*420*6;材质:1Cr18Ni9","炼铁厂","片",10]
[165,5500400029,"水渣循环泵;机械密封","250YTZX-650","MN206140 硬质合金","炼铁厂","套",1]
[166,7001800026,"水泵机械密封","SBS200-520E/486",null,"180分厂","套",2]
[167,7402900061,"耐压水密封组件","A550-V1521-2VING，","夹门密封，材质：聚氨酯组合不锈钢，长2.6米，可自由弯曲","能源分厂","套",10]
[168,7001200217,"高压泵 密封组","A-25/2.01.01.02","直径80mm","89分厂","套",1]
[169,5500100017,"上密轴密封外形圈/套环","M200-36/19","45# 钢调质 一套一个分油环 三个Yx密封 分油环尺寸：φ180*φ152*15","炼铁厂","套",2]
[170,5500100019,"上下密封阀密封圈","直径700mm","氟硅橡胶 JB/T5000.1-1998 氟硅橡胶，耐高温400℃","炼铁厂","只",2]
[171,7402500033,"眼镜阀;密封圈","HJN0901-2J-16","硅橡胶","89分厂","个",5]
[172,7502000180,"高压泵;柱塞填料","3D6.5-32/20.0-IA;","浸油石棉聚四氟乙烯12.5*12.5；","能源分厂","Kg",5]
[173,5500100031,"一次均压阀密封圈","HNJ0901-15JP","DN300 氟硅橡胶 HNJ0901-15JP 氟硅橡胶，耐高温400℃","炼铁厂","只",2]
[174,5500100004,"二次均压阀密封圈","HJN0901-2J","DN150 氟硅橡胶 密封圈 HJN0901-2J 氟硅橡胶，耐高温400℃","炼铁厂","只",2]
[175,7402700073,"热风阀方法兰密封圈","不锈钢包石墨；耐高温1200℃","1850*410*6","炼铁厂","件",1]
[176,5400300025,"煤气增压机 前端油封","AII850(M)型；NO.5101-01","锻件 材质：铝","340分厂","付",1]
[177,5400300024,"煤气增压机 后端油封","AII850(M)型；NO.5101-02","锻件 材质：铝","炼铁厂","付",1]
[178,7400100503,"轴流压缩机静叶承缸专用密封","包括：外径53*3.5的O型密封圈50个；外径42*3.5的O型密封圈190个；外径52*3.5的O型密封圈40个；外径51*3.5的O型密封圈45个；外径41*3.5的O型密封圈90个；外径32*3的O型密封圈260个","氟橡胶；耐高温≥300℃","炼铁厂","套",1]
[179,7402500053,"热风炉热风阀体法兰密封垫圈","JSBFD1818.5",null,"炼铁厂","只",3]
[180,7402800038,"耐高温陶瓷钎维盘根","带不锈钢丝;12mm*12mm",null,"能源分厂","Kg",10]
[181,7402800031,"盘根","AIG26W;8*8","材质AIG26W","炼钢厂","Kg",10]
[182,7402800031,"盘根","AIG26W;8*8","材质AIG26W","炼钢厂","Kg",15]
[183,7402800005,"盘根成型环","45度切口 CPS7600 50*66*7",null,"340分厂","只",50]
[184,7001200132,"盘根成型环","45度切口;CPS7600;75*95*10",null,"219分厂","只",10]
[185,7402800032,"盘根","CPS7600-10mm","10mm","炼铁厂","Kg",10]
[186,7402800019,"盘根","CPS2113F;8*8","石墨；耐高温500℃","能源分厂","Kg",10]
[187,7402800002,"盘根","CPS7510 14*14mm","石墨","炼铁厂","Kg",10]
[188,7402800004,"盘根","CPS7600 12*12mm",null,"340分厂","Kg",10]
[189,7402800030,"盘根","2300;","12*12;PTFE","炼铁厂","Kg",10]
[190,7402800020,"盘根","CPS8900","14*14mm","炼铁厂","Kg",5]
[191,7402800021,"四角芳纶盘根","2302","增强PTFE;10*11","340分厂","Kg",5]
[192,7402800021,"四角芳纶盘根","2302","增强PTFE;10*11","炼铁厂","Kg",5]
[193,7402800021,"四角芳纶盘根","2302","增强PTFE;10*11","炼铁厂","Kg",5]
[194,3221200006,"高温高氧耐磨碳纤布","宽500mm；厚2mm","1200度","炼钢厂","米",10]
[195,3400200001,"无尘石棉布","*","厚3mm","炼钢厂","Kg",100]
[196,4000700035,"水洗混纺无尘石棉编绳","*","直径20mm；","炼钢厂","Kg",100]
[197,7402800002,"盘根","CPS7510 14*14mm","石墨","炼铁厂","Kg",10]
[198,7402800004,"盘根","CPS7600 12*12mm",null,"340分厂","Kg",10]
[199,7402800011,"液体盘根","BH-8900黑色",null,"180分厂","Kg",5]
[200,7402800014,"石墨盘根","P600110*10","石墨 耐温500℃","炼铁厂","Kg",10]
[201,7402800016,"石墨盘根","8*8","石墨","炼铁厂","Kg",10]
[202,7402800018,"碳纤维盘根","10*10",null,"炼铁厂","Kg",10]
[203,7402800029,"高压泵盘根组","AIGI15","55*71*30","89分厂","套",10]
[204,7402800030,"盘根","2300;","12*12;PTFE","炼铁厂","Kg",10]
[205,7402800006,"盘根成型环","45度切口 CPS7600 65*79.2*6.5-6.9",null,"340分厂","只",100]
[206,7402800025,"盘根成型环 45度切口","CPS7600","80*100*10","管加工分厂","只",10]
[207,5500200001,"风筒，直吹管含锆硅酸铝纤维棉垫","直径460*直径220mm,厚13mm","硅酸铝 耐高温1200℃","炼铁厂","件",10]
[208,7402900014,"含锆硅酸铝纤维棉垫","直径550*直径230mm,厚13mm",null,"炼铁厂","件",10]
[209,7402900031,"硅酸铝石棉垫","直径420*直径240*厚度15","温度大于1200℃","炼铁厂","片",10]
[210,5202300006,"煤气增压机 支撑轴瓦","AII850(M)型；NO.5101-ZC","锻件，材质为中碳铸钢ZG35+巴氏合金","炼铁厂","套",1]
[211,5202300001,"煤气增压机 支撑轴承轴瓦","AI1508.1","锻件 材质为中碳铸钢ZG35+巴氏合金","能源分厂","套",1]
[212,5202300002,"煤气增压机 支推轴承轴瓦","AI1508.2","锻件 材质为中碳铸钢ZG35+巴氏合金","能源分厂","套",1]
[213,5202300005,"煤气增压机 止推轴瓦","AII850(M)型；NO.5102-ZT","锻件，材质为中碳铸钢ZG36+巴氏合金","炼铁厂","套",1]
[214,5202300005,"煤气增压机 止推轴瓦","AII850(M)型；NO.5102-ZT","锻件，材质为中碳铸钢ZG36+巴氏合金","炼铁厂","套",1]
[215,5202300006,"煤气增压机 支撑轴瓦","AII850(M)型；NO.5101-ZC","锻件，材质为中碳铸钢ZG35+巴氏合金","炼铁厂","套",1]
[216,5712300019,"侧烧嘴密封件;非标","*",null,"340分厂","只",10]
[217,5712300020,"侧烧嘴与炉墙密封垫","5mm 620*565*475 φ24孔均布12个",null,"340分厂","片",10]
[218,5712300018,"侧烧嘴密封件","*","390*110*2","340分厂","只",5]
[219,7402900016,"密封包","*","0-RING KIT/B-1","炼铁厂","只",5]
[220,7402500055,"密封圈","HJC03-400-700",null,"89分厂","只",2]
[221,7402500055,"密封圈","HJC03-400-700",null,"89分厂","只",1]
[222,7402900007,"高温密封环","*","JN5050 50*5.1","炼钢厂","只",100]
[223,5100100456,"联轴器弹性圈","NUP285-130513","材质:聚氨酯;外径40mm,内径20mm,长度40mm;用于1#、2#、3#煤气加压机新弹性套柱销联轴器","340分厂","只",10]
[224,5712300145,"烧嘴挡火圈","*","288*110*60","340分厂","只",10]
[225,7402500060,"橡胶平垫圈","直径65/直径48-5mm",null,"炼铁厂","只",100]
[226,7402900041,"耐高温专用密封","FB60*80*8","JN5050 CSCL","340分厂","只",10]
[227,7402900042,"耐高温专用密封","FB60*90*12","JN5050 CSCL","340分厂","只",10]
[228,7402900043,"耐高温专用密封","FB80*100*12","JN5050 CSCL","340分厂","只",10]
[229,7402500004,"硅胶密封圈","电动插板阀F941X-0.5-2000用","硅橡胶 硅橡胶，Q/HT3-2009","炼铁厂","只",2]
[230,7402500005,"硅胶密封圈","电动插板阀F941X-2.5-1600用","硅橡胶 硅橡胶，Q/HT3-2009","炼铁厂","只",5]
[231,7402600008,"煤枪石墨成型环","直径50*21*8",null,"炼铁厂","只",50]
[232,7402500062,"密封垫","BJLM-100","DN100；硅橡胶；使用温度100度； 压力；PN10","炼铁厂","只",10]
[233,7402500060,"橡胶平垫圈","直径65/直径48-5mm",null,"炼铁厂","只",100]
[234,7402900023,"BSB基础密封","HOP-PE42-3500","U203","340分厂","只",5]
[235,7402900022,"BSB型基础密封","HOP-PE32-49000","U203含胶粘剂","340分厂","只",5]
[236,7402900059,"BSB型基础密封","HOP-PE32-36767;U203","替换原O型圈尺寸为367.67*7","340分厂","只",2]
[237,7401900139,"J型油封","390*430*20","HG4-338-1966","89分厂","只",20]
[238,7400100321,"O型密封圈","直径20*3.55",null,"炼钢厂","只",200]
[239,7400100148,"O型密封圈","直径40*3.55 NBR",null,"炼钢厂","只",100]
[240,7400100159,"O型密封圈","直径49.60*5.70 NBR",null,"炼钢厂","只",200]
[241,7400100149,"O型密封圈","直径40*5.3 硅橡胶",null,"炼钢厂","只",100]
[242,7400100055,"O型密封圈","直径18*1.8G NBR",null,"炼钢厂","只",200]
[243,7400100249,"O型密封圈","直径9.25*1.78 NBR",null,"炼钢厂","只",100]
[244,7400100276,"O型密封圈","内径10.82*1.78 NBR",null,"炼钢厂","只",100]
[245,7400100318,"O型密封圈","直径351.5*5.3G",null,"炼钢厂","只",20]
[246,7400100320,"O型密封圈","直径231.4*5.3G",null,"炼钢厂","只",50]
[247,7400100225,"O型密封圈","ID56.7*3.55 NBR",null,"340分厂","只",100]
[248,7400100223,"O型密封圈","ID47.2*3.55 NBR",null,"340分厂","只",100]
[249,7400100202,"O型密封圈","ID7.5*1.5 NBR",null,"炼钢厂","只",200]
[250,7400100248,"O型密封圈","直径9.0*1.5 NBR",null,"炼钢厂","只",200]
[251,7400100212,"O型密封圈","ID6*1.5 NBR",null,"炼钢厂","只",200]
[252,7400100191,"O型密封圈","直径7.5*1.5 NBR",null,"180分厂","只",200]
[253,7400100179,"O型密封圈","直径6.0*1.5 NBR",null,"180分厂","只",200]
[254,7400100210,"O型密封圈","ID46.0*3.0 NBR",null,"炼钢厂","只",200]
[255,7400100209,"O型密封圈","ID38.0*2.5 NBR",null,"炼钢厂","只",100]
[256,7400100020,"O型密封圈","直径12.0*2.0 NBR",null,"炼钢厂","只",100]
[257,7400100208,"O型密封圈","ID26.0*2 NBR",null,"炼钢厂","只",100]
[258,7400100047,"O型密封圈","直径16.3*2.4 NBR",null,"炼钢厂","只",100]
[259,7400100074,"O型密封圈","直径20.3*2.4 NBR",null,"340分厂","只",100]
[260,7400100217,"O型密封圈","ID33.3*2.5 NBR",null,"340分厂","只",100]
[261,7400100209,"O型密封圈","ID38.0*2.5 NBR",null,"炼钢厂","只",100]
[262,7400100020,"O型密封圈","直径12.0*2.0 NBR",null,"炼钢厂","只",100]
[263,7400100208,"O型密封圈","ID26.0*2 NBR",null,"炼钢厂","只",100]
[264,7400100047,"O型密封圈","直径16.3*2.4 NBR",null,"炼钢厂","只",100]
[265,7400100074,"O型密封圈","直径20.3*2.4 NBR",null,"340分厂","只",100]
[266,7400100216,"O型密封圈","ID25.3*2.4 NBR",null,"340分厂","只",100]
[267,7400100214,"O型密封圈","ID20.3*2.4 NBR",null,"340分厂","只",100]
[268,7400100203,"O型密封圈","ID9*1.5 NBR",null,"炼钢厂","只",100]
[269,7400100228,"O型密封圈","ID9.25*1.78 NBR",null,"炼钢厂","只",100]
[270,7400100271,"O型密封圈","直径22.0*1.80A",null,"炼钢厂","只",100]
[271,7400100205,"O型密封圈","ID16.3*2.4 NBR",null,"炼钢厂","只",100]
[272,7400100215,"O型密封圈","ID18.7*3.55 NBR",null,"炼钢厂","只",100]
[273,7400100204,"O型密封圈","ID10*2 NBR",null,"炼钢厂","只",100]
[274,7400100211,"O型密封圈","ID12*2 NBR",null,"340分厂","只",100]
[275,7400100070,"O型密封圈","直径20*2.65 NBR",null,"炼钢厂","只",100]
[276,7400100086,"O型密封圈","直径24*2.4 NBR",null,"炼钢厂","只",100]
[277,7400100002,"O型密封圈","直径10*2 NBR",null,"炼钢厂","只",100]
[278,7400100108,"O型密封圈","直径30*2.4 NBR",null,"炼钢厂","只",100]
[279,7400100069,"O型密封圈","直径20*2.4 NBR",null,"炼钢厂","只",100]
[280,7400100030,"O型密封圈","直径13.2*2.65 NBR",null,"炼钢厂","只",100]
[281,7400100226,"O型密封圈","ID8*1.5 NBR",null,"180分厂","只",100]
[282,7400100034,"O型密封圈","直径14*2.4 NBR",null,"炼钢厂","只",100]
[283,7400100163,"O型密封圈","直径50*3.5 NBR",null,"炼钢厂","只",100]
[284,7400100076,"O型密封圈","直径22*2.4 NBR",null,"炼钢厂","只",100]
[285,7400100230,"O型密封圈","ID27*3 NBR",null,"炼钢厂","只",100]
[286,7400100229,"O型密封圈","ID19*3 NBR",null,"炼钢厂","只",100]
[287,7400100105,"O型密封圈","AO88363 直径28.17*3.53  NBR",null,"炼钢厂","只",100]
[288,7400100153,"O型密封圈","直径45*3.1 NBR",null,"炼钢厂","只",100]
[289,7400100110,"O型密封圈","直径30*3.1 NBR",null,"炼钢厂","只",100]
[290,7400100123,"O型密封圈","直径35*3.5 NBR",null,"炼钢厂","只",100]
[291,7400100147,"O型密封圈","直径40*3.5 NBR",null,"炼钢厂","只",100]
[292,7400100044,"O型密封圈","直径16*2.4 NBR",null,"炼钢厂","只",100]
[293,7400100154,"O型密封圈","直径45*3.5 NBR",null,"炼钢厂","只",100]
[294,7400100231,"O型密封圈","直径8*1.9 NBR",null,"炼钢厂","只",100]
[295,7400100161,"O型密封圈","直径5*1.9 NBR",null,"炼钢厂","只",100]
[296,7400100177,"O型密封圈","直径6*1.2 NBR",null,"炼钢厂","只",100]
[297,7400100190,"O型密封圈","直径7*1.9 NBR",null,"炼钢厂","只",100]
[298,7400100001,"O型密封圈","直径10*1.9 NBR",null,"炼钢厂","只",100]
[299,7400100178,"O型密封圈","直径6*1.9 NBR",null,"炼钢厂","只",100]
[300,7400100335,"O型密封圈","直径46*5.3 NBR",null,"340分厂","只",100]
[301,7400100176,"O型密封圈","直径53*5.3 PTFE",null,"340分厂","只",100]
[302,7400100151,"O型密封圈","直径42*3.5 NBR",null,"炼钢厂","只",100]
[303,7400100380,"O型密封圈","直径17.12*2.62;NBR",null,"180分厂","只",100]
[304,7400100378,"O型密封圈","直径10.0*2;NBR",null,"180分厂","只",100]
[305,7400100243,"O型密封圈","ID17.12*2.62 NBR",null,"炼钢厂","只",100]
[306,7400100170,"O型密封圈","直径54*5 NBR",null,"炼钢厂","只",20]
[307,7400100197,"O型密封圈","直径72*4 NBR",null,"炼钢厂","只",100]
[308,7400100222,"O型密封圈","ID110.7*3.55 NBR",null,"炼钢厂","只",100]
[309,7400100130,"O型密封圈","直径205*3.1 NBR",null,"180分厂","只",50]
[310,7400100023,"O型密封圈","直径120*3 NBR",null,"180分厂","只",100]
[311,7400100314,"O型密封圈","直径195*2.5 1013455 NBR72","橡胶","180分厂","只",100]
[312,7400100025,"O型密封圈","直径125*3.1 NBR",null,"炼钢厂","只",100]
[313,7400100090,"O型密封圈","直径25.3*2.4 NBR",null,"炼钢厂","只",100]
[314,7400100235,"O型密封圈","直径80*5.3G",null,"炼钢厂","只",50]
[315,7400100189,"O型密封圈","直径7*1.2 NBR",null,"炼钢厂","只",100]
[316,7402900002,"O型密封条","*","直径45*15 硅橡胶","炼钢厂","Kg",50]
[317,7400600069,"U形圈","53*61*4.5","聚氨酯","340分厂","只",20]
[318,7400600005,"U型密封圈","ODU70*82*14 BNR",null,"180分厂","只",20]
[319,7400600007,"U型密封圈","USH00360 36*46*45*7 N901",null,"炼钢厂","只",20]
[320,7400600006,"U型密封圈","UPH00700 70*90*89*13 N901",null,"炼钢厂","只",20]
[321,7400600012,"U型密封圈","USH00960 90*105*103*10 N901",null,"340分厂","只",20]
[322,7400600026,"U型油封","B45*65*8",null,"炼铁厂","只",100]
[323,7400600027,"U型油封","140*170*14",null,"炼铁厂","只",10]
[324,7400700006,"V型密封圈","CPS-V89-40*25*11.5",null,"炼钢厂","只",20]
[325,7400700026,"V型组合密封","PVE00501 50*70*30 NB83",null,"炼钢厂","只",20]
[326,7400700025,"V型组合密封","PVE00650 65*80*22.5 NB83",null,"炼钢厂","只",10]
[327,7400700011,"V型组合密封","CPS-V89-100*80*21.2",null,"炼钢厂","只",10]
[328,7400700034,"V型组合密封","PVE01600 160*130*158.5*29 NB83",null,"炼钢厂","只",10]
[329,7400700017,"V型组合密封","CPS-V89-56*71*22.5",null,"炼钢厂","只",20]
[330,7400700018,"V型组合密封","CPS-V89-70*85*22.5",null,"炼钢厂","只",20]
[331,7400700014,"V型组合密封","CPS-V89-80*60*15.2",null,"炼钢厂","只",20]
[332,7400700013,"V型组合密封","CPS-V89-63*48*13",null,"炼钢厂","只",20]
[333,7400700019,"V型组合密封","CPS-V89-90*105*22.5",null,"炼钢厂","只",20]
[334,7400700012,"V型组合密封","CPS-V89-50*35*11.5",null,"炼钢厂","只",50]
[335,7400700040,"V型组合密封","PVE01800 180*150*32 NB83",null,"炼钢厂","只",20]
[336,7400700032,"V型组合密封","PVE01100 110*125*30 NB83",null,"炼钢厂","只",20]
[337,7400700041,"V型组合密封","RVE01001 100*120*40 NB83",null,"炼钢厂","只",10]
[338,7400700037,"V型组合密封","PVE01000 100*80*99*21.2 NB83",null,"炼钢厂","只",20]
[339,7400700036,"V型组合密封","PVE00900 90*70*89*21.2 NB83",null,"炼钢厂","只",10]
[340,7400700061,"V型组合密封","CPS-V89-36*48*22.5","36*48*22.5","炼钢厂","只",20]
[341,7400700033,"V型组合密封","PVE00800 80*60*79*15.2 NB83",null,"340分厂","只",20]
[342,7400700060,"V型组合密封(活塞用)","CPS-V89-140*115*25.8","GB/T9877-2008","340分厂","只",20]
[343,7400900076,"V型组合圈","RVE00320","32*44*22.5","炼钢厂","只",10]
[344,7400700048,"V型组合圈","RVE00500","NB83;50*65*22.5","炼钢厂","只",10]
[345,7400700066,"V型组合圈","40*50*12.5","材质NB83;夹布V组","340分厂","只",50]
[346,7400800021,"Yx密封圈","d56",null,"180分厂","只",50]
[347,7400800023,"Yx密封圈","d70 橡塑",null,"炼钢厂","只",20]
[348,7400800031,"Yx密封圈","D100 橡塑 XHL-01-100",null,"219分厂","只",50]
[349,7400800013,"Yx密封圈","D220 橡塑 XHL-01-220",null,"炼钢厂","只",20]
[350,7400800002,"Yx密封圈","d100 橡塑 XHL-02-100",null,"炼钢厂","只",100]
[351,7400800045,"Y型密封圈","USH00450","45*55**54N901","89分厂","只",50]
[352,7402700050,"缠绕式密封垫圈","118*65*3.2","118*65*3.2","89分厂","个",20]
[353,7402500008,"缠绕式密封垫圈","92*40*3.2",null,"340分厂","只",50]
[354,5712300021,"缠绕式密封垫圈","*","106*63*3.2","340分厂","只",20]
[355,7402500008,"缠绕式密封垫圈","92*40*3.2",null,"340分厂","只",20]
[356,7402300010,"辰型密封圈","FB170*200*15 NBR",null,"180分厂","只",50]
[357,7402300012,"辰型密封圈","FB220*250*15;NBR;GB9877.1-88","FB220*250*15;NBR","炼钢厂","只",20]
[358,7402300013,"辰型密封圈","FB240*270*15;NBR;GB9877.1-88","FB240*270*15;NBR","炼钢厂","只",20]
[359,7402300009,"辰型密封圈","FB130*160*12 NBR",null,"炼钢厂","只",50]
[360,7402000038,"出轴油封","JRTKA87","85*140*15","炼钢厂","只",20]
[361,7402000037,"出轴油封","JRTKA107R77","118*150*12","炼钢厂","只",50]
[362,7402300003,"唇形密封圈","280*310*15",null,"180分厂","只",20]
[363,7001800252,"弹性圈","ISO9001:2000","24*44*10橡胶","180分厂","只",100]
[364,7502900100,"弹性圈","18*35*10橡胶",null,"180分厂","只",100]
[365,5100100004,"弹性圈","DIS4163.3","新天然橡胶","炼铁厂","只",100]
[366,7402900047,"导向带","WRL0150025P",null,"炼钢厂","卷",5]
[367,7401100007,"导向带","WG30  DIN53454","ZP983","89分厂","米",20]
[368,7401100008,"导向带","WG47  DIN53454","ZP983","89分厂","米",10]
[369,7401100009,"导向带","WG51  DIN53454","ZP983","89分厂","米",10]
[370,5717100009,"导向环","24315102","KB660*652*25","340分厂","只",10]
[371,7401900175,"反螺旋双层油封","*","140*165*12;氟橡胶","180分厂","只",5]
[372,7401900176,"反螺旋双层油封","*","128*150*15;氟橡胶","180分厂","只",5]
[373,7401900174,"反螺旋双层油封","*","130*155*10;氟橡胶","180分厂","只",5]
[374,7401500009,"防尘圈","WP601600 160*175*167.6*10.2 N842",null,"炼钢厂","只",100]
[375,7401500005,"防尘圈","WP600280 28*36.6*31 N842",null,"340分厂","只",150]
[376,7401500003,"防尘圈","WP600500 50*60.6*53*5.3*2.2 N842",null,"炼钢厂","只",50]
[377,7401500017,"防尘圈","WP600900 90*102.2*96 N842",null,"炼钢厂","只",50]
[378,7401500015,"防尘圈","WP600360 36*44.6*39 N842",null,"炼钢厂","只",100]
[379,7401500002,"防尘圈","WP600560 56*66.6*59 N842",null,"炼钢厂","只",100]
[380,7401500016,"防尘圈","WP600450 45*55.6*48 N842",null,"炼钢厂","只",100]
[381,7401500040,"防尘圈","P6-70*80.6*7","NBR；MERKEL","89分厂","只",50]
[382,7401500038,"防尘圈","P6-56/66.6*5.3*7","NBR","89分厂","只",50]
[383,7401500019,"防尘圈","WP601100 110*122.2*116 N842",null,"炼钢厂","只",50]
[384,7401500023,"防尘圈","WP600320 32*40.6*35*5.3",null,"炼钢厂","只",100]
[385,7401500050,"防尘圈","PU6-140*155*16",null,"340分厂","只",50]
[386,7401500034,"防尘圈","350*366*9.5","可耐压力120MPa；热收缩效应小。","管加工分厂","只",10]
[387,7401500058,"防尘圈","DHS45","45*55*6","180分厂","只",50]
[388,7400800047,"防尘圈","80*92.2*7.2*12","PU6","炼钢厂","只",50]
[389,7401500026,"防尘圈","P6-55*65*5*7 NBR",null,"340分厂","只",50]
[390,7401500063,"防尘圈","ES56153-2500-46-377-8307;250*266*9.5","250*266*9.5","340分厂","只",5]
[391,7401500065,"防尘圈","WP602000;200*220*210*10.2","材质丁晴橡胶","340分厂","只",20]
[392,7401500032,"防尘圈","P6-100*112.2*12",null,"340分厂","只",50]
[393,7001800028,"高压泵 O型密封圈","*","NBR 直径112*5.7","能源分厂","只",50]
[394,7101800167,"高压泵挡圈","D305*D291.2*2.5",null,"管加工分厂","只",10]
[395,7400400008,"格来圈","AKR0500390042","PTFE","89分厂","只",50]
[396,7400400007,"格来圈","AKR0400290042","PTFE","89分厂","只",20]
[397,7400400015,"格莱圈","PG00630","63*52*6.3","340分厂","只",20]
[398,7400400013,"格莱圈","AIG410A;100*84.5*6.3;A201",null,"219分厂","只",20]
[399,7401900014,"骨架油封","120*150*14 NBR",null,"炼钢厂","只",50]
[400,7401900170,"骨架油封","FB75*95*10","NBR","管加工分厂","只",100]
[401,7401900044,"骨架油封","85*110*12 NBR",null,"炼钢厂","只",50]
[402,7401900034,"骨架油封","PD90*120*12 NBR",null,"180分厂","只",50]
[403,7401900066,"骨架油封","70*95*10",null,"180分厂","只",50]
[404,5700400069,"骨架油封","JB2600-80","170*200*15 NBR","89分厂","只",20]
[405,7401900020,"骨架油封","200*230*16 NBR",null,"炼钢厂","只",10]
[406,7401900087,"骨架油封","DIN3760-A220*250*15 NBR",null,"340分厂","只",10]
[407,7401900004,"骨架油封","FB200*230*15",null,"炼钢厂","只",20]
[408,7401900177,"骨架油封","0109015-24.125","470*420*22","340分厂","只",10]
[409,7401900122,"骨架油封","30*62*7","NBR","89分厂","只",50]
[410,7401900003,"骨架油封","FB85*110*12 NBR",null,"炼钢厂","只",50]
[411,7401900038,"骨架油封","62*120*12",null,"180分厂","只",20]
[412,7401900112,"骨架油封","FB500*540*20B2;2544;NBR","NBR;GB13781-1992","340分厂","个",2]
[413,7401900082,"骨架油封","150*180*14 AB4624A0 NOK",null,"炼钢厂","只",100]
[414,7401900142,"骨架油封","GB13781-1992","NBR TC65*90*12","炼钢厂","只",100]
[415,7401900056,"骨架油封","FB70*90*10",null,"炼钢厂","只",100]
[416,7401900041,"骨架油封","70*95*12 NBR",null,"炼钢厂","只",100]
[417,7401900045,"骨架油封","52*100*10",null,"180分厂","只",100]
[418,7401900129,"骨架油封","FB200*230*15",null,"340分厂","个",50]
[419,7401900053,"骨架油封","FB130*160*12 NBR",null,"炼钢厂","只",50]
[420,7401900206,"骨架油封","0106008-10.464","185*210*13;NBR","炼钢厂","只",100]
[421,7401900211,"骨架油封","640*704*25","80NBR709","炼钢厂","只",5]
[422,7401900214,"骨架油封","B160*190*15",null,"炼钢厂","只",100]
[423,7401900048,"骨架油封","FB100*125*10 NBR",null,"炼铁厂","只",100]
[424,7401900076,"骨架油封","PD160*200*16NBR",null,"炼钢厂","只",50]
[425,7401900123,"骨架油封","55*75*12","NBR","89分厂","只",100]
[426,7401900021,"骨架油封","240*280*18 NBR",null,"180分厂","只",20]
[427,7401900069,"骨架油封","120*160*12 NBR",null,"炼铁厂","只",20]
[428,7401900067,"骨架油封","FB90*125*12 NBR",null,"180分厂","只",30]
[429,7401900205,"骨架油封","0106008-10.463","215*240*12;NBR","180分厂","只",20]
[430,7401900033,"骨架油封","60*85*12 NBR",null,"炼钢厂","只",100]
[431,7401900094,"骨架油封","PG63*85*10 NBR",null,"炼钢厂","只",25]
[432,7401900080,"骨架油封","0109015-25.125","364*320*20","炼钢厂","只",10]
[433,7401900050,"骨架油封","95*120*12 NBR",null,"180分厂","只",100]
[434,7401900168,"骨架油封","50*70*8","NBR","89分厂","只",100]
[435,7401900151,"骨架油封","FB60*80*10",null,"340分厂","只",100]
[436,7401900108,"骨架油封","45*70*8;NBR","材质聚氨酯；使用温度-30-120摄氏度；耐磨性较好","管加工分厂","只",20]
[437,7401900031,"骨架油封","65*90*12 NBR",null,"炼铁厂","只",20]
[438,7401900113,"骨架油封","SG75*100*12","NBR;GB13781-1992","219分厂","个",20]
[439,7401900037,"骨架油封","35*55*8 NBR",null,"炼钢厂","只",100]
[440,7401900180,"骨架油封","60*85*12","60*85*12；NBR","炼铁厂","只",100]
[441,7401900178,"骨架油封","PG55*75*12","PG55*75*12；NBR","炼铁厂","只",100]
[442,7401900179,"骨架油封","75*95*12","75*95*12；NBR","炼铁厂","只",100]
[443,7401900188,"骨架油封","FB280*320*20",null,"炼铁厂","件",20]
[444,7401900191,"骨架油封","310*370*25","AD5675A0;NOK","炼铁厂","只",5]
[445,7401900190,"骨架油封","FB175*215*16B2U;23397;NBR","NBR;GB13781-1992","炼铁厂","个",20]
[446,7401900096,"骨架油封","SD300*340*18 NBR",null,"炼铁厂","只",10]
[447,7401900010,"骨架油封","120*150*16 NBR",null,"炼铁厂","只",50]
[448,7401900080,"骨架油封","0109015-25.125","364*320*20","炼钢厂","只",20]
[449,7401900185,"骨架油封","B4560；60*45*12",null,"炼钢厂","只",50]
[450,7401900189,"骨架油封","FB250*280*15;NBR;478708;GB13871-1992","GB13871-1992","炼铁厂","个",10]
[451,7401900126,"骨架油封","TC120*140*12","NBR","89分厂","只",50]
[452,7401900201,"骨架油封","50*70*12;NBR","GB13781-1992","180分厂","只",20]
[453,7401900106,"骨架油封","FB35*50*8",null,"340分厂","只",50]
[454,7401900016,"骨架油封","140*170*16 NBR",null,"炼钢厂","只",50]
[455,7401900205,"骨架油封","0106008-10.463","215*240*12;NBR","340分厂","只",20]
[456,7401900019,"骨架油封","135*170*12",null,"炼钢厂","只",20]
[457,5700100163,"骨架油封","115*140*12","GB13781-1992","340分厂","件",20]
[458,5700900043,"骨架油封","*","PD220*260*18 NBR","89分厂","只",20]
[459,7401900146,"骨架油封","250*280*15","478708 NBR","340分厂","只",20]
[460,7401900117,"骨架油封","CPS511-620*670*22",null,"340分厂","个",5]
[461,7401900192,"骨架油封GB/T9877.1-88","35*50*7","可以在20兆帕工作环境下不漏油","炼钢厂","只",50]
[462,7401900080,"骨架油封","0109015-25.125","364*320*20","89分厂","只",10]
[463,7401900073,"油封","AB6111A0 480*540*25",null,"炼钢厂","只",2]
[464,7401900074,"油封","AD5994A0 430*480*25",null,"炼钢厂","只",2]
[465,7401900138,"内骨架油封","*","358*320*20","720分厂","只",10]
[466,7401900184,"定径机输出轴骨架油封","DIN3760-A220*250*15","DIN3760-A220*250*15；NBR;NOK","340分厂","只",10]
[467,7400900078,"鼓型基础密封圈","BHT-P200-005400","抗高温水解聚氨脂;直径540","340分厂","只",2]
[468,7400900035,"滑动环","PG00800;80*64.5*6.3;ZP983/N751/F740",null,"219分厂","只",10]
[469,7400900037,"滑动环","PG01250;125*109.5*6.3;ZP983/N751/F740",null,"219分厂","只",10]
[470,7402900027,"滑动环","RS00700 德国DIN","70*85.5*6.3 ZP983/N751/F740","340分厂","只",20]
[471,7400600033,"活塞杆密封","USH-80*90*89 N901",null,"180分厂","只",20]
[472,7400300001,"活塞杆密封","*",null,"180分厂","只",50]
[473,7401400020,"活塞杆密封","OMS-MR28/35.3*3.2 NBR",null,"340分厂","只",100]
[474,7401400039,"活塞杆密封","CU0619K0；USH50*60*6；A505",null,"89分厂","只",20]
[475,7401400041,"活塞杆密封","36*47*4.2;H905/N751;RS00360",null,"340分厂","只",50]
[476,7400900069,"活塞杆密封","RVE00900","90*105*22.5*5;NB83","720分厂","套",20]
[477,7401400042,"活塞杆密封","RS00900","90*105.5*6.3 ZP983/N751","炼钢厂","只",50]
[478,7400900065,"活塞杆密封","RVE00360","36*48*22.5*4;NB83","720分厂","套",20]
[479,7400900074,"活塞杆密封","140*165*40;","NB83;RVE01401","炼钢厂","只",10]
[480,7400900063,"活塞杆密封","USH-36*46*6","A505;NOK","180分厂","只",50]
[481,7401400021,"活塞杆密封","OMS-MR36/43.3*3.2 NBR",null,"340分厂","只",50]
[482,7401400040,"活塞杆密封","USH56/66*6；A505",null,"89分厂","只",50]
[483,7400300003,"活塞杆密封","OMS-MR56/66.7/4.2 NBR",null,"180分厂","只",10]
[484,7400600035,"活塞杆密封","USH00560+挡圈",null,"180分厂","只",20]
[485,7401400007,"活塞杆密封","RS00280 28*39*4.2","RS00280 28*39*4.2 ZP983/N751 ZP983/N751/F740","炼钢厂","只",50]
[486,7401400035,"活塞杆密封","USH-70*80*6;A505;NOK",null,"89分厂","件",50]
[487,7400600063,"活塞杆密封","UHS45","45*55*6","180分厂","只",50]
[488,7401400025,"活塞杆密封","USH-32*42*6",null,"340分厂","只",50]
[489,7400300002,"活塞杆密封","RS00320 32*43*4.2 ZP983/N751",null,"180分厂","只",20]
[490,7401400025,"活塞杆密封","USH-32*42*6",null,"340分厂","只",50]
[491,7401400031,"活塞杆密封","OMK-MR580*555.5*7.7",null,"340分厂","只",10]
[492,7401300018,"活塞密封","OMK-MR63/52*4.2 NBR",null,"340分厂","只",20]
[493,7401300017,"活塞密封","OMK-MR40/29*4.2 NBR",null,"340分厂","只",20]
[494,7401300019,"活塞密封","OMK-MR80/64.5*6.3 NBR",null,"340分厂","只",20]
[495,7401900172,"活塞密封","90*74.5*6.3;Z04",null,"340分厂","只",50]
[496,7400700049,"活塞密封","RVE01100;110*125*40.0*6","NB83","340分厂","只",10]
[497,7401300025,"活塞密封","RVE001000","NB83;100*115*30.0*5","炼钢厂","套",10]
[498,7401300013,"活塞密封","PAS01250 125*103*121*26.5*5.1 N842/PN24/P12",null,"炼钢厂","只",20]
[499,7401300032,"活塞密封","PG01250","125*109.5*6.3 ZP983/N751","炼钢厂","只",100]
[500,7401300004,"活塞密封","PG00400 40*29*4.2 ZP983/N751/F740",null,"炼钢厂","只",100]
[501,7401300020,"活塞密封","TPM248185-63*47*18.3*6.4 NBR",null,"340分厂","只",50]
[502,7401300031,"活塞密封","APR1063048009",null,"89分厂","只",20]
[503,7400700045,"活塞密封","RVE001400;140*155*34.0*6;NB83",null,"炼铁厂","套",20]
[504,7401300006,"活塞密封","PG00630 63*52*4.2 ZP983/N751/F740",null,"炼钢厂","只",20]
[505,7401300022,"活塞密封","DMK-MR660*635.5*7.7 24275495",null,"340分厂","只",5]
[506,7400600070,"活塞密封","UPI;100*125*15;NOK","NBR","340分厂","只",10]
[507,7400700047,"活塞密封","RVE02000;200*220*40.0*6;NB83",null,"340分厂","套",10]
[508,7401300043,"活塞密封","125*100*25.4*6.35","进口密封","340分厂","套",5]
[509,5100100010,"蓝色聚胺酯六角联轴器弹性缓冲垫","79*40*16-6","聚氨酯","炼铁厂","只",10]
[510,5100100038,"联轴器橡胶弹性体","80*150*230","新天然橡胶","炼铁厂","只",15]
[511,7400600071,"炼钢结晶器振动台密封圈","UN65;氟橡胶",null,"炼钢厂","只",10]
[512,7401900107,"螺旋剖分油封","AIGI522S 170*200*15 重载型",null,"340分厂","只",5]
[513,7502200017,"梅花形弹性圈","GR-55",null,"180分厂","只",10]
[514,7400200019,"密封挡圈;直径70*直径80*2.0","直径70*直径80*2.0",null,"180分厂","只",10]
[515,7402100058,"密封圈","VD200A180*210*14.3/25",null,"180分厂","只",50]
[516,7401900203,"密封圈","GMAY-120*150*12-N10175","FPM/高温复合材料","340分厂","只",10]
[517,7401900202,"密封圈","GMAY-110*140*12-N10175","FPM/高温复合材料","340分厂","只",5]
[518,7400900082,"密封圈","CMAY-90*110*12-P300组合件","高温复合材料：工作温度：-90°C ～ 250℃","340分厂","只",20]
[519,7400900079,"密封圈","CMAY-130*150*12-P300组合件","高温复合材料：工作温度：-90°C ～ 250℃","340分厂","只",20]
[520,7401900102,"双剖分油封","AIG5505H 300*340*18 A100+A203",null,"340分厂","只",5]
[521,7400300007,"斯特封","350*374*8.1",null,"炼钢厂","只",10]
[522,7400300008,"斯特圈","AIG410B;35*46*4.2;A203+VITON",null,"炼铁厂","只",20]
[523,7402500056,"通用密封","USH00300","30*40*39*7 N901","89分厂","只",50]
[524,7402500057,"通用密封","USH00400","40*50*49*7 N901","89分厂","只",20]
[525,7402500054,"橡胶密封垫","直径48*直径32*6",null,"炼铁厂","只",100]
[526,7402300011,"旋转轴唇形密封圈","65*90*10",null,"340分厂","只",50]
[527,7402300006,"旋转轴轴封","R35 430*480*22 NBR",null,"180分厂","只",10]
[528,7401000007,"液压缸密封","HY89G19-234E","氟橡胶","89分厂","套",10]
[529,7401000005,"液压缸密封","BG-D-K-F80-478度-Y",null,"180分厂","套",5]
[530,7401900132,"油封","240*270*15;","BAUMSLX7;NBR","219分厂","个",20]
[531,7401900137,"油封","300*340*16","BAUSLX7;NBR","219分厂","个",20]
[532,7401900209,"油封","AB6315AO","650*720*25","180分厂","只",5]
[533,7401900156,"油封","270*330*25  AB5523AO",null,"340分厂","只",5]
[534,7401900159,"油封","380*440*25 NOK AB5888A0",null,"340分厂","只",2]
[535,7401900208,"油封","AC5461E6","SC260*300*20","340分厂","件",10]
[536,7401900209,"油封","AB6315AO","650*720*25","340分厂","只",5]
[537,7401900074,"油封","AD5994A0 430*480*25",null,"炼钢厂","只",10]
[538,7400900061,"轴用V型组合密封圈","S01-200*230*53.3",null,"管加工分厂","只",10]
[539,7400500026,"组合垫圈","d8 PTFE",null,"炼钢厂","只",100]
[540,7400500002,"组合垫圈","d10 PTFE",null,"炼钢厂","只",100]
[541,7400500021,"组合垫圈","d52 PTFE",null,"炼钢厂","只",100]
[542,7400500019,"组合垫圈","d48 PTFE",null,"炼钢厂","只",100]
[543,7400500006,"组合垫圈","d18 PTFE",null,"炼钢厂","只",100]
[544,7400500017,"组合垫圈","d42 PTFE",null,"炼钢厂","只",100]
[545,7400500010,"组合垫圈","d25 PTFE",null,"炼钢厂","只",100]
[546,7400500015,"组合垫圈","d38 PTFE",null,"炼钢厂","只",100]
[547,7400500018,"组合垫圈","d45 PTFE",null,"炼钢厂","只",100]
[548,7400500005,"组合垫圈","d16 PTFE",null,"炼钢厂","只",100]
[549,7400500008,"组合垫圈","d22 PTFE",null,"炼钢厂","只",100]
[550,7400500009,"组合垫圈","d24 PTFE",null,"炼钢厂","只",100]
[551,7400500012,"组合垫圈","d30 PTFE",null,"炼钢厂","只",100]
[552,7400500001,"组合垫圈","d35 PTFE",null,"炼钢厂","只",100]
[553,7400500013,"组合垫圈","d32 PTFE",null,"炼钢厂","只",100]
[554,7400500007,"组合垫圈","d20 PTFE",null,"炼钢厂","只",100]
[555,7400500011,"组合垫圈","d27 PTFE",null,"炼钢厂","只",100]
[556,7400500003,"组合垫圈","d12 PTFE",null,"炼钢厂","只",100]
[557,7400500004,"组合垫圈","d14 PTFE",null,"炼钢厂","只",100]
[558,7400500020,"组合垫圈","d50 PTFE",null,"炼钢厂","只",100]
[559,7400500022,"组合垫圈","d60 PTFE",null,"炼钢厂","只",100]
[560,7400900072,"组合密封","SGKD34063000+SFA52063004;","D63;HUNGER","89分厂","套",10]
[561,7400900075,"组合密封","SGKD34125000+SFA52125004","D125;HUNGER","89分厂","套",5]
[562,7400500038,"组合密封圈","直径14 NBR",null,"炼钢厂","只",100]
[563,7400500039,"组合密封圈","直径16 NBR",null,"炼钢厂","只",100]
[564,7400500037,"组合密封圈","直径12 NBR",null,"炼钢厂","只",100]
[565,7400500036,"组合密封圈","直径10 NBR",null,"炼钢厂","只",100]
[566,7400500044,"组合密封圈","直径30 NBR",null,"炼钢厂","只",100]
[567,7400500042,"组合密封圈","直径22 NBR",null,"炼钢厂","只",100]
[568,7400500043,"组合密封圈","直径24 NBR",null,"炼钢厂","只",100]
[569,7400500032,"组合密封圈","直径39 NBR",null,"炼钢厂","只",100]
[570,7400500033,"组合密封圈","直径42 NBR",null,"炼钢厂","只",100]
[571,7400900005,"组合密封圈","直径48 NBR",null,"炼钢厂","只",100]
[572,7400500041,"组合密封圈","直径20 NBR",null,"180分厂","只",100]
[573,7400900003,"组合密封圈","直径27 NBR",null,"炼钢厂","只",100]
[574,7400500034,"组合密封圈","直径45 NBR",null,"炼钢厂","只",100]
[575,7400500040,"组合密封圈","直径18 NBR",null,"炼钢厂","只",100]
[576,7400900004,"组合密封圈","直径36 NBR",null,"炼钢厂","只",100]
[577,7400500031,"组合密封圈","直径33 NBR",null,"炼钢厂","只",100]
[578,7400500035,"组合密封圈","直径8 NBR",null,"180分厂","只",100]
[579,7400900006,"组合密封圈","直径52 NBR",null,"炼钢厂","只",100]
[580,7400100374,"炼钢220结晶器;O型密封圈","直径74*8.0(内径长)",null,"炼钢厂","只",20]
[581,7400100376,"炼钢结晶器;O型密封圈","直径9.6*170(内径长)",null,"炼钢厂","只",20]
[582,7400100377,"炼钢结晶器;O型密封圈","直径9.6*255(内径长)",null,"炼钢厂","只",50]
[583,7400100395,"炼钢结晶器O型密封圈","直径9.6*180(内径长).硅橡胶",null,"炼钢厂","只",20]
[584,7400100396,"炼钢结晶器O型密封圈","直径9.6*213(内径长).硅橡胶",null,"炼钢厂","只",20]
[585,7400100439,"炼钢220结晶器O型密封胶","直径10.5*259(内径长)，硅橡胶",null,"炼钢厂","只",50]
[586,7400100440,"炼钢280结晶器O型密封圈","直径328*10.5(内径长)，硅橡胶",null,"炼钢厂","只",10]
[587,7400100441,"炼钢220结晶器O型密封圈","直径101*5.5(内径长)，硅橡胶",null,"炼钢厂","只",100]
[588,7400100442,"炼钢250结晶器O型密封圈","直径(内径)287*10.5，硅橡胶",null,"炼钢厂","只",100]
[589,7400100444,"炼钢220结晶器O型密封圈","直径618*12;(内径长)，硅橡胶",null,"炼钢厂","只",10]
[590,7400100445,"炼钢250结晶器O型密封圈","直径(内径)880*4.7，硅橡胶",null,"炼钢厂","只",10]
[591,7400100446,"炼钢330结晶器O型密封圈","直径5.7*540(内径长)，硅橡胶",null,"炼钢厂","只",10]
[592,7400100447,"炼钢220结晶器O型密封圈","直径2.7*21(内径长)，硅橡胶",null,"炼钢厂","只",100]
[593,7400100448,"炼钢330结晶器O型密封圈","直径384*10.5(内径长)，硅橡胶",null,"炼钢厂","只",100]
[594,7400100450,"炼钢330结晶器O型密封圈","直径3.7*880(内径长)，硅橡胶",null,"炼钢厂","只",50]
[595,7400100456,"炼钢结晶器O型密封圈","直径7.5*576(内径长);硅橡胶",null,"炼钢厂","只",10]
[596,7400100458,"炼钢结晶器O型密封圈","直径12.5*830(内径长);硅橡胶",null,"炼钢厂","只",10]
[597,7400100459,"炼钢结晶器O型密封圈","直径7.5*685(内径长);硅橡胶",null,"炼钢厂","只",10]
[598,7400100461,"炼钢结晶器O型密封圈","直径765*8.5G;硅橡胶",null,"炼钢厂","只",10]
[599,7400100464,"炼钢结晶器O型密封圈","直径7.5*902(内径长);硅橡胶",null,"炼钢厂","只",10]
[600,7400100465,"炼钢结晶器O型密封圈","直径8.0*539(内径长);硅橡胶",null,"炼钢厂","只",10]
[601,7400100468,"炼钢结晶器O型密封圈","直径12.5*940(内径长);硅橡胶",null,"炼钢厂","只",10]
[602,7400100469,"炼钢结晶器O型密封圈","直径6*1813(内径长);硅橡胶",null,"炼钢厂","只",10]
[603,7400100471,"炼钢结晶器O型密封圈","直径6*2158(内径长);硅橡胶",null,"炼钢厂","只",10]
[604,7400100473,"炼钢结晶器O型密封圈","直径8*869(内径长);硅橡胶",null,"炼钢厂","只",10]
[605,7400100475,"炼钢结晶器O型密封圈","直径7.5*794(内径长);硅橡胶",null,"炼钢厂","只",10]
[606,7400100476,"炼钢结晶器O型密封圈","直径8.0*647(内径长);硅橡胶",null,"炼钢厂","只",10]
[607,7400100479,"炼钢结晶器O型密封圈","直径6*2498(内径长);硅橡胶",null,"炼钢厂","只",10]
[608,7400100480,"炼钢结晶器O型密封圈","直径12.5*951(内径长);硅橡胶",null,"炼钢厂","只",10]
[609,7400100496,"炼钢结晶器O型密封圈","直径6*248(内径长)，硅橡胶",null,"炼钢厂","只",20]
[610,7400100498,"炼钢结晶器O型密封圈","直径6*170(内径长);硅橡胶",null,"炼钢厂","只",20]