{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":85,"n_cols":12,"rows_kept":85,"merged":[[0,0,0,11],[1,0,1,11],[81,0,81,11],[82,0,82,11],[83,0,83,11],[84,0,84,11]],"flags":["formulas_cached_only"]}
["    （一）开标一览表"]
["项目名称：2021年8月液压备件采购招标项目                                         项目编号：HGZB21383"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","交货时间","使用部门","含税单价(元)","生产厂家\n","备注   "]
[1,"7502000196","铝合金钟形罩","KD550","铝合金铸件、电机Y2-280S-4 75KW B35/油泵PVXS180-M-R-DF-0000-000 VICKERS  长度272","台","2","2021-09-30","管加工厂部"]
[2,"7500500022","过滤器滤芯","0330D005BN4HC HYDAC",null,"只","10","2021-09-30","180厂部"]
[3,"7501100473","焊接式接头","N-EAKM-25-S","N-EAKM-25-S","只","50","2021-09-30","180厂部"]
[4,"7500400005","过滤/稳流器","06P.350.1Y.00.000.0","LECHLER","只","12","2021-09-30","180厂部"]
[5,"7200700005","液压马达","BM4-400PAY","1008N.M 6-305r/min GB/T20421.3-2006","台","8","2021-09-30","180厂部"]
[6,"7500500205","过滤器滤芯","0330D010BN4HC;HYDAC","过滤精度10um；滤芯材质BN4HC；额定压力16MPA;HYDAC","只","10","2021-09-30","180厂部"]
[7,"7501100001","90度弯头","90度弯头 一端长套接直径16钢管 一端德国公制M24*1.5",null,"只","50","2021-09-30","炼钢厂部"]
[8,"7501100513","不锈钢焊接式管接头","C-AGE18-LR3/8KEG","304不锈钢","个","20","2021-09-30","炼钢厂部"]
[9,"7501100514","不锈钢焊接式管接头","C-AGAI18-LR3/8KEG","内螺纹RC3/8;304不锈钢","个","20","2021-09-30","炼钢厂部"]
[10,"7100800037","油气混合块","QRHHK-4L","铝合金LF6","件","2","2021-09-30","炼钢厂部"]
[11,"7100700006","同步马达","HDD-30.17-MB+HDD-30.17-MB+C30.30-MD+HDD-30.17-MB+HDD-30.17-MB","油路一进四出","台","1","2021-09-30","炼钢厂部"]
[12,"7100700001","齿轮式分流马达","JXA-022Q-VB100-N KINSSON-HYDRAULK",null,"台","2","2021-09-30","管加工厂部"]
[13,"7500500072","过滤器滤芯","1700R010BN4HC HYDAC",null,"只","6","2021-09-30","340热轧"]
[14,"7500500125","过滤器滤芯","0660R100W/HC;HYDAC",null,"只","12","2021-09-30","340热轧"]
[15,"7501000269","可调式直角接头","SNO-VBDKO-16S/1.4571","M24*1.5;不锈钢；耐压等级450bar.","个","20","2021-09-30","180厂部"]
[16,"7501000270","可调式直角接头","SNO-VBDKO－25S/1.4571","M36*2;不锈钢；耐压等级450bar","个","20","2021-09-30","180厂部"]
[17,"7501000271","可调式直角接头","SNO-VBDKO-30S/1.4571","M42*2;不锈钢；耐压等级450bar","个","20","2021-09-30","180厂部"]
[18,"7501000272","可调式直角接头","SNO-VBDKO-20S/1.4571","M30*2;不锈钢；耐压等级450bar","个","20","2021-09-30","180厂部"]
[19,"7501000273","SAE法兰焊接组件","DSFS6001/1.4571","不锈钢；接管外径20*3；不锈钢","只","20","2021-09-30","180厂部"]
[20,"7501100277","快速接头","2\" WGS2305施备3-4-2-6",null,"只","50","2021-09-30","炼钢厂部"]
[21,"7100700007","同步分流马达","JXT-022Q-VR160-N",null,"台","1","2021-09-30","管加工厂部"]
[22,"7000200002","螺杆泵","3GR85*2W2","组合件 安全阀设定1.5MPa，GB/T10886-2002","台","1","2021-09-30","高辅工段"]
[23,"7401700004","机械密封","CDLA-22/BU2V1FF","材质:不锈钢","套","2","2021-09-30","炼钢厂部"]
[24,"7200800042","气缸","SC200*150-FB","动作方式 双作用,缸径 200（mm）标准行程 150（mm）；气缸行程20mm，接头G1/2\"；工作压力0.15-1.5MPa","只","3","2021-09-30","管加工厂部"]
[25,"7000400001","定量叶片泵","PVV21X/055LA15DM","进口成套件","台","2","2021-09-30","720厂部"]
[26,"7100200045","双单向节流阀","Z2FS16-30/S2",null,"只","5","2021-09-30","720厂部"]
[27,"7100500115","比例换向阀","DPZO-AE-371-D5/EGI+SP-ZH-7P","25通径，电流型；E型中位基能；自带放大板","只","1","2021-09-30","720厂部"]
[28,"6400600204","压力继电器","EDS348-5-016-000+ZBE08+ZBM14","品牌 HYDAC","只","36","2021-09-30","340热轧"]
[29,"5718600024","MPM管体车床;A刀架旋转液压马达控制块","M724542","{配036539；止回阀3C-60-S};M.P. COLINET/s.p.r.l.;","件","2","2021-09-30","管加工厂部"]
[30,"7501100478","变径接头","RI 1/2-1/4","RI 1/2-1/4 （带U型圈）原厂家：AGT","只","100","2021-09-30","180厂部"]
[31,"7200700003","液压马达","268.01SB0060-35 OMt315 输出460N/M 170r/min q=60L/min Danfoss","输出460N/M 170r/min q=60L/min","台","2","2021-09-30","340热轧"]
[32,"7500500060","过滤器滤芯","5u 01E900.3VG.HR.E.P.IS06",null,"只","12","2021-09-30","炼钢厂部"]
[33,"7500500059","过滤器滤芯","5u 01E950.3VG.10.S1.P.IS06",null,"只","10","2021-09-30","炼钢厂部"]
[34,"7500500061","过滤器滤芯","5u 01NR1000.3VG.10.B.P.IS06",null,"只","6","2021-09-30","炼钢厂部"]
[35,"7500500062","过滤器滤芯","5u 01E150.3VG.HR.E.P.IS06",null,"只","6","2021-09-30","炼钢厂部"]
[36,"7502900155","四辊破碎油路块","SGPSBKS1300A，280*190*130","锻件，耐压500bar","个","2","2021-09-30","烧结"]
[37,"7500500017","过滤器滤芯","0160D010BN4HC 过滤精度10um","HYDAC","只","6","2021-09-30","炼钢厂部"]
[38,"7502800025","4#水压；铜垫","XHFZ20.100-05","紫铜","只","10","2021-09-30","340热轧"]
[39,"7500500201","以色列过滤器滤芯","CA-808XLP","精度50um;压力1.6MPa;材质;不锈钢","只","2","2021-09-30","炼钢厂部"]
[40,"7500500202","过滤器滤芯","CA-204S","精度40um;压力1.6MPa;材质;不锈钢","只","8","2021-09-30","炼钢厂部"]
[41,"7501100511","不锈钢直角接头","C-GE6-LM10*1（T）","材料304","只","100","2021-09-30","炼钢厂部"]
[42,"7200800041","气缸","0640202.19.2g","QGB-ES200*80-L3；    0.4-1MPa","只","2","2021-09-30","管加工厂部"]
[43,"7501200027","管接头","A10-RS/WD","ISO7169-1998","只","50","2021-09-30","180厂部"]
[44,"7500400047","调压阀组高压滤油器","TDF240K5R-VG，PALL","承压压力35MPa，流量240L/min，附带滤芯5μm,带压差报警器，品牌PALL","套","1","2021-09-30","高炉"]
[45,"7100500076","电液比例换向阀","KBFDG4V-5-2C50N25-Z-PE7-H7-10","ISO 4401","只","2","2021-09-30","180厂部"]
[46,"7400100524","炼钢结晶器O型密封圈","（D内)Φ93×Φ5.7，硅橡胶",null,"只","50","2021-09-30","炼钢厂部"]
[47,"7400100525","炼钢结晶器O型密封圈","（D内)Φ96×Φ7，硅橡胶",null,"只","50","2021-09-30","炼钢厂部"]
[48,"7400100526","炼钢结晶器O型密封圈","（D内)Φ25×Φ3，硅橡胶",null,"只","50","2021-09-30","炼钢厂部"]
[49,"7400100527","炼钢结晶器O型密封圈","（D内)Φ24×Φ3，硅橡胶",null,"只","50","2021-09-30","炼钢厂部"]
[50,"7400100528","炼钢结晶器O型密封圈","（D内)Φ545×Φ5.7，硅橡胶",null,"只","50","2021-09-30","炼钢厂部"]
[51,"7400100529","炼钢结晶器O型密封圈","（D内)Φ623×Φ5.7，硅橡胶",null,"只","50","2021-09-30","炼钢厂部"]
[52,"7400100530","炼钢结晶器O型密封圈","（D内)Φ880×Φ5.7，硅橡胶",null,"只","50","2021-09-30","炼钢厂部"]
[53,"7400100531","炼钢结晶器O型密封圈","（D内)Φ258×Φ10，硅橡胶",null,"只","50","2021-09-30","炼钢厂部"]
[54,"7400100532","炼钢结晶器O型密封圈","（D内)Φ293×Φ10，硅橡胶",null,"只","50","2021-09-30","炼钢厂部"]
[55,"7400100533","炼钢结晶器O型密封圈","（D内)Φ326×Φ10，硅橡胶",null,"只","50","2021-09-30","炼钢厂部"]
[56,"7500500039","过滤器滤芯","0950R20BN3HC HYDAC",null,"只","12","2021-09-30","高炉"]
[57,"7501100512","不锈钢焊接式管接头","C-ASK18-L","304不锈钢","只","40","2021-09-30","炼钢厂部"]
[58,"7500500045","过滤器滤芯","0850R100BN4HC HYDAC",null,"只","10","2021-09-30","340热轧"]
[59,"5501200108","电动多路智能分油箱总成","QRDDZNFYX－6/HZPXB","6个出油口，出油口接头φ10；箱体为不锈钢材质，附件包括：1、控制模块：QR-ZNKZ-1002R2A-D24-V2；2、电动多路选择阀：QRDDLF-6ZNB；3、电动执行器：QRDDZXQ-70/B；4、位移传感器：QRWYCGQ-70；5、电动连续计量型流量计：QRDDKDLLJ－1.2ml；6、电动执行器：QRDDZXQ-10/A；7、流量传感器：QRX9500.3TG；8、磁性开关：QJLG-1G.01(NPN)；9、电动换向阀：24EJF-HY-TG/DC24QR","套","4","2021-09-30","高辅工段"]
[60,"7201300090","气缸","CDS1BN125-75J-M9BL3","缸径125 行程75 SMC","套","1","2021-09-30","89热轧"]
[61,"7500500211","高压过滤器滤芯","K3","Part NO.:K3（ The Pare Parts refer to Techmanual  McCoy Global PU7560-01 Electric Hydraulic Power Unit  )；High Pressure Filter Cartridge;","件","2","2021-09-30","检验检测中心"]
[62,"7500500208","回油过滤器滤芯","PU2500-H15","Part NO.:PU2500-H15（The Pare Parts refer to Techmanual  McCoy Global PU7560-01 Electric Hydraulic Power Unit   )；Return Filter Cartridge;","件","2","2021-09-30","检验检测中心"]
[63,"7501100515","快速插拔接头","与1/4英寸硫化氢气管相接的快速插拔接头","配套试验池顶部螺纹接口；PP材质，不锈钢316按钮，不锈钢301内置弹簧；分体（公母）式，各自带有流体截止功能，无泄漏；最高使用温度：≤60℃；外置不锈钢316管固定螺母；","套","160","2021-09-30","检验检测中心"]
[64,"7500400050","回油过滤器","ZU-A","63*20","个","1","2021-09-30","物流中心"]
[65,"7500400051","空气滤清器","QUQ2","旋装方式：管螺纹","个","1","2021-09-30","物流中心"]
[66,"7500500212","吸油滤芯","XU-B-80","M48*2","个","1","2021-09-30","物流中心"]
[67,"7500500053","过滤器滤芯","1300R005BN4HC HYDAC",null,"只","4","2021-09-30","89热轧"]
[68,"7501000181","管接头","NA50-S/M60*2",null,"只","10","2021-09-30","219厂部"]
[69,"7501000216","中间接头","38/M52*2",null,"只","20","2021-09-30","219厂部"]
[70,"7501000217","中间接头","51/M64*2",null,"只","20","2021-09-30","219厂部"]
[71,"7501100346","管接头","GAV50*10",null,"只","10","2021-09-30","219厂部"]
[72,"7501200067","管接头","NA50-L/R2\"","M68*2/2\"","只","20","2021-09-30","219厂部"]
[73,7100500041,"比例换向阀","ISO4401","KDG5V-5-33C80N-EX-M-U-H-1-10","只",1,"2021-09-30","720厂部"]
[74,7100500098,"先导阀","德国DIN24 340 A型","3DREP6C-2X/25EG24N9K4/M","台",3,"2021-12-25","管加工厂部"]
[75,7100500046,"比例减压阀","DIN24340-2-1982","DREBE6X-10/175MG24K31F1M","只",1,"2021-09-30","180厂部"]
[76,7100500038,"比例换向阀",null,"KBFDG4V-5-2C70N-Z-M1-PE7-H7-10","只",2,"2022-01-09","219厂部"]
[77,7100500011,"比例阀","JB/T10373-2002","D111FH-B31-L-2-N-E-0043-X807","只",2,"2022-01-09","炼钢厂部"]
[78,7100500012,"比例阀","JB/T10373－2002","D81FH-B31-H-2-N-E-0044-X807","只",2,"2022-01-09","炼钢厂部"]
["注：1、投标报价含税，税率13% ；2、生产厂家要求全称填写准确无误 ；                                                                                          3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）；"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2021年8月液压备件采购招标项目                             项目编号：HGZB21383"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}