{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["Macro1","附件清单表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"附件清单表","index":1,"n_rows":157,"n_cols":9,"rows_kept":157,"flags":["formulas_cached_only"]}
["序号","资材编码","资材名称","规格","技术参数","请购部门","单位","数量（以每月实际数量为准）","交货期"]
[1,7300100549,"金属软管","HM1.6JR15-10000Ad20G1/2\"","GB/T14525-1993,DN15，16BAR,长度10000，1/2\"","180分厂","根",40,"合同签订后1个月内"]
[2,7300300144,"金属软管","HM1.6JR25-1200Ad20G1\"","GB/T14525-1993，DN25，16BAR,长度1200，G1\"","180分厂","根",40,"合同签订后1个月内"]
[3,7300300197,"金属软管","HM1.6JR15-2000Ad15G1/2\" GB/T14525-1993，DN15，16BAR,长度2000，G1/2\"",null,"180分厂","根",40,"合同签订后1个月内"]
[4,7300300120,"金属软管","DN25 JT2.5GR25-700AR1\"+A1\"",null,"219分厂","根",34,"合同签订后1个月内"]
[5,7300300121,"金属软管","DN40 JT2.5GR40-250AR1 1/2\"+A1 1/2\"",null,"219分厂","根",32,"合同签订后1个月内"]
[6,7300300138,"金属软管","G1/4\" L=1200mm",null,"219分厂","根",10,"合同签订后1个月内"]
[7,7300100599,"金属软管","HM1.6JR20-1200Ad20G3/4\"","DN25，16BAR,长度1200，G3/4\"","340分厂","根",60,"合同签订后1个月内"]
[8,7300100600,"金属软管","HM1.6JR20-2000Ad20G3/4\"","DN25，16BAR,长度2000，G3/4\"","340分厂","根",80,"合同签订后1个月内"]
[9,7300100548,"金属软管","1.6JR20-2500Ad20G3/4\"",",DN20，16BAR,长度2500，C3/4\"","89分厂","根",20,"合同签订后1个月内"]
[10,7300100690,"金属软管","HM1.6JR20-600Ad20G3/4\"","20通径，长度600mm,耐压1.6MPa,内螺纹ZG3/4\"","89分厂","根",20,"合同签订后1个月内"]
[11,7300300212,"金属软管（DN25）","1.6JR25-500L，G1\"","DN25，16BAR,长度500，G1\"","89分厂","根",10,"合同签订后1个月内"]
[12,7300300213,"金属软管（DN20）","1.6JR20-500L，G3/4\"","DN20，16BAR,长度500，G3/4\"","89分厂","根",10,"合同签订后1个月内"]
[13,7300300196,"金属软管","HM1.6JR15-1200Ad20G1/2\"",null,"管加工分厂","根",10,"合同签订后1个月内"]
[14,7300300204,"金属软管","1.6ZR20-600A","G3/4\"","管加工分厂","根",60,"合同签订后1个月内"]
[15,7300300214,"1号线烧嘴用金属软管","双头活接DN20;","L=400mm;   316不锈钢","管加工分厂","根",10,"合同签订后1个月内"]
[16,7300300215,"1号线烧嘴用金属软管","双头活接DN40;","L=600mm;   316不锈钢","管加工分厂","根",10,"合同签订后1个月内"]
[17,7300300216,"1号线烧嘴用金属软管","双头活接DN40;","L=400mm;    316不锈钢","管加工分厂","根",10,"合同签订后1个月内"]
[18,7300300217,"1号线烧嘴用金属软管","双头活接DN20;","L=800mm;316不锈钢","管加工分厂","根",10,"合同签订后1个月内"]
[19,7300300220,"不锈钢编织网金属软管","G3/4-5200；接头内螺纹丝G3/4；封口型式为喇叭口；","长度5.2m；最大工作压力PN4.5；材质：不锈钢编织网金属软管","管加工分厂","根",4,"合同签订后1个月内"]
[20,7300100713,"煤气用金属软管（淬）","∮48.3*3.5*500mm;","活接+外丝 11/2\";   压力1.0MPa","管加工分厂","根",4,"合同签订后1个月内"]
[21,7300300012,"金属软管","0.6JR100-2500F/FS","100通径 最大工作压力6bar 一端焊接接头,一端松套法兰 长度2500mm","炼钢厂","根",4,"合同签订后1个月内"]
[22,7300300015,"金属软管","1.6JR100-2000F/FS","100通径 最大工作压力16bar 一端焊接接头,一端松套法兰 长度2000mm","炼钢厂","根",4,"合同签订后1个月内"]
[23,7300300016,"金属软管","1.6JR10-1300DRC3/4\"","10通径 最大工作压力16bar 内螺纹球面接头 长度1300mm 螺纹G3/4\"","炼钢厂","根",60,"合同签订后1个月内"]
[24,7300300017,"金属软管","1.6JR10-1300DRC3/4\"(左)","10通径 最大工作压力16bar 内螺纹球面接头 长度1300mm 螺纹G3/4\"(左)","炼钢厂","根",30,"合同签订后1个月内"]
[25,7300300019,"金属软管","1.6JR10-3500DRC3/4\"","10通径 最大工作压力16bar 内螺纹球面接头 长度3500mm 螺纹G3/4\"","炼钢厂","根",60,"合同签订后1个月内"]
[26,7300300020,"金属软管","1.6JR10-3500DRC3/4\"(左)","10通径 最大工作压力16bar 内螺纹球面接头 长度3500mm 螺纹G3/4\"(左)","炼钢厂","根",20,"合同签订后1个月内"]
[27,7300300021,"金属软管","1.6JR10-5000IG3/4\"","10通径 最大工作压力16bar 内螺纹球面接头 长度5000mm 螺纹G3/4\"","炼钢厂","根",20,"合同签订后1个月内"]
[28,7300300022,"金属软管","1.6JR10-630DRC3/4\"","10通径 最大工作压力16bar 内螺纹球面接头 长度630mm 螺纹G3/4\"","炼钢厂","根",40,"合同签订后1个月内"]
[29,7300300023,"金属软管","1.6JR10-800DRC3/4\"","10通径 最大工作压力16bar 内螺纹球面接头 长度800mm 螺纹G3/4\"","炼钢厂","根",40,"合同签订后1个月内"]
[30,7300300024,"金属软管","1.6JR150-1000F/F1-D240-直径22*8","150通径 最大工作压力16bar 一端焊接接头,一端松套法兰 长度1000mm","炼钢厂","根",20,"合同签订后1个月内"]
[31,7300300025,"金属软管","1.6JR150-2000 法兰中心距240 孔8*直径18","150通径 最大工作压力16bar 一端焊接接头,一端松套法兰 长度2000mm","炼钢厂","根",8,"合同签订后1个月内"]
[32,7300300026,"金属软管","1.6JR150-4000F240-8*23 两端带法兰","150通径 最大工作压力16bar 一端焊接接头,一端松套法兰 长度4000mm 两端带法兰","炼钢厂","根",4,"合同签订后1个月内"]
[33,7300300027,"金属软管","1.6JR15-1600L2-3/4\"-3/4\"","15通径 最大工作压力16bar 快速接头D3/4寸 长度1600mm 一直一弯","炼钢厂","根",200,"合同签订后1个月内"]
[34,7300300028,"金属软管","1.6JR15-3000L3/4\"/L2-3/4\"","15通径 最大工作压力16bar 快速接头D3/4寸 长度3000mm 一直一弯","炼钢厂","根",60,"合同签订后1个月内"]
[35,7300300029,"金属软管","1.6JR15-600DG3/4\"","15通径 最大工作压力16bar 内螺纹球面接头 长度600mm 螺纹G3/4\"","炼钢厂","根",200,"合同签订后1个月内"]
[36,7300300032,"金属软管","1.6JR15Y-3000 M30*1.5","15通径 最大工作压力16bar 内螺纹74°内锥面接头 长度3000mm 螺纹M30*1.5","炼钢厂","根",40,"合同签订后1个月内"]
[37,7300300034,"金属软管","1.6JR200-1000F/F1-D295-直径22*12200通径 最大工作压力16bar 一端固定法兰,一端松套法兰 长度1000mm","200通径 最大工作压力16bar 一端焊接接头,一端松套法兰 长度1000mm","炼钢厂","根",10,"合同签订后1个月内"]
[38,7300300037,"金属软管","1.6JR200-2000FD95*12*直径22","200通径 最大工作压力16bar 一端焊接接头,一端松套法兰 长度2000mm","炼钢厂","根",4,"合同签订后1个月内"]
[39,7300300038,"金属软管","1.6JR200-2100FD295*12*直径22+FED300*8*直径22200通径 最大工作压力16bar ；一端固定法兰，孔距295*12孔*直径22mm；,一端松套法兰，孔距300*8孔*直径22mm； 长度2100mm；","200通径 最大工作压力16bar 一端焊接接头,一端松套法兰 长度2100mm","炼钢厂","根",10,"合同签订后1个月内"]
[40,7300300039,"金属软管","1.6JR200-3000FD295*12*直径22+FED300*8*直径22200通径 最大工作压力16bar, 一端固定法兰，孔距295*12孔*直径22mm；,一端松套法兰，孔距300*8孔*直径22mm；长度3000mm","200通径 最大工作压力16bar 一端焊接接头,一端松套法兰 长度3000mm","炼钢厂","根",4,"合同签订后1个月内"]
[41,7300300040,"金属软管","1.6JR200-7000F/F1-D295200通径 最大工作压力16bar 一端固定法兰,一端松套法兰 长度7000mm；排泥胶管","200通径 最大工作压力16bar 一端焊接接头,一端松套法兰 长度7000mm","炼钢厂","根",2,"合同签订后1个月内"]
[42,7300300041,"金属软管","1.6JR20-10000IG3/4\"","20通径 最大工作压力16bar 英锥管外螺纹接头 长度10000mm 螺纹G3/4\"","炼钢厂","根",20,"合同签订后1个月内"]
[43,7300300042,"金属软管","1.6JR20-1000IG3/4\"","20通径 最大工作压力16bar 英锥管外螺纹接头 长度1000mm 螺纹G3/4\"","炼钢厂","根",60,"合同签订后1个月内"]
[44,7300300043,"金属软管","1.6JR20-1500I G1\"","20通径 最大工作压力16bar 英锥管外螺纹接头 长度1500mm 螺纹G1\"","炼钢厂","根",60,"合同签订后1个月内"]
[45,7300300044,"金属软管","1.6JR20-3000IRC3/4\"","20通径 最大工作压力16bar 英锥管内螺纹接头 长度3000mm 螺纹G3/4\"","炼钢厂","根",40,"合同签订后1个月内"]
[46,7300300045,"金属软管","1.6JR20-3500R3/4","20通径 最大工作压力16bar 英锥管外螺纹接头 长度3500mm 螺纹G3/4\"","炼钢厂","根",40,"合同签订后1个月内"]
[47,7300300046,"金属软管","1.6JR40-1200L/LF","40通径 最大工作压力16bar 快速接头D1-1/2寸 长度1200mm","炼钢厂","根",80,"合同签订后1个月内"]
[48,7300300047,"金属软管","1.6JR40-2000L","40通径 最大工作压力16bar 快速接头D1-1/2寸 长度2000mm","炼钢厂","根",80,"合同签订后1个月内"]
[49,7300300051,"金属软管","1.6JR50-1300L","50通径 最大工作压力16bar 快速接头D2寸 长度1300mm","炼钢厂","根",120,"合同签订后1个月内"]
[50,7300300053,"金属软管","1.6JR50-1800L","50通径 最大工作压力16bar 快速接头D2寸 长度1800mm","炼钢厂","根",120,"合同签订后1个月内"]
[51,7300300054,"金属软管","1.6JR50-2000L(90度+90度)M68*2","50通径 最大工作压力16bar 内螺纹球面接头 长度2000mm 外包石棉","炼钢厂","根",40,"合同签订后1个月内"]
[52,7300300055,"金属软管","1.6JR50-2600AM68*2/A(AM68*2)F","50通径 最大工作压力16bar A型接头 长度2600mm 螺纹M68*2","炼钢厂","根",12,"合同签订后1个月内"]
[53,7300300056,"金属软管","1.6JR50-800L","50通径 最大工作压力16bar 快速接头D2寸 长度800mm","炼钢厂","根",80,"合同签订后1个月内"]
[54,7300300057,"金属软管","1.6JR50-900L/L2","50通径 最大工作压力16bar 快速接头D2寸 长度900mm 一直一弯","炼钢厂","根",120,"合同签订后1个月内"]
[55,7300300058,"金属软管","1.6JR60-1200DG2-1/2\"","65通径 最大工作压力16bar 快速接头D2-1/2寸 长度1200mm","炼钢厂","根",40,"合同签订后1个月内"]
[56,7300300059,"金属软管","1.6JR65-1800L","65通径 最大工作压力16bar 快速接头D2-1/2寸 长度1800mm","炼钢厂","根",40,"合同签订后1个月内"]
[57,7300300061,"金属软管","1.6JR80-14000FS/FSC80通径 最大工作压力16bar 一端固定法兰,一端松套法兰 长度14000mm","80通径 最大工作压力16bar 一端焊接接头,一端松套法兰 长度14000mm","炼钢厂","根",4,"合同签订后1个月内"]
[58,7300300062,"金属软管","1.6JR80-9000 带焊接丝头","80通径 最大工作压力16bar 一端焊接接头,一端松套法兰 长度9000mm","炼钢厂","根",10,"合同签订后1个月内"]
[59,7300300063,"金属软管","1.6JR8-1000DRC1/2\"","8通径 最大工作压力16bar 内螺纹球面接头 长度1000mm 螺纹G1/2\"","炼钢厂","根",50,"合同签订后1个月内"]
[60,7300300064,"金属软管","1.6JR8-1300DRC1/2\"","8通径 最大工作压力16bar 内螺纹球面接头 长度1300mm 螺纹G1/2\"","炼钢厂","根",60,"合同签订后1个月内"]
[61,7300300065,"金属软管","1.6JR8-1300DRC1/2\"(左)","8通径 最大工作压力16bar 内螺纹球面接头 长度1300mm 螺纹G1/2\"(左)","炼钢厂","根",40,"合同签订后1个月内"]
[62,7300300066,"金属软管","1.6JR8-1300DRC3/8\"","8通径 最大工作压力16bar 内螺纹球面接头 长度1300mm 螺纹G3/8\"","炼钢厂","根",100,"合同签订后1个月内"]
[63,7300300067,"金属软管","1.6JR8-1500DRC3/8\"","8通径 最大工作压力16bar 内螺纹球面接头 长度1500mm 螺纹G3/8\"","炼钢厂","根",60,"合同签订后1个月内"]
[64,7300300068,"金属软管","1.6JR8-1500DRC3/8\"(左)/DRC1/2\"(左)","8通径 最大工作压力16bar 内螺纹球面接头 长度1500mm 螺纹G3/8\"(左)/1/2\"(左)","炼钢厂","根",20,"合同签订后1个月内"]
[65,7300300069,"金属软管","1.6JR8-1700RC3/8","8通径 最大工作压力16bar 内螺纹球面接头 长度1700mm 螺纹G3/8\"","炼钢厂","根",100,"合同签订后1个月内"]
[66,7300300070,"金属软管","1.6JR8-3500DRC1/2\"","8通径 最大工作压力16bar 内螺纹球面接头 长度3500mm 螺纹G1/2\"","炼钢厂","根",20,"合同签订后1个月内"]
[67,7300300071,"金属软管","1.6JR8-3500DRC1/2\"(左)","8通径 最大工作压力16bar 内螺纹球面接头 长度3500mm 螺纹G1/2\"(左)","炼钢厂","根",20,"合同签订后1个月内"]
[68,7300300072,"金属软管","1.6JR8-630DRC1/2\"","8通径 最大工作压力16bar 内螺纹球面接头 长度630mm 螺纹G1/2\"","炼钢厂","根",60,"合同签订后1个月内"]
[69,7300300073,"金属软管","1.6JR8-630DRC3/8\"","8通径 最大工作压力16bar 内螺纹球面接头 长度630mm 螺纹G3/8\"","炼钢厂","根",60,"合同签订后1个月内"]
[70,7300300075,"金属软管","1.6JR8-800DRC1/2\"","8通径 最大工作压力16bar 内螺纹球面接头 长度800mm 螺纹G1/2\"","炼钢厂","根",20,"合同签订后1个月内"]
[71,7300300077,"金属软管","1.6JR8-800DRC3/8\"","8通径 最大工作压力16bar 内螺纹球面接头 长度800mm 螺纹G3/8\"","炼钢厂","根",100,"合同签订后1个月内"]
[72,7300300079,"金属软管","1.6JRD125F-L3200 法兰螺距中心:直径210","125通径 最大工作压力16bar 一端焊接接头,一端松套法兰 长度3250mm","炼钢厂","根",12,"合同签订后1个月内"]
[73,7300300082,"金属软管","1.6ZR20-2000A G3/4\"","20通径 最大工作压力16bar A型接头 长度2000mm 螺纹G3/4\"","炼钢厂","根",10,"合同签订后1个月内"]
[74,7300300085,"金属软管","140K1BF9-10000","32通径 最大工作压力16bar 内螺纹24°锥接头 长度10000mm 螺纹M52*2","炼钢厂","根",6,"合同签订后1个月内"]
[75,7300300086,"金属软管","16-16-2000P1+N-R1/2=P1+N-∮21*3G","15通径 最大工作压力16bar 内螺纹24°锥接头 长度2000mm 螺纹M30*2","炼钢厂","根",20,"合同签订后1个月内"]
[76,7300300089,"金属软管","1JR15-1000IR1/2J M27*1.5","15通径 最大工作压力16bar 内螺纹74°内锥面接头 长度1000mm 螺纹M27*1.5","炼钢厂","根",40,"合同签订后1个月内"]
[77,7300300092,"金属软管","1JR15-600IR1/2J M27*1.5","15通径 最大工作压力16bar 内螺纹74°内锥面接头 长度600mm 螺纹M27*1.5","炼钢厂","根",60,"合同签订后1个月内"]
[78,7300300093,"金属软管","1JR80A-2500 法兰 1MPa80通径 最大工作压力16bar 一端固定法兰,一端松套法兰 长度2500mm","80通径 最大工作压力16bar 一端焊接接头,一端松套法兰 长度2500mm","炼钢厂","根",20,"合同签订后1个月内"]
[79,7300300094,"金属软管","2.5JR50-7000F50通径 最大工作压力16bar 一端焊接法兰,一端松套法兰 长度7000mm","50通径 最大工作压力16bar 一端焊接接头,一端松套法兰 长度7000mm","炼钢厂","根",6,"合同签订后1个月内"]
[80,7300300097,"金属软管","20-16-1200P1+N-∮27*3=A5","20通径 最大工作压力16bar 内螺纹24°锥接头 长度1200mm 螺纹M36*2","炼钢厂","根",40,"合同签订后1个月内"]
[81,7300300099,"金属软管","40-16-1000A8=A8G","40通径 最大工作压力16bar 快速接头D1-1/2寸 长度1000mm","炼钢厂","根",40,"合同签订后1个月内"]
[82,7300300100,"金属软管","40-16-1200P1+N-∮48*3.5=D240通径 最大工作压力16bar  长度1200mm螺纹M60*2的活螺母喇叭口","40通径 最大工作压力16bar 快速接头D1-1/2寸 长度1200mm","炼钢厂","根",30,"合同签订后1个月内"]
[83,7300300104,"金属软管","BTR10BL1-2000-16C","10通径 最大工作压力16bar 内螺纹平面接头 长度2000mm 螺纹M18*1.5","炼钢厂","根",60,"合同签订后1个月内"]
[84,7300300105,"金属软管","BTR10BL5-800-16C","10通径 最大工作压力16bar 内螺纹球面接头 长度800mm 螺纹M18*1.5","炼钢厂","根",100,"合同签订后1个月内"]
[85,7300300107,"金属软管","BTR15BL8-3000-16C","15通径 最大工作压力16bar 内螺纹球面接头 长度3000mm 螺纹M16*1.5","炼钢厂","根",20,"合同签订后1个月内"]
[86,7300300108,"金属软管","BTR15BL8-800-16C","15通径 最大工作压力16bar 内螺纹球面接头 长度800mm 螺纹M16*1.5","炼钢厂","根",60,"合同签订后1个月内"]
[87,7300300109,"金属软管","BTR20BL1-1300-16F M30*1.5","20通径 最大工作压力16bar 内螺纹平面接头 长度1300mm 螺纹M30*1.5","炼钢厂","根",40,"合同签订后1个月内"]
[88,7300300110,"金属软管","BTR20BL1-800-16F M30*1.5","20通径 最大工作压力16bar 内螺纹平面接头 长度800mm 螺纹M30*1.5","炼钢厂","根",40,"合同签订后1个月内"]
[89,7300300111,"金属软管","BTR20BL5-2000-16C","20通径 最大工作压力16bar 内螺纹平面接头 长度2000mm 螺纹M30*1.5","炼钢厂","根",40,"合同签订后1个月内"]
[90,7300300112,"金属软管","BTR20BL5-3000-16C","20通径 最大工作压力16bar 内螺纹平面接头 长度3000mm 螺纹M30*1.5","炼钢厂","根",20,"合同签订后1个月内"]
[91,7300300113,"金属软管","BTR20BL6BL8-1500-16F","20通径 最大工作压力16bar 一端内螺纹球面接头，一端锥管外丝接头 长度1500mm 螺纹M30*1.5 一端ZG3/4\"","炼钢厂","根",40,"合同签订后1个月内"]
[92,7300300119,"金属软管","D2.5JR8016-2000D11 带全套法兰","125通径 最大工作压力16bar 一端焊接接头,一端松套法兰 长度2000mm","炼钢厂","根",4,"合同签订后1个月内"]
[93,7300300122,"金属软管","DT1.6JR0516-1000D7.4","8通径 最大工作压力16bar 内螺纹球面接头 长度1000mm 螺纹M16*1.5","炼钢厂","根",40,"合同签订后1个月内"]
[94,7300300123,"金属软管","DT1.6JR0516-1300D7.4-3/8”","8通径 最大工作压力16bar 内螺纹球面接头 长度1300mm 螺纹M16*1.5/螺纹3/8”","炼钢厂","根",60,"合同签订后1个月内"]
[95,7300300124,"金属软管","DT1.6JR0516-800D7.4-3/8","8通径 最大工作压力16bar 内螺纹球面接头 长度800mm 螺纹M16*1.5/螺纹3/8”","炼钢厂","根",20,"合同签订后1个月内"]
[96,7300300125,"金属软管","DT1.6JR0816-1300D7.4-1/2”(左)","13通径 最大工作压力16bar 内螺纹球面接头 长度1300mm 螺纹M22*1.5/螺纹1/2”(左)","炼钢厂","根",40,"合同签订后1个月内"]
[97,7300300129,"金属软管","DT1.6JR1616-1200D10.1","25通径 最大工作压力16bar 快速接头D1\" 长度1200mm","炼钢厂","根",120,"合同签订后1个月内"]
[98,7300300131,"金属软管","DT1.6JR1616-2000D10.125通径 最大工作压力16bar；内螺纹球面接头M36*1.5；长度2000mm","25通径 最大工作压力16bar 快速接头D1\" 长度2000mm","炼钢厂","根",60,"合同签订后1个月内"]
[99,7300300132,"金属软管","DT1.6JR1616-800D10.1","25通径 最大工作压力16bar 快速接头D1\" 长度800mm","炼钢厂","根",40,"合同签订后1个月内"]
[100,7300300136,"金属软管","DT1.6JR4016-80000D10.1/D11","65通径 最大工作压力16bar 快速接头D2-1/2\" 一端法兰 长度80000mm","炼钢厂","根",8,"合同签订后1个月内"]
[101,7300300137,"金属软管","DT1.6JR8016-1400D11","125通径 最大工作压力16bar 一端焊接接头,一端松套法兰 长度1400mm","炼钢厂","根",12,"合同签订后1个月内"]
[102,7300300139,"金属软管","G1016-310C6.1C6.3-T","15通径 最大工作压力16bar 内螺纹平面接头 长度3100mm 螺纹M27*1.5 两头弯","炼钢厂","根",160,"合同签订后1个月内"]
[103,7300300140,"金属软管","G11016-1500-D6.3V180 M27*1.5","15通径 最大工作压力16bar 内螺纹平面接头 长度1500mm 螺纹M27*1.5 两头弯","炼钢厂","根",60,"合同签订后1个月内"]
[104,7300300141,"金属软管","G12416-600-D7.1-T0","40通径 最大工作压力16bar 快速接头D1-1/2寸 长度600mm","炼钢厂","根",40,"合同签订后1个月内"]
[105,7300300143,"金属软管","G12416-800-D7.1-T0","40通径 最大工作压力16bar 快速接头D1-1/2寸 长度800mm","炼钢厂","根",80,"合同签订后1个月内"]
[106,7300300147,"金属软管","HT2000T.2-T01-LG","40通径 最大工作压力16bar 快速接头D1-1/2寸 长度2000mm","炼钢厂","根",20,"合同签订后1个月内"]
[107,7300300150,"金属软管","HT-P16PT10C-LG4600+F","40通径 最大工作压力16bar 快速接头D1-1/2寸 长度4600mm","炼钢厂","根",4,"合同签订后1个月内"]
[108,7300300154,"金属软管","JRD150SL-3800 螺距中心孔:直径270长度3200mm，法兰中心距270 孔8*直径23","150通径 最大工作压力16bar 一端焊接接头,一端松套法兰 长度3800mm","炼钢厂","根",20,"合同签订后1个月内"]
[109,7300300158,"金属软管","JRD20SL1-500 M24*1.5","20通径 最大工作压力16bar M24*1.5 长度500mm","炼钢厂","根",60,"合同签订后1个月内"]
[110,7300300162,"金属软管","JRD25SL-1000 M39*2长度1000mm 螺纹M39*2                               的活螺母喇叭口              ","25通径 最大工作压力16bar M39*2 长度1000mm","炼钢厂","根",20,"合同签订后1个月内"]
[111,7300300163,"金属软管","JRD25SL1-1500 M39*2长度1500mm 螺纹M39*2                               的活螺母喇叭口              ","25通径 最大工作压力16bar M39*2 长度1500mm","炼钢厂","根",40,"合同签订后1个月内"]
[112,7300300164,"金属软管","JRD25SL1-2000 M39*2环氧管：长度2000mm 螺纹M39*2                               的活螺母喇叭口              天然气管：内螺纹74°内锥面接头 长度2000mm 螺纹M36*1.5","25通径 最大工作压力16bar 内螺纹74°内锥面接头 长度2000mm 螺纹M39*2","炼钢厂","根",40,"合同签订后1个月内"]
[113,7300300165,"金属软管","JRD25SL1-650 M39*2长度650mm 螺纹M39*2                               的活螺母喇叭口              ","25通径 最大工作压力16bar 内螺纹74°内锥面接头 长度650mm 螺纹M39*2","炼钢厂","根",40,"合同签订后1个月内"]
[114,7300300166,"金属软管","JRD40SL1-1500 M60*240通径，螺纹M60*2的活螺母喇叭口，长度1500mm","40通径 最大工作压力16bar 内螺纹74°内锥面接头 长度1500mm 螺纹M60*2","炼钢厂","根",40,"合同签订后1个月内"]
[115,7300300167,"金属软管","JRD40SL1-2000 M60*240通径，螺纹M60*2的活螺母喇叭口，长度2000mm","40通径 最大工作压力16bar 内螺纹74°内锥面接头 长度2000mm 螺纹M60*2","炼钢厂","根",40,"合同签订后1个月内"]
[116,7300300171,"金属软管","KJ20-800/90度+90度","20通径 最大工作压力16bar 快速接头D3/4\" 长度900mm 两头弯","炼钢厂","根",40,"合同签订后1个月内"]
[117,7300300175,"金属软管","P10J2-1.2-8C11J-LT6.6","65通径 最大工作压力16bar 一端焊接接头,一端松套法兰 长度6600mm","炼钢厂","根",12,"合同签订后1个月内"]
[118,7300300176,"金属软管","P10J2-1.2-8C12J-LT4.2","65通径 最大工作压力16bar 一端焊接接头,一端松套法兰 长度4200mm","炼钢厂","根",8,"合同签订后1个月内"]
[119,7300300178,"金属软管","WGS2305施钢 43350 带法兰 L=3300mm带钢丝网","50通径 最大工作压力16bar 两端法兰 长度3300mm 碳粉管","炼钢厂","根",30,"合同签订后1个月内"]
[120,7300300179,"金属软管","WGS2305施钢9-7 带法兰 L=1000mm带钢丝网","50通径 最大工作压力16bar 两端法兰 长度1000mm 碳粉管","炼钢厂","根",20,"合同签订后1个月内"]
[121,7300300180,"金属软管","WGS2305施钢9-7 带法兰 L=7000mm带钢丝网","50通径 最大工作压力16bar 两端法兰 长度7000mm 碳粉管","炼钢厂","根",12,"合同签订后1个月内"]
[122,7300300181,"铠装金属软管","DT1.6JR1016-900D10.1/D10.3","15通径 最大工作压力16bar 快速接头D3/4\" 长度900mm 一直一弯","炼钢厂","根",20,"合同签订后1个月内"]
[123,7300300189,"金属软管","1.6JR40*1300-V40通径 最大工作压力16bar  快速接头D1-1/2寸 长度1500mm ",null,"炼钢厂","根",40,"合同签订后1个月内"]
[124,7300300195,"金属软管","DT1.6JR1016-1000D7.4",null,"炼钢厂","根",60,"合同签订后1个月内"]
[125,7300300211,"耐高温金属软管","6JRL50A-700","介质:天燃气;使用温度:100度;长度700mm;口径DN50;法兰连接","炼钢厂","根",4,"合同签订后1个月内"]
[126,7300300188,"金属软管","1.6JR32-1600","两头带快速接头连接","炼钢厂","根",20,"合同签订后1个月内"]
[127,7300300208,"金属软管","DN65","两头带方法兰,总长度930;短管弯头200mm带DN15排气阀孔","炼钢厂","根",10,"合同签订后1个月内"]
[128,7300300117,"金属软管","BTR50BL1-10000","50通径 最大工作压力16bar 锥管内丝接头 长度10000mm 螺纹ZG2\"","炼钢厂","根",4,"合同签订后1个月内"]
[129,7300300018,"金属软管","1.6JR10-1500DRC3/4\"(左)","10通径 最大工作压力16bar 内螺纹球面接头 长度1500mm 螺纹G3/4\"(左)","炼钢厂","根",4,"合同签订后1个月内"]
[130,7300300002,"夹布输水管总成","25*1500DG1\"1.0MPa","25通径 最大工作压力10bar 内螺纹球面接头 长度1500mm 螺纹G1\"","炼钢厂","根",20,"合同签订后1个月内"]
[131,7300300003,"夹布输水管总成","25*2200DG1\" 1.0MPa","25通径 最大工作压力10bar 内螺纹球面接头 长度2200mm 螺纹G1\"","炼钢厂","根",20,"合同签订后1个月内"]
[132,7300300004,"夹布输水管总成","51*13000DG2\" 1.0MPa","51通径 最大工作压力10bar 内螺纹球面接头 长度13000mm 螺纹G2\"","炼钢厂","根",20,"合同签订后1个月内"]
[133,7300300005,"夹布输水管总成","51*2500DG2\" 1.0MPa51通径 最大工作压力10bar ；快接接头2寸；长度2500mm ","51通径 最大工作压力10bar 内螺纹球面接头 长度2500mm 螺纹G2\"","炼钢厂","根",12,"合同签订后1个月内"]
[134,7300300006,"夹布输水管总成","JB51WW50000D16.1/D16.251通径 最大工作压力10bar 快速接头D1-1/2寸 长度8000mm","51通径 最大工作压力10bar 快速接头D2寸 长度5000mm","炼钢厂","根",16,"合同签订后1个月内"]
[135,7300300007,"夹布输水管总成","JB51WW80000D16.2/C6.1-2长度8000mm；","51通径 最大工作压力10bar 快速接头D2寸 长度5000mm","炼钢厂","根",20,"合同签订后1个月内"]
[136,7300300010,"夹布输水管总成","25*5500A 1MPa","带机压头25通径 最大工作压力10bar A型接头 长度5500mm 螺纹M36*1.5","炼钢厂","根",20,"合同签订后1个月内"]
[137,7300300011,"夹布输水管总成","50*8500A 1MPa50通径 最大工作压力10bar 快速接头2寸；一头公接头，一头母接头； 长度8000mm","带机压头50通径 最大工作压力10bar A型接头 长度8500mm 螺纹M68*2","炼钢厂","根",20,"合同签订后1个月内"]
[138,7300300060,"金属软管","1.6JR65-4800L/LF","不锈钢+橡胶 GB/T14525-1993","炼铁厂","根",80,"合同签订后1个月内"]
[139,7300300103,"金属软管","JRD40SL1-650 M60*2","不锈钢+橡胶 JC886-2001，DN50，1层钢丝，1.0MPa，总长度675mm,24°锥，M60×2","炼铁厂","根",8,"合同签订后1个月内"]
[140,7300300142,"金属软管","1.6JR65-1200F/FSF","65通径 最大工作压力16bar 一端焊接接头,一端松套法兰 长度1200mm","炼铁厂","根",20,"合同签订后1个月内"]
[141,7300300145,"金属软管","S221-050，G1/4接口","不锈钢+橡胶 JC886-2001","炼铁厂","根",10,"合同签订后1个月内"]
[142,7300300188,"金属软管","1.6JR32-1600","两头带快速接头连接","炼铁厂","根",40,"合同签订后1个月内"]
[143,7300300199,"金属软管","1.6JR32-2800F/FSF",null,"炼铁厂","根",6,"合同签订后1个月内"]
[144,7300300200,"金属软管","1.6JR40-4600F/FSF",null,"炼铁厂","根",6,"合同签订后1个月内"]
[145,7300300205,"金属软管","2.5JRL25F-500(加内衬筒)",null,"炼铁厂","根",8,"合同签订后1个月内"]
[146,7300300206,"金属软管","2.5JRL80F-500(加内衬筒)",null,"炼铁厂","根",8,"合同签订后1个月内"]
[147,7300300207,"金属软管","DN65","一头丝扣一头圆法兰;总长度950mm;短管弯头200mm","炼铁厂","根",6,"合同签订后1个月内"]
[148,7300300208,"金属软管","DN65","两头带方法兰,总长度930;短管弯头200mm带DN15排气阀孔","炼铁厂","根",12,"合同签订后1个月内"]
[149,7300300209,"金属软管","2.5JRL150F-800(加内衬筒)",null,"炼铁厂","根",4,"合同签订后1个月内"]
[150,7300300218,"金属软管","DN65","两头带快速接头，总长度900mm","炼铁厂","根",20,"合同签订后1个月内"]
[151,7300300190,"金属软管","15;G1/2;1000mm","带密封","能源分厂","根",20,"合同签订后1个月内"]
[152,7300300191,"金属软管","15;G1/2;1500mm","带密封","能源分厂","根",20,"合同签订后1个月内"]
[153,7300300192,"金属软管","20;G3/4;1000mm","带密封","能源分厂","根",20,"合同签订后1个月内"]
[154,7300300193,"金属软管","20;G3/4;1500mm","带密封","能源分厂","根",20,"合同签订后1个月内"]
[155,7300300194,"耐高温金属软管","6JRL200A-1000法兰连接，8孔，法兰中心孔距295mm","使用温度200度 压力；PN10   口径；DN200；介质；煤气；温度130℃;长度1米","能源分厂","只",12,"合同签订后1个月内"]
[156,7300300211,"耐高温金属软管","6JRL50A-700","介质:天燃气;使用温度:100度;长度700mm;口径DN50;法兰连接","能源分厂","根",8,"合同签订后1个月内"]