{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","附件","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"附件","index":1,"n_rows":12,"n_cols":9,"rows_kept":12,"merged":[[0,0,0,8]],"flags":["formulas_cached_only"]}
["附件清单"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","交货时间","使用部门"]
[1,"5000500069","齿轮减速电机","图号：89CLD-02-02-01","型号：R67DT80K4  电机型号：Y80M1-4  功率：0.55kw  转速17r/min（50HZ)","件","1","2021-10-30","89油管车丝委外"]
[2,"5000500076","齿轮减速电动机","OXT65-V1.5-75","功率1.5KW变频;380V；n1=1410rpm;n2=75rpm;电机选用变频调速电机;级数=4","台","2","2021-10-30","219厂部"]
[3,"5000500077","齿轮减速电动机","OXT65-1.5-38","功率1.5KW; 380V;n1=1410rpm;n2=38rpm;电机选用变频调速电机;级数=4","台","2","2021-10-30","219厂部"]
[4,"5000500081","轧钢辊道减速机","R57DV100L4","118r/min;输出转速-11.9;带电机","台","2","2021-10-30","219厂部"]
[5,"5603300002","冷却塔专用减速器","NW-L-F81","速比5.67;带30Kw电机;输出165r/min;IP55;S1工作制;Δ接法;B级;Lw≤72db(A)","台","1","2021-10-30","炼钢厂部"]
[6,"5706500038","轧钢辊道减速机","R67DV100L4/BMG/HF","带电机","台","1","2021-10-30","219厂部"]
[7,"5709700153","进口轧钢辊道电动机","KAZ97BDM180/BM/HF/TF/V SEW-EURORIVE","额定功率：22KW 额定电压：380V 额定电流：45A 额定转速：1460rpmm绝缘等级:F级 防护等级:IP54 安装方式B35 频率:50HZ","台","1","2021-10-30","340热轧"]
[8,"6000200429","轧钢减速电机","TKA48B-MY100L4-9.1-M1-A 3Kw 出口方向A 安装方式M1 i=9.1",null,"台","3","2021-10-30","219厂部"]
[9,"6000200863","辊道电动机","YGB132M2-8/B5 1.8KW","S1 星形接法 F级 IP54","台","3","2021-10-30","89热轧"]
[10,"6000200874","三相交流异步电机","YE2-80M2-4;0.75KW;带小齿轮","额定电压 380V; 额定电流 1.9A; 额定转速 1430r/min ;绝缘等级F; 防护等级IP55 ; 安装方式B5 ;接线方式 Y;功率因素0.76;50HZ;出厂编号12225","台","2","2021-10-30","89油管车丝委外"]

{"sheet":"Sheet1","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}