{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":36,"n_cols":11,"rows_kept":36,"merged":[[0,0,0,10],[1,0,1,10],[32,0,32,10],[33,0,33,10],[34,0,34,10],[35,0,35,10]],"flags":["formulas_cached_only"]}
["    （一）开标一览表"]
["项目名称：2022年3月液压缸采购项目                             项目编号：HGCGD22027"]
["序号","资材编号","资材名称","规格型号","技术参数","单位","数量","使用部门","交货时间","含税单价","生产厂家\n（品牌）"]
[1,7200200004,"夹钳升降液压缸","02690017DR5004ME002-39","额定压力25MPa 实验压力32MPa JB/T 5000","台",1,"180厂部","2022-06-30"]
[2,7201300061,"2#矫直机中下辊锁紧缸","Z8037.03.04.00",null,"台",2,"340热轧","2022-06-30"]
[3,7200600177,"切管机QG1163机械手用钢管夹紧液压缸","90/60-96",null,"台",4,"720厂部","2022-07-30"]
[4,7200600051,"切割移动辊道液压缸","63/45-1000","中间铰接式油缸 缸径Φ63,杆径Φ45,行程1000 工作环境温度-20℃~150℃ 工作压力25MPa,试验压力37.5MPa 活塞及活塞杆采用V型组合密封 伸缩防护套耐温150度 工作介质水乙二醇液压油","台",3,"炼钢厂部","2022-07-30"]
[5,7200600098,"液压缸","HYZ099-45 40/25-50","缸径Φ40,杆径Φ25,行程50 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",2,"340热轧","2022-07-30"]
[6,7200100336,"液压缸","CD250E160/110-1200A10/02-CGDMA+GAK80,L10=892.5","缸径Φ160,杆径110,行程1200， 工作环境温度-20℃~70℃ 工作压力15MPa,试验压力18MPa 活塞及活塞杆采用V型组合密封","台",1,"340热轧","2022-05-30"]
[7,7200100176,"液压缸","SF601859","额定压力25MPa JB/T 5000","台",4,"180厂部","2022-07-30"]
[8,7200500069,"液压缸","0107119-41.011",null,"台",2,"180厂部","2022-07-30"]
[9,5716000025,"切管机QG1163机械手用钢管夹紧液压缸","90/60-170",null,"台",8,"720厂部","2022-06-30"]
[10,7200100409,"液压油缸","CD250B160/100-350ACGDMA",null,"台",4,"219厂部","2022-05-30"]
[11,7200100374,"脱管机机架推拉液压缸","按CD250C125/90-2000A10/01CGDMA标准制造，带磁环，不带位移传感器，带耳环，压力等级250BAR",null,"台",1,"89热轧","2022-05-30"]
[12,7200100301,"液压缸","02680014DR5005ME052-13","CD250E63/36-160A10/01CGDMA,L10=315","台",1,"89热轧","2022-05-30"]
[13,7200600206,"液压缸","YF0176-23P","CD250E50/36-220A10/01CADMA;L10=200,带与位移传感器953AC40230MXXSX相配的磁环；不带传感器","台",2,"89热轧","2022-05-30"]
[14,7501800045,"液压缸活塞杆","H-268-4H-4","45；27.4kg","根",5,"89热轧","2022-05-30"]
[15,7501800046,"液压缸活塞杆","HM28R100","45;24.7Kg","根",2,"89热轧","2022-05-30"]
[16,7502000053,"液压缸耳环","GAK45",null,"件",6,"219厂部","2022-06-30"]
[17,7200600237,"快开油缸","KZ1810.02.01.01.00","缸径Φ280,杆径Φ140, 工作压力25MPa,试验压力25MPa 工作环境温度-20℃~70℃，厂家：太原科达重工成套设备有限公司","套",1,"89油管热处理","2022-06-30"]
[18,7200600238,"快开油缸","KZ1810.02.03.01.00","工作压力32MPa,试验压力25MPa 工作环境温度-20℃~70℃，厂家：太原科达重工成套设备有限公司","套",1,"89油管热处理","2022-06-30"]
[19,7200100410,"宽辊道挡管器油缸","液压缸;CD250F80/56-200A10/01CADMA","缸径80，杆径56，行程200，压力等级25MPA","台",1,"219厂部","2022-05-30"]
[20,7200600228,"液压缸","Z0745.04.03.03G","100/70-1185;耐压等级25MPA；耐高温；带GAS50耳环。","台",3,"180厂部","2022-05-30"]
[21,7200100411,"液压缸","CD250B125/90-280A10/01CADMA","带铰接头GAS60","台",2,"720厂部","2022-05-30"]
[22,7200100412,"液压缸","CD250B160/100-180A10/01CGDMA",null,"台",1,"720厂部","2022-05-30"]
[23,7200100413,"液压缸","ETBKC2056 CD250A160/110-180A10",null,"台",1,"720厂部","2022-05-30"]
[24,7200100414,"液压缸","CD250E200/140-735A10/01CGDMA-L10=771",null,"台",1,"720厂部","2022-05-30"]
[25,7200100415,"液压缸","CD250E200/140-500A10/01CGDMA-L10=580",null,"台",1,"720厂部","2022-05-30"]
[26,7200100416,"液压缸","CD250F200/140-480A10/02CADMA",null,"台",1,"720厂部","2022-05-30"]
[27,5722600045,"带锯机夹紧油缸","G4240/60",null,"台",1,"180厂部","2022-05-30"]
[28,7200500069,"液压缸","0107119-41.011",null,"台","2","180厂部","2022-08-10"]
[29,7200500078,"液压缸","KZ2102.01.01.01","规格125/90-135;不带位移传感器；需留有位移传感器接口；带磁环；带关节轴承；耐压等级250bar；耳环与活塞杆整体锻造","台","3","180厂部","2022-05-30"]
["注：1、投标报价含税，税率13% ；                                                                                                                          2、生产厂家要求全称填写准确无误 ；                                                                                                                     3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）；"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2022年3月液压缸采购项目                             项目编号：HGCGD22027"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]