{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":48,"n_cols":11,"rows_kept":48,"merged":[[0,0,0,10],[1,0,1,10],[44,0,44,10],[45,0,45,10],[46,0,46,10],[47,0,47,10]],"flags":["formulas_cached_only"]}
["    （一）开标一览表"]
["项目名称：2022年4月液压备件等采购项目                            项目编号：HGCGD22038"]
["序号","资材编号","资材名称","规格型号","技术参数","单位","数量","使用部门","交货时间","含税单价\n(元）","生产厂家\n（品牌）"]
[1,7100300421,"电磁换向阀","WV700-6-3/3-E-24-V-C*00;Bieri","DN6，耐压等级70Mpa","只",1,"720厂部","2022-07-28"]
[2,7100300422,"液控单向阀","405063 006;Dr.BREIT","DN70，耐压等级31.5Mpa;","只",1,"720厂部","2022-07-28"]
[3,5712000039,"气缸","DNG-250-80-PPV-A 151892 FESTO",null,"台",2,"340热轧","2022-06-30"]
[4,7200700014,"液压马达","MR7000M-P2E1F1N1N RIVA CALZONI OLEODINAMICA",null,"台",1,"340热轧","2022-07-28"]
[5,7000400008,"叶片泵","150T-75-F-R",null,"台",2,"720厂部","2022-06-30"]
[6,7501100233,"铰接式接头","12-G3/8(SN865-WH12SR-KDS)不锈钢","SN865-WH12SR-KDS不锈钢","只",100,"180厂部","2022-06-30"]
[7,7501100233,"铰接式接头","12-G3/8(SN865-WH12SR-KDS)不锈钢","SN865-WH12SR-KDS不锈钢","只",40,"340热轧","2022-06-30"]
[8,7100700011,"同步马达","FMP-2I-EB",null,"台",1,"340热轧","2022-06-30"]
[9,7200900060,"气缸","QGSQ100*300MT4-Y","行程300，气管接头与耳轴错开90°，接头尺寸G1/2","件",4,"高炉","2022-06-30"]
[10,7201300094,"活塞筒体BARREL","27774","PUMP SECTOPM -T SEAL 3/4\" PACKED PLUNGER GAS BOOSTER -315 RATIO ;CODE IDENT NO. 81400;DWG NO.27780;Haskel气体增压泵14AGT-125/315-29125用","件",1,"检验检测中心","2022-06-30"]
[11,7201300095,"活塞杆PLUNGER","28199","PUMP SECTOPM -T SEAL 3/4\" PACKED PLUNGER GAS BOOSTER -315 RATIO ;CODE IDENT NO. 81400;DWG NO.27780;Haskel气体增压泵14AGT-125/315-29125用","件",1,"检验检测中心","2022-06-30"]
[12,7500400070,"炉顶液压站过滤器","SRFA-250×10FC","配套滤芯型号：FAX-250×10","台",1,"高炉","2022-06-30"]
[13,7000200060,"螺杆泵组","HSG940*2-42TQ/YB180L-4","压力1.0MPa；流量740L/min，介质46#汽轮机油；带电机，电机型号YB180L-4","台",1,"高辅工段","2022-06-30"]
[14,7500500022,"过滤器滤芯","0330D005BN4HC HYDAC",null,"只","4","89热轧","2022-07-28"]
[15,7500500036,"过滤器滤芯","0660R010BN4HC HYDAC",null,"只","4","340热轧","2022-07-28"]
[16,7500500032,"过滤器滤芯","0660D010BN4HC HYDAC",null,"只","10","720厂部","2022-07-28"]
[17,7500500033,"过滤器滤芯","0850R005BN4HC HYDAC",null,"只","10","720厂部","2022-07-28"]
[18,7500500037,"过滤器滤芯","0850R010BN4HC HYDAC",null,"只","4","340热轧","2022-07-28"]
[19,7500500023,"过滤器滤芯","0330R010BN4HC HYDAC",null,"只","4","340热轧","2022-07-28"]
[20,7500500019,"过滤器滤芯","1300R010BN4HC 过滤精度10um","纸质 HYDAC","只","4","340热轧","2022-07-28"]
[21,7500500040,"过滤器滤芯","0850R020BN4HC HYDAC",null,"只","10","720厂部","2022-07-28"]
[22,7000500016,"手动液压装卸车","CTYB-2000",null,"台","1","89热轧","2022-06-30"]
[23,7000100069,"恒压变量泵","KD-A10VSO71DFR1/31R-PPA12N00","平键安装，顺时针旋向，SAE法兰连接。科达液压","台","1","720厂部","2022-07-28"]
[24,7000200050,"叶片泵","1PV2V4-2X/50RA01MC1-16A1","品牌：WERDOHLER","台","1","89热轧","2022-06-30"]
[25,7100700001,"齿轮式分流马达","JXA-022Q-VB100-N KINSSON-HYDRAULK",null,"台","1","720厂部","2022-06-30"]
[26,7200700012,"液压马达","NHM16-1600D3 进出油口和泄漏油口在同一面",null,"台","1","180厂部","2022-06-30"]
[27,7000500011,"液压马达","JMDG2-100",null,"台","2","89油管热处理","2022-06-30"]
[28,7002000009,"液压马达","BM3-100P-A-Y",null,"台","2","89油管热处理","2022-06-30"]
[29,7000100032,"液压泵","63PCY14-1B","排量63ml/r，定量泵，顺时针，平键安装","台","2","89油管热处理","2022-06-30"]
[30,7000300023,"人字齿轮泵","RCB160 逆时针",null,"台","1","340热轧","2022-06-30"]
[31,7000300024,"人字齿轮泵","RCB160 顺时针",null,"台","1","340热轧","2022-06-30"]
[32,7000300017,"齿轮油泵","CB-B125",null,"台","2","720厂部","2022-06-30"]
[33,7100300383,"方向阀芯","Z32A20",null,"只","4","管加工厂部","2022-06-30"]
[34,7402100202,"密封圈","HJT01-206，","聚氨酯;    耐压等级120Mpa ， 定制非标，","套","8","管加工厂部","2022-06-30"]
[35,7500600055,"蓄能器组","Z0745.90.00.01","按图纸要求；含油路块、蓄能器、蓄能器控制阀组、油盆、阀台架及其它附件","套","4","管加工厂部","2022-06-30"]
[36,7200600234,"气缸","SC 80*600 AirTAC","缸径：80，行程：600","台","3","89油管热处理","2022-06-30"]
[37,7201100078,"140：不锈钢三爪气缸","不锈钢三爪气缸  MI 25*35","不锈钢三爪气缸  MI 25*35","台","4","89包装","2022-06-30"]
[38,7501600005,"油水分离储液罐","200L","用于液压油和水的混合物等杂质分离；物理静置分离；立式；材质Q235-B;箱体直径Ф618mm*高750mm*厚1.5mm,总高1250mm","个","1","检验检测中心","2022-06-30"]
[39,4300100016,"TRT动静叶片缓蚀阻垢药剂(气相)","SGR-1002",null,"KG",3000,"炼铁厂","2022-04-30"]
[40,7100900049,"给油指示器","GZQ-15","公称压力15bar；公称通径15;丝G3/8","只",4,"180厂部","2022-06-30"]
[41,7000800028,"干油喷射阀","GPZ-135",null,"只",8,"180厂部","2022-06-30"]
["注：1、投标报价含税，税率13% ；                                                                                                                          2、生产厂家要求全称填写准确无误 ；                                                                                                                     3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）；"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2022年4月液压备件等采购项目                       项目编号：HGCGD22038"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]