{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":28,"n_cols":13,"rows_kept":28,"merged":[[0,0,0,8],[1,0,1,12],[24,0,24,8],[25,0,25,8],[26,0,26,8],[27,0,27,8]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2022年6月机械备件采购项目Ⅱ                     项目编号：HGCGD22088"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,6600300167,"电动调节阀","RXDF-1v PN40 DN65","公称压力：4.0MPa，通径65mm，阀体材质：ZG230-450,滤芯材质OCr 18Ni 9,带配套电动执行机构","台",1,"TS-2743018-2022","能源厂部","2022-07-27"]
[2,5501700003,"堆取料机;斗轮机构轴承座","D223A-11.0","ZG35 孔径50，轴向孔距145，径向孔距530，座低平面与孔中心线夹角5°侧端盖带注油孔M10","件",2,null,"原料工段","2022-09-10"]
[3,5723700007,"阀座","SFA9.120-08","材质0Cr18Ni9Ti; 0.7kg;","件",10,"GB/T24588-2009","管加工厂部","2022-08-26"]
[4,5723700002,"密封单向阀组阀座","MDXFZB20.15-VS","材质0Cr18Ni9Ti; 1.3kg;","件",4,"GB/T24588-2009","管加工厂部","2022-07-27"]
[5,5723700003,"增压单向阀组阀芯","ZDXFZB20.100-VC","材质0Cr18Ni9Ti;   1.4kg;","件",4,"GB/T24588-2009","管加工厂部","2022-07-27"]
[6,5723700004,"增压单向阀组阀座","ZDXFZB20.100-VS","材质0Cr18Ni9Ti;   2.2kg;","件",4,"GB/T24588-2009","管加工厂部","2022-07-27"]
[7,7101600168,"气动控制阀门","D376XE73;OMAL","DN125;OMAL;带执行器","台",1,"ISO5211","89油管车丝委外","2022-08-26"]
[8,5501000072,"烧结筛筛板","TTHBS-350-2","单层双面悬臂棒条    材质：55CrSi","套",2,"JB5015-1985","高辅工段","2022-08-26"]
[9,5400100044,"离心式空压机 中间冷却器","FS-ELLIOTT 260","铆焊 材质：管道为紫铜，翅片为铝 耐压大于1.6Mpa 耐温大于250℃ 冷却气量大于300m3/min 冷却出口温度<52℃","台",1,"JB/T10598","能源厂部","2022-07-12"]
[10,5601700022,"拖链","TL180III-R450*510*8640","支撑板宽度510mm:节数48;附订货图","件",2,"JB/T6608-1993","炼钢厂部","2022-07-27"]
[11,5713700093,"拖链","02690045DR5005ME053-34；1600Kg；",null,"件",1,"审核图纸","720厂部","2022-08-26"]
[12,5701900190,"3#水压增压器","18Q00601.04.01","φ300/φ140-800;2000kg;原制作厂家:宁波骏嘉","件",1,"审核图纸","89油管热处理","2022-07-27"]
[13,5000400014,"减速机","QSC16-14",null,"台",1,"JB/T8853-1999","炼钢厂部","2022-08-26"]
[14,5602600064,"点火枪","YI025BS-LZJ-440L","接头螺纹G3/8","把",8,"GB25723-2010","炼钢厂部","2022-08-26"]
[15,5714100070,"马达行星减速箱","0102040-82.007","不包含马达","台",1,"审核图纸","720厂部","2022-08-26"]
[16,5701300172,"调角机构","KZ1810.02.01.05.00","不带电机减速机","套",1,"审核图纸","89油管热处理","2022-08-26"]
[17,5603400079,"走行减速机（右）","68017.12.01","带11KW电机;带制动（手动释放）;带缓冲垫2个;立式安装","台",1,"审核图纸","炼钢厂部","2022-08-26"]
[18,5603400080,"走行减速机（左）","68017.04.01","带11KW电机;带制动（手动释放）;带缓冲垫2个;立式安装","台",1,"审核图纸","炼钢厂部","2022-08-26"]
[19,5000400115,"减速机","型号：KF127A-102-AE5-B51-100626E；速比：i=102","输入：nf=1450rpm；速比：i=102","台",1,"Q/ZTB 06-2001","720厂部","2022-08-26"]
[20,5400100135,"初效板式空气过滤器","595*595*46","铆焊 框板式折叠V型密褶式过滤器，材质：玻璃纤维，过滤精度20um","块",160,null,"能源厂部","2022-08-27"]
[21,5501700066,"堆取料机:大车行走电机减速箱","K310TK-D13-D421-YZ132M4B75AC3-F0H01-044+G20","内花键输出 N85×3m×27z×9H/DIN5480；配冶金起重用变频制动电机 7.5KW-4 极，电机端小齿轮另配套2个","套",4,"JB/T2982-1994","原料工段","2022-08-12"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2022年6月机械备件采购项目Ⅱ           项目编号：HGCGD22088"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":4,"n_cols":1,"rows_kept":4,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,8],[3,0,3,8]],"flags":["formulas_cached_only"]}
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]