{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":27,"n_cols":13,"rows_kept":27,"merged":[[0,0,0,8],[1,0,1,12],[23,0,23,8],[24,0,24,8],[25,0,25,8],[26,0,26,8]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2022年8月机械备件采购项目                     项目编号：HGCGD22101"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,5000400014,"减速机","QSC16-14",null,"台",1,"JB/T8853-1999","炼钢厂部","2022-09-26"]
[2,5000400112,"蜗轮蜗杆斜齿轮减速机","SA92-1/100-YEJ4kW-6P-M1","传动比47.2;额定功率4Kw;配反力矩环板GST97-01QT K","台",2,"Q/ZTB04-2000","炼钢厂部","2022-09-26"]
[3,5400100044,"离心式空压机 中间冷却器","FS-ELLIOTT 260","铆焊 材质：管道为紫铜，翅片为铝 耐压大于1.6Mpa 耐温大于250℃ 冷却气量大于300m3/min 冷却出口温度<52℃","台",1,"JB/T10598","能源厂部","2022-09-26"]
[4,5501700003,"堆取料机;斗轮机构轴承座","D223A-11.0","ZG35 孔径50，轴向孔距145，径向孔距530，座低平面与孔中心线夹角5°侧端盖带注油孔M10","件",2,null,"原料工段","2022-09-26"]
[5,7502300044,"1#机分体点火枪","DHQ304-L280","材质304不锈钢;接口方式M14*1.5","把",2,"JB5101-1991","炼钢厂部","2022-09-26"]
[6,5601700022,"拖链","TL180III-R450*510*8640","支撑板宽度510mm:节数48;附订货图","件",2,"JB/T6608-1993","炼钢厂部","2022-09-26"]
[7,6100100031,"交流电焊机","BX3-500-2","380V","台",13,"GB/T8118-1995","高辅工段","2022-09-26"]
[8,7500300011,"冷却器","ASA-PL53-20EKit",null,"台",3,"JB/T4715-1992","180厂部","2022-09-26"]
[9,7502500096,"离心通风机","F9-26-5D;左旋90°","15Kw 2900r/min 带轴承座","台",1,"GB/T13274-1991","炼钢厂部","2022-09-26"]
[10,7502500097,"离心通风机","F9-26-5D;右旋90°","15Kw 2900r/min 带轴承座","台",1,"GB/T13274-1991","炼钢厂部","2022-09-26"]
[11,6300600034,"卧式车床","呼合环球卡盘板手","CA6136 K11200","把",5,"JIS B6151-1993","检验检测中心","2022-09-26"]
[12,6700200044,"冲击试验机 硫化氢减压阀 R11LG-EGG-00-00","R11LG-EGG-00-00",null,"只",1,"JB/T10365-2002","检验检测中心","2022-09-26"]
[13,7001200343,"高压泵连杆","3D-250-0102",null,"根",4,null,"219厂部","2022-09-26"]
[14,5704000030,"铝合金手轮","空心16*160键5","空心16*160键5；G4250带锯机用","个",6,"JB/T4318.2-2002","检验检测中心","2022-09-26"]
[15,7101800177,"不锈钢水嘴",15,null,"只",10,"CJ/T406-2012","219厂部","2022-09-26"]
[16,7502500087,"离心通风机","225FLJ7F","380V/50Hz;170w","台",5,"JB/T2977-1992","89油管车丝委外","2022-09-26"]
[17,7502300059,"空气喷嘴","780LA；07800269351","连接螺纹G11/2,替换开口管直径38mm，最高工作压力1MPa,重量3.484kg，材料1.4305（303）；品牌SILVENT","只",3,"JB/T12493-2014","89油管热处理","2022-09-26"]
[18,5501000065,"焦炭筛聚氨酯筛板","GY20220127-CX","介质：焦炭，材质：聚氨酯，使用寿命3个月处理能力300吨/小时。包含整套焦炭筛所用聚氨酯HW筛板和聚氨酯HW筛板托架。槽下全套筛板由16块高弹悬浮面小筛板","套",4,"审核图纸","高辅工段","2022-09-26"]
[19,5501000072,"烧结筛筛板","TTHBS-350-2","单层双面悬臂棒条    材质：55CrSi","套",2,"JB5015-1985","高辅工段","2022-09-26"]
[20,5501000064,"往复筛分机","KER-1500*700","上层方孔40*40mm;下层方孔25*25mm","台",1,null,"原料工段","2022-08-15"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2022年8月机械备件采购项目            项目编号：HGCGD22101"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":4,"n_cols":1,"rows_kept":4,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,8],[3,0,3,8]],"flags":["formulas_cached_only"]}
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]