{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":79,"n_cols":14,"rows_kept":79,"merged":[[0,1,0,9],[1,1,1,9],[51,6,52,6],[53,6,55,6],[56,6,57,6],[75,0,75,8],[76,0,76,3],[77,0,77,3],[78,0,78,3]]}
[null,"（一）开标一览表"]
[null,"项目名称：2022年8月工程类阀门采购项目                                              项目编号：HGCGD22111"]
["序号","物料编码","物料描述","规格型号","材质牌号","计量单位","定尺尺寸\n其他要求","计划数量","建议交货日期","交货地点","含税单价(元)","含税金额（元）","生产厂家","备注"]
[1,null,"手动球阀\n（带活接头） ","Q11F-16P，DN50，P=1.0MPa，内丝连接",null,"个","配两端接管活接头，活接头材质碳钢,交货时活接头与阀门连接",4,"2022-08-30","涟钢建设"]
[2,null," 304不锈钢内丝水流指示器","DN50，P=1.0MPa ，内丝连接",null,"个","配两端接管活接头，活接头材质碳钢，交货时活接头与阀门连接",2,"2022-08-30","涟钢建设"]
[3,null,"手动球阀\n（带活接头） ","Q11F-16P，DN50，P=1.0MPa，内丝连接",null,"个","配两端接管活接头，活接头材质碳钢，交货时活接头与阀门连接",4,"2022-08-30","涟钢建设"]
[4,null," 304不锈钢内丝水流指示器","DN50，P=1.0MPa ，内丝连接",null,"个","配两端接管活接头，活接头材质碳钢，交货时活接头与阀门连接",2,"2022-08-30","涟钢建设"]
[5,null,"手动球阀\n（带活接头） ","Q11F-16P，DN25，P=1.0MPa，丝扣连接",null,"个","配两端接管活接头，活接头材质碳钢，交货时活接头与阀门连接",3,"2022-08-30","二十三冶"]
[6,null,"手动球阀\n（带活接头） ","Q11F-16P，DN50，P=1.0MPa，内丝连接",null,"个","配两端接管活接头，活接头材质碳钢，交货时活接头与阀门连接",4,"2022-08-30","二十三冶"]
[7,null,"手动球阀\n（带活接头） ","Q11F-16P，DN70，P=1.0MPa，丝扣连接",null,"个","配两端接管活接头，活接头材质碳钢，交货时活接头与阀门连接",2,"2022-08-30","二十三冶"]
[8,null," 304不锈钢内丝水流指示器","DN50，P=1.0MPa ，内丝连接",null,"个","配两端接管活接头，活接头材质碳钢，交货时活接头与阀门连接",2,"2022-08-30","二十三冶"]
[9,null,"手动球阀\n（带活接头） ","Q11F-16P，DN50，P=1.0MPa，内丝连接",null,"个","配两端接管活接头，活接头材质碳钢，交货时活接头与阀门连接",4,"2022-08-30","涟钢建设"]
[10,null,"手动球阀\n（带活接头） ","Q11F-16P，DN70，P=1.0MPa，丝扣连接",null,"个","配两端接管活接头，活接头材质碳钢，交货时活接头与阀门连接",2,"2022-08-30","涟钢建设"]
[11,null,"双向承压法兰式手动蝶阀 ","型号：D341X-10Q\n规格：DN200  P＝1.0MPa  \n",null,"台","规格：DN200 P＝1.0MPa\n阀体――球铁，轴――不锈钢，阀板―\n―球铁\n带配对法兰、垫片及紧固件，交货时法兰螺栓与阀门连接",1,"2022-08-30","二十三冶"]
[12,null,"法兰式手动球阀 ","Q41F-10C，DN100,PN1.0MPa",null,"台","带配对法兰、垫片及紧固件，交货时法兰螺栓与阀门连接",15,"2022-08-30","二十三冶"]
[13,null,"双向承压法兰式手动蝶阀 ","型号：D341X-10Q\n规格：DN80  P＝1.0MPa  \n",null,"台","材质：阀体――球铁，轴――不锈钢，阀板――球铁，密封圈或者阀座――三元乙丙 \n带配对法兰及紧固件，交货时法兰螺栓与阀门连接",8,"2022-08-30","二十三冶"]
[14,null,"双向承压法兰式手动蝶阀 ","型号：D341X-10Q \n规格：DN100  P＝1.0MPa  \n",null,"台","材质：阀体――球铁，轴――不锈钢，阀板――球铁，密封圈或者阀座――三元乙丙 \n带配对法兰及紧固件，交货时法兰螺栓与阀门连接",8,"2022-08-30","二十三冶"]
[15,null,"双向承压法兰式手动蝶阀 ","型号：D341X-10Q \n规格：DN125  P＝1.0MPa  \n",null,"台","材质：阀体――球铁，轴――不锈钢，阀板――球铁，密封圈或者阀座――三元乙丙 \n带配对法兰及紧固件，交货时法兰螺栓与阀门连接",4,"2022-08-30","二十三冶"]
[16,null,"双向承压法兰式手动蝶阀 ","型号：D341X-10Q \n规格：DN200  P＝1.0MPa  \n",null,"台","材质：阀体――球铁，轴――不锈钢，阀板――球铁，密封圈或者阀座――三元乙丙 \n带配对法兰及紧固件，交货时法兰螺栓与阀门连接",8,"2022-08-30","二十三冶"]
[17,null,"Y型过滤器","GL41H-16Q，DN125",null,"台","阀体材质：球墨铸铁，滤网：不锈钢，带配对法兰、螺栓及密封紧固件，交货时法兰螺栓与阀门连接",{"v":2,"d":"2.0"},"2022-08-30","二十三冶"]
[18,null,"内螺纹手动球阀","Q11H-16C，DN25，P=1.6MPa，内丝连接",null,"个",null,36,"2022-08-30","涟钢建设"]
[19,null,"手动闸阀","Z41H-16C,DN80,P=1.6MPa,法兰连接，介质：压缩空气",null,"个","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",1,"2022-08-30","涟钢建设"]
[20,null,"手动闸阀","Z41H-16C,DN150,P=1.6MPa,法兰连接，介质：压缩空气",null,"个","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",1,"2022-08-30","涟钢建设"]
[21,null,"手动闸阀","Z41H-16C,DN200,P=1.6MPa,法兰连接，介质：压缩空气",null,"个","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",2,"2022-08-30","涟钢建设"]
[22,null,"法兰式手动闸阀","Z41H-25C,DN200,P=2.5MPa,法兰连接，介质：250℃蒸汽",null,"个","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",2,"2022-08-30","涟钢建设"]
[23,null,"法兰式手动闸阀","Z41H-25C,DN100,P=2.5MPa,法兰连接，介质：250℃蒸汽",null,"个","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",1,"2022-08-30","涟钢建设"]
[24,null,"法兰式手动闸阀","Z41H-25C,DN50,P=2.5MPa,法兰连接，介质：250℃蒸汽",null,"个","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",1,"2022-08-30","涟钢建设"]
[25,null,"法兰式手动截止阀","J41H-25C,DN25,P=2.5MPa,法兰连接，介质：蒸汽凝结水",null,"个","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",18,"2022-08-30","涟钢建设"]
[26,null,"自由浮球式疏水阀","CS41H-25C,DN25,P=2.5MPa,法兰连接，介质：蒸汽凝结水",null,"个","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",6,"2022-08-30","涟钢建设"]
[27,null,"疏水阀","CS44H-16,DN20，P=1.6MPa,法兰连接",null,"套","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",1,"2022-08-28","二十三冶"]
[28,null,"旋启式止回阀","H44H-16C,DN65,P=1.6MPa，法兰连接",null,"套","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",3,"2022-08-28","二十三冶"]
[29,null,"内螺纹截止阀","J11H-16C,DN20，p=1.6MPa，丝接",null,"套",null,1,"2022-08-28","二十三冶"]
[30,null,"手动法兰截止阀","J41H-16C,DN65，p=1.6MPa，法兰连接",null,"套","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",6,"2022-08-28","二十三冶"]
[31,null,"手动法兰球阀","Q41H-16C,DN80,P=1.6MPa，法兰连接",null,"套","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",2,"2022-08-28","二十三冶"]
[32,null,"手动法兰球阀","Q41H-16C,DN100,P=1.6MPa，法兰连接",null,"套","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",1,"2022-08-28","二十三冶"]
[33,null,"手动法兰球阀","Q41H-16C,DN125,P=1.6MPa，法兰连接",null,"套","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",3,"2022-08-28","二十三冶"]
[34,null,"手动法兰球阀","Q41H-16C,DN150,P=1.6MPa，法兰连接",null,"套","带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",1,"2022-08-28","二十三冶"]
[35,null,"法兰止回阀","H44H-16C,DN100,P=1.6MPa，法兰连接",null,"套","带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",2,"2022-08-30","二十三冶"]
[36,null,"内螺纹球阀","Q11F-16C，DN15,P=1.6MPa,内丝连接",null,"套",null,18,"2022-08-30","二十三冶"]
[37,null,"内螺纹球阀","Q11F-16C，DN25,P=1.6MPa,内丝连接",null,"套",null,40,"2022-08-30","二十三冶"]
[38,null,"法兰截止阀","J41H-16C,DN32，p=1.6MPa，法兰连接",null,"台","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",6,"2022-08-30","二十三冶"]
[39,null,"法兰截止阀","J41H-16C,DN40，p=1.6MPa，法兰连接",null,"台","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",2,"2022-08-30","二十三冶"]
[40,null,"法兰截止阀","J41H-16C,DN50，p=1.6MPa，法兰连接",null,"台","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",4,"2022-08-30","二十三冶"]
[41,null,"法兰截止阀","J41H-16C,DN65，p=1.6MPa，法兰连接",null,"台","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",2,"2022-08-30","二十三冶"]
[42,null,"法兰截止阀","J41H-16C,DN80，p=1.6MPa，法兰连接",null,"台","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",2,"2022-08-30","二十三冶"]
[43,null,"法兰截止阀","J41H-16C,DN100，p=1.6MPa，法兰连接",null,"台","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",2,"2022-08-30","二十三冶"]
[44,null,"法兰式天然气球阀","Q41H-10C，DN50，P=1.0MPa，法兰连接",null,"台","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",8,"2022-08-30","二十三冶"]
[45,null,"法兰式天然气球阀","Q41H-10C，DN80，P=1.0MPa，法兰连接",null,"台","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",2,"2022-08-30","二十三冶"]
[46,null,"法兰式天然气球阀","Q41H-10C，DN150，P=1.0MPa，法兰连接",null,"台","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",1,"2022-08-30","二十三冶"]
[47,null,"法兰式手动闸阀","Z41W-10C，DN100，P=1.0MPa，法兰连接",null,"台","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",2,"2022-08-30","二十三冶"]
[48,null,"法兰式手动球阀","Q41H-16C，DN50，P=1.6MPa，法兰连接",null,"台","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",11,"2022-08-30","二十三冶"]
[49,null,"法兰式手动截止阀","J41H-16C,DN50，p=1.6MPa，法兰连接",null,"台","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",3,"2022-08-30","二十三冶"]
[50,null,"法兰式手动截止阀","J41H-16C,DN250，p=1.6MPa，法兰连接",null,"台",null,1,"2022-08-30","二十三冶"]
[51,null,"法兰式手动球阀","Q41H-10C，DN25，P=1.0MPa，法兰连接",null,"台","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",36,"2022-08-30","二十三冶"]
[52,null,"法兰式手动球阀","Q41H-10C，DN50，P=1.0MPa，法兰连接",null,"台",null,7,"2022-08-30","二十三冶"]
[53,null,"法兰式手动球阀","Q41H-10C，DN80，P=1.0MPa，法兰连接",null,"台",null,3,"2022-08-30","二十三冶"]
[54,null,"法兰式手动闸阀","Z41W-10C，DN50，P=1.0MPa，法兰连接",null,"台","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",2,"2022-08-30","二十三冶"]
[55,null,"法兰式手动闸阀","Z41W-10C，DN250，P=1.0MPa，法兰连接",null,"台",null,2,"2022-08-30","二十三冶"]
[56,null,"内螺纹球阀","Q11F-10C，DN25,P=1.0MPa,内丝连接",null,"个",null,{"v":13,"d":"13.00"},"2022-08-30","二十三冶"]
[57,null,"双向承压法兰式手动蝶阀 ","型号：D341X-10Q\n规格：DN125  P＝1.0MPa  \n",null,"个","规格：DN125 P＝1.0MPa\n阀体――球铁，轴――不锈钢，阀板―\n―球铁\n带配对法兰、垫片及紧固件，交货时法兰螺栓与阀门连接",{"v":2,"d":"2.00"},"2022-08-30","二十三冶"]
[58,null,"双向承压法兰式手动蝶阀 ","型号：D341X-10Q\n规格：DN200  P＝1.0MPa  \n",null,"个","规格：DN200 P＝1.0MPa\n阀体――球铁，轴――不锈钢，阀板―\n―球铁\n带配对法兰、垫片及紧固件，交货时法兰螺栓与阀门连接",{"v":1,"d":"1.00"},"2022-08-30","二十三冶"]
[59,null,"双向承压法兰式手动蝶阀 ","型号：D341X-10Q\n规格：DN250  P＝1.0MPa  \n",null,"个","规格：DN250 P＝1.0MPa\n阀体――球铁，轴――不锈钢，阀板―\n―球铁\n带配对法兰、垫片及紧固件，交货时法兰螺栓与阀门连接",{"v":2,"d":"2.00"},"2022-08-30","二十三冶"]
[60,null,"法兰截止阀","J41H-16C,DN65，p=1.6MPa，法兰连接",null,"台","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",2,"2022-08-22","二十三冶"]
[61,null,"法兰截止阀","J41H-16C,DN150，p=1.6MPa，法兰连接",null,"台","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",2,"2022-08-22","二十三冶"]
[62,null,"法兰截止阀","J41H-16C,DN50，p=1.6MPa，法兰连接",null,"台","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",2,"2022-08-22","二十三冶"]
[63,null,"法兰截止阀","J41H-16C,DN40，p=1.6MPa，法兰连接",null,"台","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",2,"2022-08-22","二十三冶"]
[64,null,"法兰截止阀","J41H-16C,DN32，p=1.6MPa，法兰连接",null,"台","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",2,"2022-08-22","二十三冶"]
[65,null,"法兰截止阀","J41H-16C,DN25，p=1.6MPa，法兰连接",null,"台","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",7,"2022-08-22","二十三冶"]
[66,null,"法兰闸阀","Z41H-16C，DN400，PN1.6MPa，介质:天然气","密封材质-合金密封，压力等级：1.6MPa，阀体材质：WCB","台","阀体长度：406mm，带配对法兰（锻钢整体制造），紧固件及垫片，供货时要求：法兰与阀体用匹配螺栓紧固连接，以便清点验收。",2,"2022-08-30","涟钢建设"]
[67,null,"法兰式手动球阀","Q41H-16C，DN150，P=1.6MPa，法兰连接",null,"台","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",1,"2022-08-30","涟钢建设"]
[68,null,"法兰式手动球阀","Q41H-16C，DN200，P=1.6MPa，法兰连接",null,"台","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",1,"2022-08-30","涟钢建设"]
[69,null,"手动盲板阀","F343X-2.5C DN400,压力等级：0.25MPa",null,"台","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",2,"2022-08-30","涟钢建设"]
[70,null,"硬密封手动法兰蝶阀","D343H-2.5C,DN400,压力等级：0.25MPa",null,"台","阀体材质：铸钢；带配对法兰及密封紧固件，交货时法兰螺栓与阀门连接",2,"2022-08-30","涟钢建设"]
[71,null,"法兰闸阀","Z41H-10C，DN100，PN1.0MPa，介质:天然气","密封材质-合金密封，压力等级：1.0MPa，阀体材质：WCB","台","0带配对法兰（锻钢整体制造），紧固件及垫片，供货时要求：法兰与阀体用匹配螺栓紧固连接，以便清点验收。",8,"2022-08-30","涟钢建设"]
[{"$nulls":9},"合计"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet2","index":1,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]]}
["   （二）商务/技术偏离表"]
["项目名称：2022年8月工程类阀门采购项目               项目编号：HGCGD22111"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet3","index":2,"n_rows":4,"n_cols":1,"rows_kept":4,"merged":[[1,0,1,3],[2,0,2,3],[3,0,3,3]]}
[]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]