{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":29,"n_cols":13,"rows_kept":29,"merged":[[0,0,0,8],[1,0,1,12],[25,0,25,8],[26,0,26,8],[27,0,27,8],[28,0,28,8]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2022年9月机械配件采购项目Ⅱ                     项目编号：HGCGD22127"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,6700200044,"冲击试验机 硫化氢减压阀 R11LG-EGG-00-00","R11LG-EGG-00-00",null,"只",1,"JB/T10365-2002","检验检测中心","2022-11-26"]
[2,7001200343,"高压泵连杆","3D-250-0102",null,"根",4,null,"219厂部","2022-11-26"]
[3,5702000063,"充水阀","18Q00601.01.05","装配件;185kg;配安装螺栓。","件",1,"审核图纸","89油管热处理","2022-11-26"]
[4,5702000062,"排气阀","18Q00601.02.02","装配件;164.9kg;配安装螺栓。","件",1,"审核图纸","89油管热处理","2022-11-26"]
[5,5702000061,"控制阀组件","18Q00602.02.05.01","装配件;10.7kg","件",2,"审核图纸","89油管热处理","2022-11-26"]
[7,5501700003,"堆取料机;斗轮机构轴承座","D223A-11.0","ZG35 孔径50，轴向孔距145，径向孔距530，座低平面与孔中心线夹角5°侧端盖带注油孔M10","件",2,null,"原料工段","2022-11-26"]
[8,7100100089,"减压阀","DR30-1-30/315YM","ISO 4401","只",2,"GB2514-1987","180厂部","2022-11-26"]
[9,7100300398,"气动换向阀","MN1H-5/3G-D-3-C","3-10bar:FESTO","只",4,"FESTO","180厂部","2022-11-26"]
[10,7100100254,"安全阀","A48Y-25-100","压力等级1.3-1.6Mpa；整定压力1.45Mpa，DN100","只",1,"GB/T12243-2005","能源厂部","2022-11-26"]
[11,7502400138,"机床切削液专用混配器","Master Mix M-10","配比浓度0%~20%，流量38升/分，进水口1/2英寸，出水口3/4英寸，水压：2bar~4bar","套",2,"Q/MT 005-2016","管加工厂部","2022-11-26"]
[12,5602600067,"事故割炬","SG-II","图号QGJ-22;L=2400mm","把",4,"GB5108-1985","炼钢厂部","2022-11-26"]
[13,4000300241,"轴承座","HX110(GB/T2563-2007);轴承座材质ZG270-500；","带铜瓦；润滑油口M10*1；","套",10,"审核图纸","管加工厂部","2022-11-26"]
[16,6400500876,"蓝色油墨","LLY-1","适应1.0mm喷枪；适应标准GB/T1723-1993","桶",20,"GB/T1723-1993","180厂部","2022-11-26"]
[17,5712400006,"42100带锯机 右导向爪装配","G42100B-04300-04302",null,"套",2,null,"720厂部","2022-11-26"]
[18,5712400010,"42100带锯机 左导向爪装配","G42100B-04300-04301",null,"套",2,null,"720厂部","2022-11-26"]
[19,5501400007,"烧结;成品仓振动给料机","QZS-80-130F 不带电机；面宽800mm，长1300mm","铆焊","台",4,"JB/T8096-2013","烧结","2022-11-26"]
[20,5300200061,"圆柱齿轮减速机","ZSC50-Ⅲ-1i=33.1",null,"台",1,"JB/T8853-2001","物流中心","2022-11-26"]
[21,5718600026,"MPM管体车床；前卡爪拐臂","M715683；LEVER；","M.P. COLINET s.p.r.l.","件",3,"COLINET国产化","管加工厂部","2022-12-27"]
[22,5603200029,"布袋龙骨","QC-HY1-002-CN-01040001","V350-4400;喷塑复合;2.09kg","件",220,"审核图纸","炼钢厂部","2022-10-15"]
[23,5603200030,"导向锥套","QC-HY1-002-CN-01040003","VZ212;0.09kg","件",200,"审核图纸","炼钢厂部","2022-10-15"]
[24,6000300242,"空-水冷却器","AWLJ5000-350","风机电机功率：两台15KW;换热功率：350KW；最高进水温度：33℃；水量：36m3/h；工作压力：0.4MPa；最高出风温度：40℃；冷却器带风压开关2件，进出风口配有测温装置，进水口有压力表，配有漏水检测装置","台",1,"JB/T 2728.2-2008","340热轧","2022-11-27"]
[25,7001500003,"罗茨真空泵","DDR40000（2030144）","极限压力0.03Pa;抽速40000m3/h;转速Max3600r/min;功率37Kw;带电机","台",1,"Q/SOEU17-2007","炼钢厂部","2022-11-27"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2022年9月机械配件采购项目Ⅱ                项目编号：HGCGD22127"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":4,"n_cols":1,"rows_kept":4,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,8],[3,0,3,8]],"flags":["formulas_cached_only"]}
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]