{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":30,"n_cols":13,"rows_kept":30,"merged":[[0,0,0,8],[1,0,1,12],[26,0,26,8],[27,0,27,8],[28,0,28,8],[29,0,29,8]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2022年11月机械备件采购项目Ⅱ                     项目编号：HGCGD22139"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,5501700003,"堆取料机;斗轮机构轴承座","D223A-11.0","ZG35 孔径50，轴向孔距145，径向孔距530，座低平面与孔中心线夹角5°侧端盖带注油孔M10","件",2,null,"原料工段","2023-01-26"]
[2,5400300008,"煤气冷凝水排水器","SDLT-4000-100","Q235 GB6222","台",2,"GB6222","高辅工段","2023-01-26"]
[3,5501400007,"烧结;成品仓振动给料机","QZS-80-130F 不带电机；面宽800mm，长1300mm","铆焊","台",4,"JB/T8096-2013","烧结","2023-01-26"]
[4,7502400138,"机床切削液专用混配器","Master Mix M-10","配比浓度0%~20%，流量38升/分，进水口1/2英寸，出水口3/4英寸，水压：2bar~4bar","套",2,"Q/MT 005-2016","管加工厂部","2023-01-26"]
[5,5602600067,"事故割炬","SG-II","图号QGJ-22;L=2400mm","把",4,"GB5108-1985","炼钢厂部","2023-01-26"]
[6,4000300241,"轴承座","HX110(GB/T2563-2007);轴承座材质ZG270-500；","带铜瓦；润滑油口M10*1；","套",10,"审核图纸","管加工厂部","2023-01-26"]
[7,5501100052,"智能振打装置","ZGD1500","电压380~220V,电流2.2A,频率50HZ,振动力15KN,重量153kg，安装尺寸长600*宽350*高550","套",6,"JB/T1038.3-2016","烧结","2023-01-26"]
[8,7502400141,"加药搅拌轴及叶轮","750-32","搅拌轴：304不锈钢材质，直径32mm,长度：1200mm，实心；三叶叶轮：不锈钢材质，内孔Φ32mm，外直径Φ750mm，厚度6mm","套",2,null,"340热轧","2023-01-26"]
[9,6600300111,"空气过滤减压阀","YT-200B","出口气压2-8公斤可调","只",5,null,"340热轧","2023-01-26"]
[10,5719700002,"PP袋式污水过滤袋","180*810-150微米--2号；","过滤精度：150μm；过滤面积：0.5㎡；最大流量：40m3/h ；袋口固定环：镀锌钢圈","只",50,"GB12625-1990","管加工厂部","2023-01-26"]
[11,7102600084,"电动调节阀","RXDF-1v","公称压力：1.6MPa，通径50mm，阀体材质：ZG230-450,滤芯材质OCr 18Ni 9,带配套电动执行机构","台",1,"TS-2743018-2022","能源厂部","2023-01-26"]
[12,5501200134,"柔性翻板式新型双层卸灰装置","JYXF300×1800","\"驱动方式：下阀板分别由单个独立液压缸驱动；液压站（含滤油器+缓冲装置）：电机功率：2.2KW   厂家：节能高效电机\n油泵：康百世齿轮泵   ；密封件材质：橡胶软密封（耐温200℃）；工作压力：16Kpa～20Kpa；物料堆重比：2.2t/m3；漏风率：≤0.05%\"","套",2,"审核图纸","烧结","2023-01-26"]
[13,7001200343,"高压泵连杆","3D-250-0102",null,"根",4,null,"219厂部","2023-01-26"]
[14,5700800113,"铁屑运输链","0.0341-536 国产化","0.0341-536 国产化","套",1,"审核图纸","89热轧","2023-01-26"]
[15,5701600053,"预热式烧嘴换热器","SINMAX2M/C545","60kW","只",3,null,"89厂部","2023-01-26"]
[16,5701600056,"预热式烧嘴陶瓷燃烧室","SINMAX2M/C545",null,"只",4,"GB/T21944.4-2009","89厂部","2023-01-26"]
[17,5701600036,"燃气式高温陶瓷管二","*","L=200mm","根",4,null,"89厂部","2023-01-26"]
[18,5701600038,"燃气式高温陶瓷管三","*","L=300mm","根",24,null,"89厂部","2023-01-26"]
[19,5500300029,"上下调整拉杆","KD300","锻钢调质 炉前泥炮KD300 上下调整拉杆，45# 锻造，调质处理，带销轴，带干油嘴","件",1,null,"高炉","2023-01-26"]
[20,5603200033,"布袋","D120*4402","纤维;玄武岩/PI;克重>750g/m2;厚度1.2mm;透气量6m3/m2/min@12.5mmH20;后处理;PTFE乳液浸渍处理","条",166,"GB12625-1990","炼钢厂部","2023-01-26"]
[21,7502300060,"气水雾化喷嘴","HPZ2.8-75QZ2","材质:黄铜；喷射角75°","只",100,"J11Q20961R3M","炼钢厂部","2023-01-26"]
[22,5300300863,"GK1C机车：柴油机喷油器压装圆垫","外φ35 ,内孔φ20*8","6240ZB,材质45#钢","片",30,"GB/T18655-2010","物流中心","2023-01-26"]
[23,5707900001,"半自动卧式带锯机","G4240/50",null,"台",2,"GB/16454-2008","180厂部","2023-01-26"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2022年11月机械备件采购项目Ⅱ            项目编号：HGCGD22139"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":4,"n_cols":1,"rows_kept":4,"merged":[[0,0,0,8],[1,0,1,8],[2,0,2,8],[3,0,3,8]],"flags":["formulas_cached_only"]}
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]