{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":29,"n_cols":12,"rows_kept":29,"merged":[[0,0,0,10],[1,0,1,10],[25,0,25,10],[26,0,26,10],[27,0,27,10],[28,0,28,10]],"flags":["formulas_cached_only"]}
["    （一）开标一览表"]
["项目名称：2023年5月刀具等备件年度招标项目                           项目编号：HGJY-G2023068"]
["序号","资材编号","资材名称","规格型号","技术参数","单位","年需求量约","使用部门","交货时间","含税单价\n(元）","生产厂家或\n品牌","备注"]
[1,5712200293,"CNC刀片","RCGL190700-LAS20020","直径16.5mm 厚度6mm","片",500,"340热轧","按合同要求交货"]
[2,4201000243,"毛刺机刀具,","TSL1230,硬质合金锥形圆头，","头径 12mm，头长30mm，柄径6mm，全长75mm，齿形 双切齿,齿数20.","根",1000,"180厂部","按合同要求交货"]
[3,4201000223,"C1600车床配套刀片","RCMX25 07 00 4205",null,"片",250,"340热轧","按合同要求交货"]
[4,8700500069,"刀头连接器 进口KM","刀头连接器 DW-0001 进口KM","原装进口KM材料，其它执行ISO 26623标准","只",3,"340厂部","按合同要求交货"]
[5,8700500065,"偏扣粗车刀头 进口KM材料","偏扣粗车刀头 TT90002 进口KM材料","原装进口KM材料，其它执行ISO 26623标准","只",4,"340厂部","按合同要求交货"]
[6,8700500064,"偏扣精车刀头 进口KM材料","偏扣精车刀头 TT90001 进口KM材料","原装进口KM材料，其它执行ISO 26623标准","只",3,"340厂部","按合同要求交货"]
[7,8700500067,"圆扣粗车刀头 进口KM材料","圆扣粗车刀头 TT90004 进口KM材料","原装进口KM材料，其它执行ISO 26623标准","只",2,"340厂部","按合同要求交货"]
[8,8700500066,"圆扣精车刀头 进口KM材料","圆扣精车刀头 TT90003 进口KM材料","原装进口KM材料，其它执行ISO 26623标准","只",2,"340厂部","按合同要求交货"]
[9,5700700455,"卡刀体(刀杆)","0107067-10.400.08、组合件φ80-95mm","VALENITE-D-03.94C097B-A2-0141、C097A-A2-0225、C042Z-A1-0418、WDφ80-95mm 42CrMo：24.6Kg","套",2,"89热轧","按合同要求交货"]
[10,7102900170,"冲压弯头","直径φ530*壁厚10","90度;20#钢","只",54,"炼钢厂部","按合同要求交货"]
[11,6400500841,"碳刷","板簧和碳H742003","H742039  BH DS","个",50,"340厂部","按合同要求交货"]
[12,7501100275,"快速接头","10P1BM27*1.5/10S2BM27*1.5",null,"只",530,"炼钢厂部","按合同要求交货"]
[13,7200700016,"液压马达","OMT400 输出轴∮40,长82,E=1/2\" DEFOSS",null,"台",8,"720厂部","按合同要求交货"]
[14,7500500220,"反渗透膜","UL22-8040","介质：水；耐酸耐碱、耐高压","根",15,"能源厂部","按合同要求交货"]
[15,4301000045,"正力单螺杆压缩机专用机油","型号：GN-D60","20升/桶","桶",100,"能源厂部","按合同要求交货"]
[16,4301000035,"螺杆空压机高级冷却液(复盛螺杆压缩机专用）","20L",null,"桶",115,"能源厂部","按合同要求交货"]
[17,4301000026,"Ingersoll Rand;Uitra EL超级冷却剂","No.2406124;","15L/桶;倾点-39℃;闪点230℃;粘度指数;46;使用寿命大于16000h；GB 5904-1986","桶",8,"能源厂部","按合同要求交货"]
[18,5500900007,"TRT发电机组前后轴封石墨环","*","石墨 GT60.D","只",18,"高辅工段","按合同要求交货"]
[19,3300200010,"螺纹脂","螺纹脂型号：BEST-O-LIFE 2000，重量：500LB/桶（226.796KG/桶）",null,"桶",8,"340管加工车丝","按合同要求交货"]
[20,3300200003,"螺纹脂","JETLUBE 22.68Kg/桶",null,"桶",50,"340管加工车丝","按合同要求交货"]
[21,3300200004,"螺纹脂","Bestolife 72733 20kg/桶",null,"桶",28,"340管加工车丝","按合同要求交货"]
[22,3300200001,"储存脂","KENDEX 186Kg/桶",null,"桶",4,"340管加工车丝","按合同要求交货"]
["注：1、投标报价含税，税率13% ；                                                                                                                          2、生产厂家要求全称填写准确无误 ；                                                                                                                     3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）；"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2023年5月刀具等备件年度招标项目                  项目编号：HGJY-G2023068"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]