{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":17,"n_cols":13,"rows_kept":17,"merged":[[0,0,0,12],[1,0,1,12],[13,0,13,8],[14,0,14,8],[15,0,15,8],[16,0,16,8]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2023年6月电磁备件采购项目                     项目编号：HGJY-G2023073"]
["标包号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,5800200107,"吸盘链条","10+10T","MW32-150130L/CG吸盘用;1套8根;每根链条由四个∮36链环组成;每根链条长880mm;材质;20Mn2","套",1,"GB 5802-1996","炼钢厂部","2023-07-27"]
[2,4100400039,"电缆卷筒","DF100/20-45/35-8/8","容量100A 8通道 电缆长度20米","台",2,"JT/T806.4-2011","炼钢厂部","2023-07-27"]
[3,5300100525,"吸盘链条","MW5-250200",null,"付",3,"GB54a-1977","炼钢厂部","2023-07-27"]
[4,4100400040,"电缆卷筒","JDF60/V-40-6/6","带YJCV6*10+RVVP6*0.5屏蔽、耐高温180 电缆200米","台",1,"JT/T806.4-2011","炼钢厂部","2023-07-27"]
[5,4100400044,"电缆卷筒","JTA20-25-9-Ⅱ","容量20A 电缆长度25米9通道 外置滑环","台",1,"JT/T806.4-2011","炼钢厂部","2023-07-27"]
[6,6100100099,"整流控制柜变压器","ZSG-40 40KVA 380V+10%/220V","GB/T18494.1-2001 40KVA 输入380V 输出220V","台",1,"JB4315-1986","340热轧","2023-07-27"]
[7,4100400291,"电缆卷筒",62180.02,"最大行程（55+45）m;电缆长度70m;行走速度3-30m/min;最大转堵力矩3000Nm;最大堵转电流25A;配带三相力矩电机YLEJ132-25/6及减速箱;力矩调节控制柜","套",1,"JT/T806.4-2011","炼钢厂部","2023-07-27"]
[8,5300100522,"吸盘链条","20t+20t",null,"条",4,"GB5802-1986","物流中心","2023-07-27"]
[9,5300100936,"电磁吸盘链条","5T+5T；配MW929-14084L/1电磁铁","大环内径：185*90；环径：φ45；小环内径：160*65；环径：φ30；长1M；20Mn2。","条",4,"GB 5802-1996","物流中心","2023-07-27"]
[10,6000400076,"超高温起重电磁吸盘","MW12-165100/G-75-YHM","自重4500kg;电压DC220V;电流45A;通电持续率75%;长*宽*高1650*1000*550;耐高温达650℃以下;最大吸重达32吨","台",2,null,"180热轧","2023-07-27"]
["注：1、投标报价含税，税率13% ；                                                                                                 2、生产厂家要求全称填写准确无误 ；                                                                                        \n3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）；"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2023年6月电磁备件招标采购项目      项目编号：HGJY-G2023073"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}