{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":20,"n_cols":14,"rows_kept":20,"merged":[[0,0,0,13],[1,0,1,13],[3,0,4,0],[3,11,4,11],[5,0,9,0],[5,11,9,11],[10,0,11,0],[10,11,11,11],[12,0,13,0],[12,11,13,11],[14,0,15,0],[14,11,15,11],[16,0,16,8],[17,0,17,8],[18,0,18,8],[19,0,19,8]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2023年7月至2024年6月喷标机备件采购项目                      项目编号：HGJY-G2023099"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","标包总价（元）","生产厂家","备注"]
[1,3300900028,"喷标专用油漆","颜色:白色；16L/件(每件4瓶，4L/瓶)","(ZYG)Special paint for marking machine;；粘度:20±2秒(温度25度-4杯)，附着力:不低于3级。","件",27,"SXMD/JW-PY-01","各分厂","按合同要求交货"]
[null,3300900029,"喷标专用清洗剂","16L/件(每件4瓶，4L/瓶)","(ZYG)Special cleaning agent for spray marking machine；密度:1.40±0.028g/m1(温度15度)；闪点>90度","件",200,"SXMD/JW-PY-0","各分厂","按合同要求交货"]
[2,3301000030,"喷码机清洗剂","DRA5100；1升/瓶 CANEC1308825804","CANEC1308825804","瓶",610,"CANEC1308825804","各分厂","按合同要求交货"]
[null,3301000031,"喷码机油墨","DRA1016-P1升/瓶 CANEC1408426302",null,"瓶",658,"CANEC1408426302","各分厂","按合同要求交货"]
[null,3301000039,"喷码机油墨","DRA1012-TG","1升/瓶","瓶",156,"CANEC1408426302","各分厂","按合同要求交货"]
[null,6300600051,"手持式喷码机;油墨盒;","DRA14BOX","SGS","盒",345,"GB/T29017-2012","各分厂","按合同要求交货"]
[null,6300600052,"手持式喷码机;清洗盒;","DRA51BOX","SGS","盒",65,"GB/T29017-2012","各分厂","按合同要求交货"]
[3,4100900044,"打孔机镀铜碳棒","HGDTB51016","尺寸510*16 单位:mm,长度510mm，直径16mm 额定电流：2000安培 额定电压：80V","支",23000,null,"180厂","按合同要求交货"]
[null,5709600170,"打孔机专用碳棒","DTB-30-520",null,"件",10000,null,"340厂","按合同要求交货"]
[4,7001900024,"喷印机油漆","1件4瓶，1瓶4升。","DMJ-1/P","件",75,null,"各分厂","按合同要求交货"]
[null,7001900025,"油漆清洗剂","1件4瓶，1瓶4升。","DMJ-1/R","件",110,null,"各分厂","按合同要求交货"]
[5,4300200048,"喷标油漆","WMark-NT-1/Y","4L/桶","桶",30,"GB/T6750-2007","各分厂","按合同要求交货"]
[null,4300200049,"清洗剂","WClean-NT-1/Q","4L/桶","桶",50,"GB/T1922-2006","各分厂","按合同要求交货"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误，采购数量以月度实际计划需求为准。"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2023年7月至2024年6月喷标机备件采购项目      \n项目编号：HGJY-G2023099"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}