{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":12,"n_cols":13,"rows_kept":12,"merged":[[0,0,0,12],[1,0,1,12],[8,0,8,8],[9,0,9,8],[10,0,10,8],[11,0,11,8]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2023年7月电磁备件采购项目                     项目编号：HGJY-G2023117"]
["标包号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,6000400006,"电磁吸盘","MW929-165100/G-75 DC200V 46.7A 10.27Kw Kf=2.5 通电持续率:75% 4280Kg","4280Kg","台",2,"JB/T10577-2006","炼钢厂部","2023-09-10"]
[2,6100900059,"无触点停电保持柜","LMOBM-200/20-C-UPS-T","进线AC380，输出直流电压DC220V,采用恒电流控制，输出电流可调,最大220A，停电保持时间20MIN，控制器S7-200,电器元件为Schneider","台",1,"JB/T8680-2008","炼钢厂部","2023-09-26"]
[3,4100400287,"电缆卷筒","JTA250-20-C","工作电压380V;电流;250A;行程;20m","台",2,"JT/T806.4-2011","炼钢厂部","2023-09-26"]
[4,5800200107,"吸盘链条","10+10T","MW32-150130L/CG吸盘用;1套8根;每根链条由四个∮36链环组成;每根链条长880mm;材质;20Mn2","套",1,"GB 5802-1996","炼钢厂部","2023-09-26"]
[5,6000400080,"起重电磁铁","MW32-150130L/CG","DC220V;50A;通电持续率75%;带链条;自重4350Kg","台",2,"GB/T33545-2017","炼钢厂部","2023-09-26"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误\n3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2023年7月电磁备件采购项目       项目编号：HGJY-G2023117"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}