{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":466,"n_cols":11,"rows_kept":466,"merged":[[0,0,0,10],[1,0,1,10],[461,0,461,10],[463,0,463,10],[464,0,464,10],[464,11,464,21],[464,22,464,32],[464,33,464,43],[464,44,464,54],[464,55,464,65],[464,66,464,76],[464,77,464,87],[464,88,464,98],[464,99,464,109],[464,110,464,120],[464,121,464,131],[464,132,464,142],[464,143,464,153],[464,154,464,164],[464,165,464,175],[464,176,464,186],[464,187,464,197],[464,198,464,208],[464,209,464,219],[464,220,464,230],[464,231,464,241],[464,242,464,252],[464,253,464,255],[465,0,465,10],[465,11,465,21],[465,22,465,32],[465,33,465,43],[465,44,465,54],[465,55,465,65],[465,66,465,76],[465,77,465,87],[465,88,465,98],[465,99,465,109],[465,110,465,120],[465,121,465,131],[465,132,465,142],[465,143,465,153],[465,154,465,164],[465,165,465,175],[465,176,465,186],[465,187,465,197],[465,198,465,208],[465,209,465,219],[465,220,465,230],[465,231,465,241],[465,242,465,252],[465,253,465,255]],"flags":["formulas_cached_only"]}
["    （一）开标一览表"]
["项目名称：2023年10月-2024年9月密封年度采购项目                            项目编号：HGJY-G2023161"]
["序号","资材编号","资材名称","规格型号","技术参数","单位","数量","交货时间","使用部门","含税单价(元)","生产厂家\n"]
[1,7001800264,"水泵机械密封","SBS250-370F",null,"套",2,"按合同要求交货","180厂"]
[2,7001800078,"离心水泵 机械密封","KQS N200-N5/334",null,"套",2,"按合同要求交货","180厂"]
[3,7001800026,"水泵机械密封","SBS200-520E/486",null,"套",2,"按合同要求交货","180厂"]
[4,7502400054,"高压泵 密封组","L-YL95.01.02",null,"套",2,"按合同要求交货","180厂"]
[5,7401000005,"液压缸密封","BG-D-K-F80-478度-Y",null,"套",5,"按合同要求交货","180厂"]
[6,7402800011,"液体盘根","BH-8900黑色",null,"Kg",5,"按合同要求交货","180厂"]
[7,7401900175,"反螺旋双层油封","*","140*165*12;氟橡胶","只",5,"按合同要求交货","180厂"]
[8,7401900176,"反螺旋双层油封","*","128*150*15;氟橡胶","只",5,"按合同要求交货","180厂"]
[9,7401900174,"反螺旋双层油封","*","130*155*10;氟橡胶","只",5,"按合同要求交货","180厂"]
[10,7401900209,"油封","AB6315AO","650*720*25","只",5,"按合同要求交货","180厂"]
[11,7402500042,"密封垫圈","?445*?360*3.5/1.5/1.0/0.75","石棉橡胶板","个",10,"按合同要求交货","180厂"]
[12,7401700001,"端盖密封套件","*","HPS30011","套",10,"按合同要求交货","180厂"]
[13,5702400099,"气缸内阀板密封件","HJ-HX22509 HJ-HX22509","直径248*直径255*3.5，配金属石墨垫","只",10,"按合同要求交货","180厂"]
[14,5702400098,"气缸内阀板密封件","HJ-HX22509 HJ-HX22509","直径274*直径291*3.5，配金属石墨垫","只",10,"按合同要求交货","180厂"]
[15,7402300006,"旋转轴轴封","R35 430*480*22 NBR",null,"只",10,"按合同要求交货","180厂"]
[16,7402400001,"碟阀密封","HPS030009",null,"只",10,"按合同要求交货","180厂"]
[17,7402400002,"碟阀密封圈","H0P1-DN80","BNR","只",10,"按合同要求交货","180厂"]
[18,7400900061,"轴用V型组合密封圈","S01-200*230*53.3",null,"只",10,"按合同要求交货","180厂"]
[19,7401500034,"防尘圈","350*366*9.5","可耐压力120MPa；热收缩效应小。","只",10,"按合同要求交货","180厂"]
[20,7402100058,"密封圈","VD200A180*210*14.3/25",null,"只",50,"按合同要求交货","180厂"]
[21,7402600028,"石墨垫片","CPS-316","不锈钢;直径180*125*3.2","片",100,"按合同要求交货","180厂"]
[22,5702800067,"密封圈","Z0219.09.11.05.05","聚四氟乙烯 0.1Kg","件",20,"按合同要求交货","180厂"]
[23,7400700041,"V型组合密封","RVE01001 100*120*40 NB83",null,"只",20,"按合同要求交货","180厂"]
[24,7401900099,"油封","155*180*15 AB4666E0 NBR NOK",null,"只",3,"按合同要求交货","180厂"]
[25,7401900229,"骨架密封闷盖","EC 47*7","氟橡胶","只",8,"按合同要求交货","180厂"]
[26,7401900230,"骨架密封闷盖","EC 52*8","氟橡胶","只",10,"按合同要求交货","180厂"]
[27,7402300003,"唇形密封圈","280*310*15","1、材料：氟橡胶，2、温度：200-270度","只",30,"按合同要求交货","180厂"]
[28,7201200008,"孔用四氟导向带","TD-Ⅱ400*2.5*25",null,"只",3,"按合同要求交货","180厂"]
[29,7400100372,"O型密封圈","Z0247.52.01.02.05","内径525 厚度8.6","只",10,"按合同要求交货","180厂"]
[30,7401100003,"导向环","SB250*255*14.8",null,"只",2,"按合同要求交货","180厂"]
[31,7401100004,"导向环","KB580*575*24.5",null,"只",2,"按合同要求交货","180厂"]
[32,7401100012,"导向环","SB340*345*24.5",null,"只",2,"按合同要求交货","180厂"]
[33,7401100018,"活塞导向环","160*155*9.6   B+S",null,"只",3,"按合同要求交货","180厂"]
[34,7401300037,"密封圈","OMS-MR340*364*7.6",null,"只",2,"按合同要求交货","180厂"]
[35,7401500031,"防尘圈","P6/250*270*18",null,"只",2,"按合同要求交货","180厂"]
[36,7401500049,"防尘圈","P6/340*360*18",null,"只",2,"按合同要求交货","180厂"]
[37,7402500014,"密封圈","OMS-MR250*270.5*7.6",null,"只",2,"按合同要求交货","180厂"]
[38,7400400001,"格莱圈","PG01800 180*159.0*8.1",null,"只",10,"按合同要求交货","180厂"]
[39,7401500030,"防尘圈","120*132.2*8.1 HNBR",null,"只",10,"按合同要求交货","180厂"]
[40,7402700059,"316不锈钢高温专用垫片","DN250;245/321","耐温>500℃","片",8,"按合同要求交货","180厂"]
[41,7402900033,"水密封","VING V-550A1521-2",null,"只",10,"按合同要求交货","180厂"]
[42,7402900058,"耐磨环","350*355*25;(技术要求：材料酚醛夹布)","材料酚醛夹布","只",6,"按合同要求交货","180厂"]
[43,5702800069,"密封套件","Z0745.05.02.03.05",null,"套",40,"按合同要求交货","180厂"]
[44,7400100285,"O型密封圈","直径530*3 NBR",null,"只",5,"按合同要求交货","180厂"]
[45,7402100054,"密封圈","HJC01-220-700",null,"只",8,"按合同要求交货","180厂"]
[46,7402500043,"密封垫圈","0109030-23.535","软木橡胶","个",200,"按合同要求交货","180厂"]
[47,7402600050,"石墨垫片","CPS-316;","不锈钢;410*350*3.2","片",20,"按合同要求交货","180厂"]
[48,7401900137,"油封","300*340*16","BAUSLX7;NBR","个",20,"按合同要求交货","219厂"]
[49,5716600016,"骨架油封","*","430*480*25 NBR","只",10,"按合同要求交货","219厂"]
[50,7400500029,"组合垫圈","d90 PTFE",null,"只",3,"按合同要求交货","219厂"]
[51,7400600070,"活塞密封","UPI;100*125*15;NOK","NBR","只",10,"按合同要求交货","219厂"]
[52,7400700017,"V型组合密封","CPS-V89-56*71*22.5",null,"只",50,"按合同要求交货","219厂"]
[53,7400700071,"V型密封圈","PVEO5500  550*590*80","NB83;夹布V组","套",1,"按合同要求交货","219厂"]
[54,7400800051,"高压泵;挺杆密封","Yx70","内径70","只",15,"按合同要求交货","219厂"]
[55,7400900085,"活塞杆密封","AIG526B;90*105*22","A203+A100+A203，原厂家艾志","套",20,"按合同要求交货","219厂"]
[56,7401500075,"防尘圈",";WS00800;80.0*88.8*6.0*81.5*3.0;ZP983;N751/F740","ZP983;N751/F740","只",3,"按合同要求交货","219厂"]
[57,7401500076,"防尘圈","防尘圈;WS01600;160*168.8*6.0*161.5*3.0;ZP983;N751/F740","ZP983;N751/F740","只",3,"按合同要求交货","219厂"]
[58,7401900054,"骨架油封","FB320*360*20 NBR",null,"只",10,"按合同要求交货","219厂"]
[59,7401900132,"油封","240*270*15;","BAUMSLX7;NBR","个",40,"按合同要求交货","219厂"]
[60,7402600012,"石墨垫片","直径360*300*3.2","不锈钢 GB/T9877-2008","片",2,"按合同要求交货","219厂"]
[61,7402600017,"石墨垫片","CPS-316;直径84*40*3","不锈钢;直径84*40*3","片",40,"按合同要求交货","219厂"]
[62,7402600026,"石墨垫片","CPS-316","CPS-316;不锈钢;直径100*50*3","片",20,"按合同要求交货","219厂"]
[63,7402600040,"石墨垫片","CPS-316","不锈钢 直径56*20*3","片",20,"按合同要求交货","219厂"]
[64,5400300025,"煤气增压机 前端油封","AII850(M)型；NO.5101-01","锻件 材质：铝","付",1,"按合同要求交货","340厂"]
[65,7401900159,"油封","380*440*25 NOK AB5888A0",null,"只",2,"按合同要求交货","340厂"]
[66,7402900059,"BSB型基础密封","HOP-PE32-36767;U203","替换原O型圈尺寸为367.67*7","只",2,"按合同要求交货","340厂"]
[67,7400900078,"鼓型基础密封圈","BHT-P200-005400","抗高温水解聚氨脂;直径540","只",2,"按合同要求交货","340厂"]
[68,5712200111,"机械密封","0109015-25.115","1.组合件配合良好 2.满足生产要求","套",3,"按合同要求交货","340厂"]
[69,7401500063,"防尘圈","ES56153-2500-46-377-8307;250*266*9.5","250*266*9.5","只",5,"按合同要求交货","340厂"]
[70,7402700074,"金属包覆垫片","直径1380*直径1310*8","304/石墨橡胶+石墨 耐高温≤300℃","片",5,"按合同要求交货","340厂"]
[71,7401900156,"油封","270*330*25  AB5523AO",null,"只",5,"按合同要求交货","340厂"]
[72,7401300022,"活塞密封","DMK-MR660*635.5*7.7 24275495",null,"只",5,"按合同要求交货","340厂"]
[73,7402800021,"四角芳纶盘根","2302","增强PTFE;10*11","Kg",5,"按合同要求交货","340厂"]
[74,7401900202,"密封圈","GMAY-110*140*12-N10175","FPM/高温复合材料","只",5,"按合同要求交货","340厂"]
[75,7401900117,"骨架油封","CPS511-620*670*22",null,"个",5,"按合同要求交货","340厂"]
[76,7401900107,"螺旋剖分油封","AIGI522S 170*200*15 重载型",null,"只",5,"按合同要求交货","340厂"]
[77,7402900023,"BSB基础密封","HOP-PE42-3500","U203","只",5,"按合同要求交货","340厂"]
[78,7401900102,"双剖分油封","AIG5505H 300*340*18 A100+A203",null,"只",5,"按合同要求交货","340厂"]
[79,7402900022,"BSB型基础密封","HOP-PE32-49000","U203含胶粘剂","只",5,"按合同要求交货","340厂"]
[80,7402700040,"金属包履垫片","CSCL","DN200","只",10,"按合同要求交货","340厂"]
[81,7402700043,"316不锈钢高温专用垫片","DN500","530/622 耐温>500℃","片",10,"按合同要求交货","340厂"]
[82,7402900043,"耐高温专用密封","FB80*100*12","JN5050 CSCL","只",10,"按合同要求交货","340厂"]
[83,7402800004,"盘根","CPS7600 12*12mm",null,"Kg",10,"按合同要求交货","340厂"]
[84,5712300145,"烧嘴挡火圈","*","288*110*60","只",10,"按合同要求交货","340厂"]
[85,5712300121,"煤气管道金属硬密封垫圈","*",null,"只",10,"按合同要求交货","340厂"]
[86,7400700047,"活塞密封","RVE02000;200*220*40.0*6;NB83",null,"套",10,"按合同要求交货","340厂"]
[87,7402700075,"316不锈钢高温专用垫片","DN700;720/846;耐温>500℃",null,"片",10,"按合同要求交货","340厂"]
[88,5712300164,"步进炉加热段烧嘴密封垫","*","耐温500℃","只",10,"按合同要求交货","340厂"]
[89,5712300020,"侧烧嘴与炉墙密封垫","5mm 620*565*475 φ24孔均布12个",null,"片",10,"按合同要求交货","340厂"]
[90,7401900177,"骨架油封","0109015-24.125","470*420*22","只",10,"按合同要求交货","340厂"]
[91,5717100009,"导向环","24315102","KB660*652*25","只",10,"按合同要求交货","340厂"]
[92,7402400004,"蝶阀特制密封圈","DN65","直径64*直径101.5*50 E704","只",10,"按合同要求交货","340厂"]
[93,7402400003,"蝶阀特制密封圈","DN100","直径97.8*直径137.5*56 E704","只",10,"按合同要求交货","340厂"]
[94,7402700076,"金属缠绕式垫片","φ1030*φ1090*8；不锈钢 耐温1200度","不锈钢 GB/T4622.2-2003","片",10,"按合同要求交货","340厂"]
[95,7401400031,"活塞杆密封","OMK-MR580*555.5*7.7",null,"只",10,"按合同要求交货","340厂"]
[96,7401900203,"密封圈","GMAY-120*150*12-N10175","FPM/高温复合材料","只",10,"按合同要求交货","340厂"]
[97,5712200110,"机械密封","0109015-24.115","1.组合件配合良好 2.满足生产要求","套",20,"按合同要求交货","340厂"]
[98,7401300020,"活塞密封","TPM248185-63*47*18.3*6.4 NBR",null,"只",50,"按合同要求交货","340厂"]
[99,7402800006,"盘根成型环","45度切口 CPS7600 65*79.2*6.5-6.9",null,"只",100,"按合同要求交货","340厂"]
[100,5712300018,"侧烧嘴密封件","*","390*110*2","只",15,"按合同要求交货","340厂"]
[101,7402500065,"缠绕式密封垫圈","325*250*3.5","基本型","只",10,"按合同要求交货","340厂"]
[102,7402600011,"石墨垫片","直径275*200*3.2","不锈钢 GB/T9877-2008","片",10,"按合同要求交货","340厂"]
[103,7001200132,"盘根成型环","CPS7600 75*95*10","45度切口  材料：芳纶角线黑四氟盘根","只",150,"按合同要求交货","340厂"]
[104,7400600069,"U形圈","53*61*4.5","聚氨酯","只",60,"按合同要求交货","340厂"]
[105,5712300021,"缠绕式密封垫圈","*","106*63*3.2","只",20,"按合同要求交货","340厂"]
[106,5712300221,"步进炉加热段烧嘴内密封垫","直径225*268*305*3.2","8孔20均布;耐温500℃","个",20,"按合同要求交货","340厂"]
[107,7001200246,"五柱塞往复泵;填料环甲","5XND-315-0211-D",null,"个",10,"按合同要求交货","340厂"]
[108,7001200271,"五柱塞往复泵;填料环乙","5XND-315-0212-D","材质黄铜；重量0.1Kg","只",10,"按合同要求交货","340厂"]
[109,7402800005,"盘根成型环","45度切口 CPS7600 50*66*7",null,"只",100,"按合同要求交货","340厂"]
[110,7502000180,"高压泵;柱塞填料","3D6.5-32/20.0-IA;","浸油石棉聚四氟乙烯12.5*12.5；","Kg",10,"按合同要求交货","340厂"]
[111,5709900116,"骨架油封","FB220*260*18","1、材料：氟橡胶，2、温度：200-270度","只",1,"按合同要求交货","340厂"]
[112,5710200181,"密封套件","*","Z0650114","件",5,"按合同要求交货","340厂"]
[113,5710600211,"骨架油封","280*316*18;AC5558E1",null,"个",2,"按合同要求交货","340厂"]
[114,5711100103,"步进炉加热段烧嘴内密封垫","直径155*192*235*3.2;8孔φ20均布","耐温500℃","只",10,"按合同要求交货","340厂"]
[115,5711100104,"步进炉加热段烧嘴密封垫","直径285*305*325*3.2;8孔φ20均布","耐温500℃","只",10,"按合同要求交货","340厂"]
[116,7400100140,"O型密封圈","直径545*7.00G  NBR",null,"只",6,"按合同要求交货","340厂"]
[117,7400700002,"V型密封圈","57*77*4/7 FKM",null,"只",25,"按合同要求交货","340厂"]
[118,7400700003,"V型密封圈","57*77*4/7 PTFE",null,"只",25,"按合同要求交货","340厂"]
[119,7400700037,"V型组合密封","PVE01000 100*80*99*21.2 NB83",null,"只",15,"按合同要求交货","340厂"]
[120,7401000001,"小舱密封","B+S之55013Merkel之OMS-MR","B74422改 直径360*直径376*11","只",14,"按合同要求交货","340厂"]
[121,7401000002,"小舱密封","B+S之55013Merkel之OMS-MR","B74505改 直径270*直径286*11","只",7,"按合同要求交货","340厂"]
[122,7401400023,"活塞杆密封","USH00700+挡圈 70*80*79*7 N901",null,"只",15,"按合同要求交货","340厂"]
[123,7401400024,"活塞杆密封","USH00550+挡圈 55*65*64*7 N901",null,"套",15,"按合同要求交货","340厂"]
[124,7401500041,"防尘圈","VD320A NBR510",null,"个",120,"按合同要求交货","340厂"]
[125,7401500061,"防尘圈","0109015-21.122;","198*228*25;NBR","只",4,"按合同要求交货","340厂"]
[126,7401900035,"骨架油封","95*170*12/13 FKM",null,"只",5,"按合同要求交货","340厂"]
[127,7401900084,"骨架油封","270*310*18 NBR",null,"只",25,"按合同要求交货","340厂"]
[128,7401900088,"骨架油封","DIN3760-A63*85*10 FPM",null,"只",20,"按合同要求交货","340厂"]
[129,7401900105,"骨架油封","CPS511 280*320*20/14 FKM",null,"只",7,"按合同要求交货","340厂"]
[130,7401900149,"骨架油封","460*520*25","AB6079A0 NOK","只",2,"按合同要求交货","340厂"]
[131,7401900153,"内包骨架油封","240*280*15","CPS511","只",10,"按合同要求交货","340厂"]
[132,7401900182,"骨架油封","FB175*215*16B2U;23397;NBR",null,"个",5,"按合同要求交货","340厂"]
[133,7401900188,"骨架油封","FB280*320*20",null,"件",4,"按合同要求交货","340厂"]
[134,7401900189,"骨架油封","FB250*280*15;NBR;478708;GB13871-1992","GB13871-1992","个",3,"按合同要求交货","340厂"]
[135,7401900190,"骨架油封","FB175*215*16B2U;23397;NBR","NBR;GB13781-1992","个",20,"按合同要求交货","340厂"]
[136,7401900205,"骨架油封","0106008-10.463","215*240*12;NBR","只",110,"按合同要求交货","340厂"]
[137,7401900217,"油封","CPS511","650*710*25","只",1,"按合同要求交货","340厂"]
[138,7401900250,"氟胶TC骨架油封","145*180*12","氟胶","个",15,"按合同要求交货","340厂"]
[139,7402200023,"U型密封圈","U11-140*160*10",null,"只",5,"按合同要求交货","340厂"]
[140,7402300013,"辰型密封圈","FB240*270*15;NBR;GB9877.1-88","FB240*270*15;NBR","只",40,"按合同要求交货","340厂"]
[141,7402600052,"石墨垫片","CPS-316","不锈钢;429*355*6.0","片",5,"按合同要求交货","340厂"]
[142,7402800023,"盘根","AIG26V;12mm",null,"个",15,"按合同要求交货","340厂"]
[143,7402000044,"机械密封","CPS-MTN90","直径90mm","只",2,"按合同要求交货","720厂"]
[144,7400900069,"活塞杆密封","RVE00900","90*105*22.5*5;NB83","套",20,"按合同要求交货","720厂"]
[145,5714400016,"弹性元件Ⅰ","*","橡胶 19.65Kg","件",30,"按合同要求交货","720厂"]
[146,5714400017,"弹性元件Ⅱ","*","橡胶 19.65Kg","件",20,"按合同要求交货","720厂"]
[147,7400100139,"O型密封圈","直径515*7.00G  NBR",null,"只",5,"按合同要求交货","720厂"]
[148,7400100141,"O型密封圈","直径615*7.00G  NBR",null,"只",5,"按合同要求交货","720厂"]
[149,7400100142,"O型密封圈","直径630*7.00G  NBR",null,"只",5,"按合同要求交货","720厂"]
[150,7400100315,"O型密封圈","直径608.7*7.0G",null,"只",2,"按合同要求交货","720厂"]
[151,7400100316,"O型密封圈","直径718.7*7.0G",null,"只",2,"按合同要求交货","720厂"]
[152,7400100572,"O型密封圈","直径740*8.4","NBR","只",10,"按合同要求交货","720厂"]
[153,7400100573,"O型密封圈","直径715*8.4","NBR","只",10,"按合同要求交货","720厂"]
[154,7400200022,"孔用挡圈","直径210","直径210","件",5,"按合同要求交货","720厂"]
[155,7400300014,"斯特封","RS01400 140*155.5*6.3",null,"只",5,"按合同要求交货","720厂"]
[156,7400400003,"格莱圈","PG01400 140*119*8.1 ZP983/N751/F740",null,"只",15,"按合同要求交货","720厂"]
[157,7400400018,"格莱圈","PG02000 200*179*8.1",null,"只",5,"按合同要求交货","720厂"]
[158,7400400019,"格莱圈","PG02200 220*199*8.1",null,"只",5,"按合同要求交货","720厂"]
[159,7400400020,"格莱圈","PG02600 260*239*8.1",null,"只",5,"按合同要求交货","720厂"]
[160,7400700028,"V型组合密封","PVE01800 180*200*40 NB83",null,"只",5,"按合同要求交货","720厂"]
[161,7400700065,"密封圈","VD630A",null,"只",2,"按合同要求交货","720厂"]
[162,7401200003,"支撑环","600*605*10;厚度2.5mm",null,"只",3,"按合同要求交货","720厂"]
[163,7401200004,"支撑环","360*368*25;厚度5mm",null,"只",100,"按合同要求交货","720厂"]
[164,7401200005,"支撑环","600*610*20;厚度5mm",null,"只",18,"按合同要求交货","720厂"]
[165,7401400002,"活塞杆密封","RS01600 160*175.5*6.3",null,"只",5,"按合同要求交货","720厂"]
[166,7401400010,"密封","d200","RS02000 CB00704","只",4,"按合同要求交货","720厂"]
[167,7401400011,"密封","d200","RVE02001 BD44448","只",2,"按合同要求交货","720厂"]
[168,7401400032,"活塞杆密封","OMS-MR-360-384-7.6;","24214095;Simrit","只",40,"按合同要求交货","720厂"]
[169,7401400033,"活塞杆密封","OMS-MR-600-635-16.4;","24299600;Simrit","只",40,"按合同要求交货","720厂"]
[170,7401500035,"防尘圈","360*376*9.5;BUSAK",null,"只",20,"按合同要求交货","720厂"]
[171,7401900057,"骨架油封","360*300*25 NBR",null,"只",25,"按合同要求交货","720厂"]
[172,7401900138,"内骨架油封","*","358*320*20","只",10,"按合同要求交货","720厂"]
[173,7401900208,"油封","AC5461E6","SC260*300*20","件",15,"按合同要求交货","720厂"]
[174,7401900236,"油封（二）","02690045DR5005ME005-29","02690045DR5005ME005-29；80NBR B241;500*550*22；0.03Kg","件",5,"按合同要求交货","720厂"]
[175,7401900237,"油封（三）","02690045DR5005ME005-33","02690045DR5005ME005-33；80NBR B241;467*510*25；0.02Kg","件",5,"按合同要求交货","720厂"]
[176,7402600027,"石墨垫片","CPS-316","不锈钢;直径503*400*3","片",20,"按合同要求交货","720厂"]
[177,7402500055,"密封圈","HJC03-400-700",null,"只",1,"按合同要求交货","89厂"]
[178,7001200217,"高压泵 密封组","A-25/2.01.01.02","直径80mm","套",1,"按合同要求交货","89厂"]
[179,7402500034,"电动盲板阀密封","F943X-1.6C","DN600","个",2,"按合同要求交货","89厂"]
[180,7400900075,"组合密封","SGKD34125000+SFA52125004","D125;HUNGER","套",5,"按合同要求交货","89厂"]
[181,7402500033,"眼镜阀;密封圈","HJN0901-2J-16","硅橡胶","个",5,"按合同要求交货","89厂"]
[182,7400900072,"组合密封","SGKD34063000+SFA52063004;","D63;HUNGER","套",10,"按合同要求交货","89厂"]
[183,7402800029,"高压泵盘根组","AIGI15","55*71*30","套",10,"按合同要求交货","89厂"]
[184,7401000007,"液压缸密封","HY89G19-234E","氟橡胶","套",10,"按合同要求交货","89厂"]
[185,7401900139,"J型油封","390*430*20","HG4-338-1966","只",20,"按合同要求交货","89厂"]
[186,7401100007,"导向带","WG30  DIN53454","ZP983","米",20,"按合同要求交货","89厂"]
[187,7401900258,"BHT型特殊油封","9.82\"*11.05\"*0.6\"   VITON复合材料  DIN3760",null,"只",20,"按合同要求交货","89厂"]
[188,7402700050,"缠绕式密封垫圈","118*65*3.2","118*65*3.2","个",100,"按合同要求交货","89厂"]
[189,5701000012,"密封","进口","RDR240 61*5.33","只",10,"按合同要求交货","89厂"]
[190,5701000013,"密封","进口","RDR158 12*5.33","只",10,"按合同要求交货","89厂"]
[191,7401900223,"骨架油封","190*220*12","*","个",10,"按合同要求交货","89厂"]
[192,7402900056,"180旋转头密封圈","内径290，线径7","氟硅橡胶","只",25,"按合同要求交货","89厂"]
[193,7400300003,"活塞杆密封","OMS-MR56/66.7/4.2 NBR",null,"只",15,"按合同要求交货","89厂"]
[194,7400700011,"V型组合密封","CPS-V89-100*80*21.2",null,"只",35,"按合同要求交货","89厂"]
[195,7400700018,"V型组合密封","CPS-V89-70*85*22.5",null,"只",25,"按合同要求交货","89厂"]
[196,7400700034,"V型组合密封","PVE01600 160*130*158.5*29 NB83",null,"只",12,"按合同要求交货","89厂"]
[197,7400700059,"V型组合密封(活塞用)","CPS-V89-125*100*25.8",null,"只",20,"按合同要求交货","89厂"]
[198,7400700060,"V型组合密封(活塞用)","CPS-V89-140*115*25.8","GB/T9877-2008","只",30,"按合同要求交货","89厂"]
[199,7400700061,"V型组合密封","CPS-V89-36*48*22.5","36*48*22.5","只",10,"按合同要求交货","89厂"]
[200,7400900084,"活塞密封","AIG526B;100*125*25","A203+A100+A203，原厂家艾志","套",25,"按合同要求交货","89厂"]
[201,7401300025,"活塞密封","RVE001000","NB83;100*115*30.0*5","套",12,"按合同要求交货","89厂"]
[202,7401300031,"活塞密封","APR1063048009",null,"只",5,"按合同要求交货","89厂"]
[203,7401500071,"防尘圈","027160H8000P","橡胶","只",6,"按合同要求交货","89厂"]
[204,7401500072,"防尘圈","027161H9000P","橡胶","只",4,"按合同要求交货","89厂"]
[205,7401700005,"轧机稀油站螺杆泵油封","AP2668G","TCN45*68*12","个",5,"按合同要求交货","89厂"]
[206,7401900146,"骨架油封","250*280*15","478708 NBR","只",150,"按合同要求交货","89厂"]
[207,7401900226,"骨架油封","270*310*18","氟橡胶;耐高温≥500℃","只",15,"按合同要求交货","89厂"]
[208,7401900241,"骨架油封","240*270*15","NBR","件",5,"按合同要求交货","89厂"]
[209,7400100509,"O型密封圈","内径387*7 NBR","NBR 内径387 硬度90","只",5,"按合同要求交货","89厂"]
[210,7400700067,"骨架油封","450*490*67.5;CARCO;TEX/UN;橡胶I-4","450*490*67.5","套",1,"按合同要求交货","89厂"]
[211,7400700068,"骨架油封","380*420*67.5;CARCO;TEX/UN;橡胶I-4","380*420*67.5","套",1,"按合同要求交货","89厂"]
[212,7402600037,"石墨垫片","CPS-316","不锈钢 直径275*200*3.2","片",30,"按合同要求交货","89厂"]
[213,7402600013,"316不锈钢石墨垫片","直径80*125*3","316不锈钢 耐温250℃，GB/T9877-2008","片",10,"按合同要求交货","89厂"]
[214,7402600043,"石墨垫片","CPS-316","不锈钢 直径135*80*3.2","片",50,"按合同要求交货","89厂"]
[215,6700300030,"高压增压泵;密封圈",28426,"Gas booster Haskel 14AGT-125-315-29125 Serial 4762643-1 Air Cycling Valve Seal Kit.","套",2,"按合同要求交货","检验检测中心"]
[216,6700300031,"高压增压泵 密封圈",50881,"Gas booster Haskel 14AGT-125-315-29125 Serial 4762643-1 Air Drive Seal Kit.","套",2,"按合同要求交货","检验检测中心"]
[217,6700300032,"高压增压泵 密封圈","51544-15","Gas booster Haskel AGT-32-62-28881 Serial 0814-2 High Pressure Seal Kit(15 Ratio).","套",1,"按合同要求交货","检验检测中心"]
[218,6700300033,"高压增压泵 密封圈","51544-30","Gas booster Haskel AGT-32-62-28881 Serial 0814-2 High Pressure Seal Kit(30 Ratio).","套",2,"按合同要求交货","检验检测中心"]
[219,6700300060,"高压增压泵密封圈","51545-3;Gas booster Haskel;AGT-32-62-28881;Serial;0814-2;Air Drive seal Kit",null,"套",2,"按合同要求交货","检验检测中心"]
[220,6700300088,"空气阀密封安装包",16771,"Liquid Pump  Haskel ：HSF-202;Air Valve Seal Kit","包",3,"按合同要求交货","检验检测中心"]
[221,6700300089,"液压密封安装包（包括单向阀密封安装包）","51532-302","Liquid Pump, Haskel # HSF-302, Serial # 0614-0075；Hydraulic Seal Kit, includes check valves","包",2,"按合同要求交货","检验检测中心"]
[222,6700300090,"液压密封安装包","51532-202","Liquid Pump, Haskel # HSF-202, Fluid Section Seal Kit","包",1,"按合同要求交货","检验检测中心"]
[223,6700300092,"高压增压泵密封安装包",28349,"Gas booster Haskel;14AGT-125/315-29125, Serial # 4762643-1；High Pressure Seal Kit (125 Ratio)","包",2,"按合同要求交货","检验检测中心"]
[224,7001200261,"高压增压泵密封圈17325","Gas booster Haskel",null,"套",1,"按合同要求交货","检验检测中心"]
[225,7400100587,"O型条","线径φ16.0±0.10mm","材质：NBR70A；黑色；用于外压挤毁试验试样装配用O型圈接驳；KIMBBINS","米",15,"按合同要求交货","检验检测中心"]
[226,7402900067,"高压增压泵密封安装包",51398,"Gas booster Haskel;14AGT-125/315-29125;Serial # 4762643-1;Air Cycling valve Seal Kit","包",3,"按合同要求交货","检验检测中心"]
[227,7402900010,"高温密封填条","*","JN5050 50*15*16.2","根",1,"按合同要求交货","炼钢厂"]
[228,7402900009,"高温密封填条","*","JN5050 12*10*10","根",1,"按合同要求交货","炼钢厂"]
[229,7401900073,"油封","AB6111A0 480*540*25",null,"只",2,"按合同要求交货","炼钢厂"]
[230,7402000039,"机械密封","CPS-MTN55","直径55mm","只",2,"按合同要求交货","炼钢厂"]
[231,7402000043,"水泵机械密封","SLOW300-450(I)",null,"套",2,"按合同要求交货","炼钢厂"]
[232,7402300018,"PQF专用密封圈","279.8×310.4×15.1",null,"只",2,"按合同要求交货","炼钢厂"]
[233,7402300017,"PQF专用密封圈","199.9×230.3×16.1",null,"只",2,"按合同要求交货","炼钢厂"]
[234,7400900091,"（新）一均阀板密封件","QP745Y/Xφ354*φ312*21；材质：硅橡胶；耐温200-300℃；硬度：邵氏65-70；重量：0.15KG",null,"只",2,"按合同要求交货","炼钢厂"]
[235,7401400022,"活塞杆密封","OMS-MR-45*55.7*4.2 PTFE/NBR",null,"只",2,"按合同要求交货","炼钢厂"]
[236,7400100451,"结晶器座密封圈","DN125;B227G35-8;HⅡ744;1.3Kg",null,"只",4,"按合同要求交货","炼钢厂"]
[237,7402900047,"导向带","WRL0150025P",null,"卷",5,"按合同要求交货","炼钢厂"]
[238,7401900211,"骨架油封","640*704*25","80NBR709","只",5,"按合同要求交货","炼钢厂"]
[239,7402300016,"TC双唇内包骨架油封","440*480*20",null,"只",5,"按合同要求交货","炼钢厂"]
[240,7400100480,"炼钢结晶器O型密封圈","直径12.5*951(内径长);硅橡胶",null,"只",10,"按合同要求交货","炼钢厂"]
[241,3221200006,"高温高氧耐磨碳纤布","宽500mm；厚2mm","1200度","米",10,"按合同要求交货","炼钢厂"]
[242,7400100444,"炼钢220结晶器O型密封圈","直径618*12;(内径长)，硅橡胶",null,"只",10,"按合同要求交货","炼钢厂"]
[243,7400100469,"炼钢结晶器O型密封圈","直径6*1813(内径长);硅橡胶",null,"只",10,"按合同要求交货","炼钢厂"]
[244,7400900083,"高压泵盘根组合密封","AIGI871;  60*76*30","3个高油四氟成型密封环、2个聚甲醛支撑环   AIGI","套",10,"按合同要求交货","炼钢厂"]
[245,7400100471,"炼钢结晶器O型密封圈","直径6*2158(内径长);硅橡胶",null,"只",10,"按合同要求交货","炼钢厂"]
[246,7400100479,"炼钢结晶器O型密封圈","直径6*2498(内径长);硅橡胶",null,"只",10,"按合同要求交货","炼钢厂"]
[247,7400100440,"炼钢280结晶器O型密封圈","直径328*10.5(内径长)，硅橡胶",null,"只",10,"按合同要求交货","炼钢厂"]
[248,7400300007,"斯特封","350*374*8.1",null,"只",10,"按合同要求交货","炼钢厂"]
[249,7400100445,"炼钢250结晶器O型密封圈","直径(内径)880*4.7，硅橡胶",null,"只",10,"按合同要求交货","炼钢厂"]
[250,7400900074,"活塞杆密封","140*165*40;","NB83;RVE01401","只",10,"按合同要求交货","炼钢厂"]
[251,7401900074,"油封","AD5994A0 430*480*25",null,"只",10,"按合同要求交货","炼钢厂"]
[252,5701900088,"挡圈 D300","18Q00601.04.01-02聚四氟乙烯,0.1kg",null,"只",10,"按合同要求交货","炼钢厂"]
[253,7402800031,"盘根","AIG26W;8*8","材质AIG26W","Kg",15,"按合同要求交货","炼钢厂"]
[254,7401300013,"活塞密封","PAS01250 125*103*121*26.5*5.1 N842/PN24/P12",null,"只",20,"按合同要求交货","炼钢厂"]
[255,7401900080,"骨架油封","0109015-25.125","364*320*20","只",20,"按合同要求交货","炼钢厂"]
[256,7400700040,"V型组合密封","PVE01800 180*150*32 NB83",null,"只",20,"按合同要求交货","炼钢厂"]
[257,7400700019,"V型组合密封","CPS-V89-90*105*22.5",null,"只",20,"按合同要求交货","炼钢厂"]
[258,7400700032,"V型组合密封","PVE01100 110*125*30 NB83",null,"只",20,"按合同要求交货","炼钢厂"]
[259,7400100377,"炼钢结晶器;O型密封圈","直径9.6*255(内径长)",null,"只",50,"按合同要求交货","炼钢厂"]
[260,7402900002,"O型密封条","*","直径45*15 硅橡胶","Kg",50,"按合同要求交货","炼钢厂"]
[261,7402900007,"高温密封环","*","JN5050 50*5.1","只",100,"按合同要求交货","炼钢厂"]
[262,7401900206,"骨架油封","0106008-10.464","185*210*13;NBR","只",100,"按合同要求交货","炼钢厂"]
[263,7400100448,"炼钢330结晶器O型密封圈","直径384*10.5(内径长)，硅橡胶",null,"只",100,"按合同要求交货","炼钢厂"]
[264,7401300032,"活塞密封","PG01250","125*109.5*6.3 ZP983/N751","只",100,"按合同要求交货","炼钢厂"]
[265,6000300111,"辊道电动机 密封端盖","直径80*9",null,"件",50,"按合同要求交货","炼钢厂"]
[266,7400100453,"结晶器座密封圈","DN40;B227G35-7;HⅡ744;0.7Kg",null,"只",5,"按合同要求交货","炼钢厂"]
[267,7400100528,"炼钢结晶器O型密封圈","（D内)Φ545×Φ5.7，硅橡胶",null,"只",100,"按合同要求交货","炼钢厂"]
[268,7400600020,"U型密封圈","USH02000 200*220*218*13 N901",null,"只",5,"按合同要求交货","炼钢厂"]
[269,7400600065,"炼钢结晶器底座U型内骨架橡胶密封圈","134*108*14.5",null,"只",25,"按合同要求交货","炼钢厂"]
[270,7400600066,"炼钢结晶器试验台密封圈","UN125;氟橡胶",null,"只",15,"按合同要求交货","炼钢厂"]
[271,7400600067,"炼钢结晶器试验台密封圈","UN40;氟橡胶",null,"只",15,"按合同要求交货","炼钢厂"]
[272,7400600071,"炼钢结晶器振动台密封圈","UN65;氟橡胶",null,"只",25,"按合同要求交货","炼钢厂"]
[273,7400700009,"V型组合密封","125*100*25.8","氟橡胶 NB83","只",10,"按合同要求交货","炼钢厂"]
[274,7400700014,"V型组合密封","CPS-V89-80*60*15.2",null,"只",80,"按合同要求交货","炼钢厂"]
[275,7400700023,"V型组合密封","GE3-1400 140*115*25.8",null,"只",10,"按合同要求交货","炼钢厂"]
[276,7400700026,"V型组合密封","PVE00501 50*70*30 NB83",null,"只",7,"按合同要求交货","炼钢厂"]
[277,7400700035,"V型组合密封","PVE02000 200*170*198.5*33.5 NB83",null,"只",22,"按合同要求交货","炼钢厂"]
[278,7400700039,"V型组合密封","PVE01100 110*90*109*21.2 NB83",null,"只",10,"按合同要求交货","炼钢厂"]
[279,7400700042,"V型组合密封","HT1007.1-FPMK674 MERKEL",null,"只",60,"按合同要求交货","炼钢厂"]
[280,7400700043,"V型组合密封","HT1007.2-FPMK674 MERKEL",null,"只",50,"按合同要求交货","炼钢厂"]
[281,7400700048,"V型组合圈","RVE00500","NB83;50*65*22.5","只",45,"按合同要求交货","炼钢厂"]
[282,7400900068,"活塞杆密封","RVE00700","70*85*22.5*5;NB83","套",10,"按合同要求交货","炼钢厂"]
[283,7401400028,"活塞杆密封","USH01000",null,"只",7,"按合同要求交货","炼钢厂"]
[284,7401700002,"主泵轴封","AIGAR202","55*72*7;铝+A830","套",5,"按合同要求交货","炼钢厂"]
[285,7402000028,"水泵机械密封","*","CSCL SLOW100-320A","套",2,"按合同要求交货","炼钢厂"]
[286,7402000030,"中开双吸泵 净环水机械密封","SBS100-310FG/301",null,"套",2,"按合同要求交货","炼钢厂"]
[287,7402000031,"中开双吸泵 浊环水机械密封","SBS100-310EG/325",null,"套",3,"按合同要求交货","炼钢厂"]
[288,7402000048,"离心水泵机械密封","SLOW100-320A","机械密封摩擦副材质;浸渍树脂或金属的石墨","套",2,"按合同要求交货","炼钢厂"]
[289,7402500075,"油封","TX8#","∮102×∮75×14;材质:橡胶","只",10,"按合同要求交货","炼钢厂"]
[290,7402600009,"石墨垫片","CPS-316 不锈钢 直径319*250*3.2 HG20608",null,"片",45,"按合同要求交货","炼钢厂"]
[291,7402600031,"石墨垫片","CPS-316","不锈钢；直径330*250*3.2","片",25,"按合同要求交货","炼钢厂"]
[292,7402600033,"石墨垫片","CPS-316","不锈钢；直径210*150*3.2","片",15,"按合同要求交货","炼钢厂"]
[293,7402600041,"石墨垫片","CPS-316","不锈钢 直径350*320*3","片",13,"按合同要求交货","炼钢厂"]
[294,7402800008,"石墨盘根","12*12","石墨","Kg",120,"按合同要求交货","炼钢厂"]
[295,7402800009,"石墨盘根","18*18","石墨","Kg",5,"按合同要求交货","炼钢厂"]
[296,7402900004,"仓门盖密封条","*","H=25mm B=20mm B=20mm b=6mm 槽宽4mm 槽高15mm","米",400,"按合同要求交货","炼钢厂"]
[297,7402900005,"仓门盖密封条","*","H=25mm B=25mm B=25mm 发泡橡胶","米",500,"按合同要求交货","炼钢厂"]
[298,7402900042,"耐高温专用密封","FB60*90*12","JN5050 CSCL","只",10,"按合同要求交货","炼钢厂"]
[299,3400200001,"无尘石棉布","*","厚3mm","Kg",2000,"按合同要求交货","炼钢厂"]
[300,7402000040,"水泵机械密封","SLOW250-390A",null,"套",1,"按合同要求交货","炼钢厂"]
[301,7402000041,"水泵机械密封","SLOW250-610A",null,"套",1,"按合同要求交货","炼钢厂"]
[302,7402000042,"水泵机械密封","SLOW200-530",null,"套",1,"按合同要求交货","炼钢厂"]
[303,7402700055,"316不锈钢垫片","直径210*直径160*3","耐高温500℃；紫铜；压力2.5MPa 16Kg/cm2","片",20,"按合同要求交货","炼钢厂"]
[304,4000700057,"水洗混纺无尘非石棉编绳","5mm",null,"kg",200,"按合同要求交货","炼钢厂"]
[305,7402000033,"P302冲渣泵;机械密封","100YTZX-500","橡胶","套",1,"按合同要求交货","炼铁厂"]
[306,7402000032,"机械密封","250YTZX-650","橡胶","套",1,"按合同要求交货","炼铁厂"]
[307,7402000025,"离心水泵 机械密封","KQSN600-N27/466",null,"套",1,"按合同要求交货","炼铁厂"]
[308,7402000024,"离心水泵 机械密封","KQSN200-M13/188",null,"套",1,"按合同要求交货","炼铁厂"]
[309,7402000034,"机械密封","MN206-110","150YTZ-560 橡胶","套",1,"按合同要求交货","炼铁厂"]
[310,5500100007,"炉顶放散阀密封件","HJN0901-15D","DN500 氟硅橡胶 HJN0901-15D 氟硅橡胶，耐高温400℃","只",1,"按合同要求交货","炼铁厂"]
[311,5500400033,"水渣渣浆泵;机械密封","MN206-100","100YTZX-500, 硬质合金","套",1,"按合同要求交货","炼铁厂"]
[312,7402000022,"离心水泵 机械密封","KQSN350-N4/693","P201","套",1,"按合同要求交货","炼铁厂"]
[313,7402700073,"热风阀方法兰密封圈","不锈钢包石墨；耐高温1200℃","1850*410*6","件",1,"按合同要求交货","炼铁厂"]
[314,5400300024,"煤气增压机 后端油封","AII850(M)型；NO.5101-02","锻件 材质：铝","付",1,"按合同要求交货","炼铁厂"]
[315,5500600054,"离心水泵 机械密封","KQSN350-M9/473","MG1/90-G60","套",1,"按合同要求交货","炼铁厂"]
[316,5500400029,"水渣循环泵;机械密封","250YTZX-650","MN206140 硬质合金","套",1,"按合同要求交货","炼铁厂"]
[317,7400100503,"轴流压缩机静叶承缸专用密封","包括：外径53*3.5的O型密封圈50个；外径42*3.5的O型密封圈190个；外径52*3.5的O型密封圈40个；外径51*3.5的O型密封圈45个；外径41*3.5的O型密封圈90个；外径32*3的O型密封圈260个","氟橡胶；耐高温≥300℃","套",1,"按合同要求交货","炼铁厂"]
[318,7402500010,"硅胶密封圈","电动插板阀CCF944X-0.5","DN2000用 硅橡胶 硅橡胶，4根/套，Q/HT3-2009","套",1,"按合同要求交货","炼铁厂"]
[319,5500100031,"一次均压阀密封圈","HNJ0901-15JP","DN300 氟硅橡胶 HNJ0901-15JP 氟硅橡胶，耐高温400℃","只",2,"按合同要求交货","炼铁厂"]
[320,7402500004,"硅胶密封圈","电动插板阀F941X-0.5-2000用","硅橡胶 硅橡胶，Q/HT3-2009","只",2,"按合同要求交货","炼铁厂"]
[321,5500100017,"上密轴密封外形圈/套环","M200-36/19","45# 钢调质 一套一个分油环 三个Yx密封 分油环尺寸：φ180*φ152*15","套",2,"按合同要求交货","炼铁厂"]
[322,7402700015,"金属包覆垫片","直径1684*直径1624*6 304/石墨橡胶+石墨 耐温≤300℃","304/石墨橡胶+石墨 GB/T15601-1995","片",2,"按合同要求交货","炼铁厂"]
[323,7402700019,"金属包覆垫片","直径2086*直径2026*6 304/石墨橡胶+石墨 耐温≤300℃","304/石墨橡胶+石墨 GB/T15601-1995","片",2,"按合同要求交货","炼铁厂"]
[324,7402700051,"金属包覆垫","1215*1300","压实厚度10mm;;耐温1200度;316不锈钢包石墨","片",2,"按合同要求交货","炼铁厂"]
[325,7402700052,"金属包覆垫","1220*1340","压实厚度10mm;;耐温1200度;316不锈钢包石墨","片",2,"按合同要求交货","炼铁厂"]
[326,5500100019,"上下密封阀密封圈","直径700mm","氟硅橡胶 JB/T5000.1-1998 氟硅橡胶，耐高温400℃","只",2,"按合同要求交货","炼铁厂"]
[327,7402700013,"金属包覆垫片","直径2180*2080*8","不锈钢 耐高温500℃，GB/T15601-1995","片",2,"按合同要求交货","炼铁厂"]
[328,7402700063,"金属包覆垫片","CSCLBXG1800-355/10mm","耐高温1200度","片",2,"按合同要求交货","炼铁厂"]
[329,7402500053,"热风炉热风阀体法兰密封垫圈","JSBFD1818.5",null,"只",3,"按合同要求交货","炼铁厂"]
[330,7402700012,"金属包覆垫片","直径1780*1690*8","不锈钢 耐高温500℃，GB/T15601-1995","片",4,"按合同要求交货","炼铁厂"]
[331,7401900140,"油封","490*550*25",null,"只",4,"按合同要求交货","炼铁厂"]
[332,7401900196,"油封","340X380X20",null,"只",4,"按合同要求交货","炼铁厂"]
[333,7402900016,"密封包","*","0-RING KIT/B-1","只",5,"按合同要求交货","炼铁厂"]
[334,7401900191,"骨架油封","310*370*25","AD5675A0;NOK","只",5,"按合同要求交货","炼铁厂"]
[335,7402700027,"金属包式垫片","直径1255*30*10 304/石棉橡胶+石墨","304/石棉橡胶+石墨 GB/T15601-1995","片",5,"按合同要求交货","炼铁厂"]
[336,7402700034,"金属包覆垫片","直径1300/1240*10","316不锈钢包石墨 GB/T4622.2-2003耐高温1304℃","片",5,"按合同要求交货","炼铁厂"]
[337,7402700070,"金属垫圈","1400*1490*厚度5mm","适用于煤气加压电动插板阀;DN1400;F944X","只",5,"按合同要求交货","炼铁厂"]
[338,7402800020,"盘根","CPS8900","14*14mm","Kg",5,"按合同要求交货","炼铁厂"]
[339,7402500059,"煤气加压电动敞开式盲板阀密封垫圈","DN1200;","F944X","只",5,"按合同要求交货","炼铁厂"]
[340,7402700014,"金属包覆垫","直径1333*直径1230*8 304/石墨橡胶+石墨","304/石墨橡胶+石墨 GB/T15601-1995","片",5,"按合同要求交货","炼铁厂"]
[341,7402500005,"硅胶密封圈","电动插板阀F941X-2.5-1600用","硅橡胶 硅橡胶，Q/HT3-2009","只",5,"按合同要求交货","炼铁厂"]
[342,7402900069,"仓门盖密封条","截面尺寸20*22",null,"米",5,"按合同要求交货","炼铁厂"]
[343,7402700033,"金属包覆垫片","直径210/160*10","316不锈钢包石墨 GB/T4622.2-2003耐高温1303℃","片",10,"按合同要求交货","炼铁厂"]
[344,7402900031,"硅酸铝石棉垫","直径420*直径240*厚度15","温度大于1200℃","片",10,"按合同要求交货","炼铁厂"]
[345,7402700003,"金属缠绕式垫片","直径680*直径600 厚度6mm 不锈钢 耐高温1200度","不锈钢 GB/T4622.2-2003","片",10,"按合同要求交货","炼铁厂"]
[346,7402700010,"金属包覆垫片","∮300*∮360*6","不锈钢 耐高温500℃，压实厚度6mm","片",10,"按合同要求交货","炼铁厂"]
[347,7402700036,"金属包覆垫片","直径325/285*10","316不锈钢包石墨 GB/T4622.2-2003耐高温1306℃","片",10,"按合同要求交货","炼铁厂"]
[348,7402800018,"碳纤维盘根","10*10",null,"Kg",10,"按合同要求交货","炼铁厂"]
[349,7402800002,"盘根","CPS7510 14*14mm","石墨","Kg",10,"按合同要求交货","炼铁厂"]
[350,7402500061,"金属垫圈","1000*1090*厚度5mm","适用于金属硬密封碟阀;D943P-2.5;DN1000","只",10,"按合同要求交货","炼铁厂"]
[351,7402800016,"石墨盘根","8*8","石墨","Kg",10,"按合同要求交货","炼铁厂"]
[352,7402700044,"金属硬密封垫圈","Q37F-16C","DN400","只",10,"按合同要求交货","炼铁厂"]
[353,7402800032,"盘根","CPS7600-10mm","10mm","Kg",10,"按合同要求交货","炼铁厂"]
[354,4000800865,"金属包覆垫","680*600*6","不锈钢耐高温1200度","个",10,"按合同要求交货","炼铁厂"]
[355,7402800014,"石墨盘根","P600110*10","石墨 耐温500℃","Kg",10,"按合同要求交货","炼铁厂"]
[356,7402700029,"金属包覆垫片","直径520*450*8","不锈钢 GB/T150601-1995","只",10,"按合同要求交货","炼铁厂"]
[357,7402400005,"阀门耐压密封垫","D343H400.10C-P","480*420*6;材质:1Cr18Ni9","片",10,"按合同要求交货","炼铁厂"]
[358,7402700002,"金属缠绕式垫片","直径575*直径485 厚度8mm 不锈钢 耐温1200度","不锈钢 GB/T4622.2-2003","片",10,"按合同要求交货","炼铁厂"]
[359,7402700037,"送风管道金属密封垫圈","CSCLBFD620-540/10","耐高温1200度","只",10,"按合同要求交货","炼铁厂"]
[360,7402900013,"密封填条","*","CSCL25GJKD18-HD12","米",10,"按合同要求交货","炼铁厂"]
[361,7402700062,"金属包覆垫片","315*705*375*8","耐温1200度","片",10,"按合同要求交货","炼铁厂"]
[362,7402700007,"金属包覆垫片","直径780/直径730 厚度8mm","不锈钢 耐温1200度","片",10,"按合同要求交货","炼铁厂"]
[363,7402700018,"送风管道金属密封垫圈","CSCLBFD530-630/10","耐高温1200度","只",10,"按合同要求交货","炼铁厂"]
[364,7402800030,"盘根","2300;","12*12;PTFE","Kg",10,"按合同要求交货","炼铁厂"]
[365,7402700030,"金属包覆垫片","直径1100/1000*10","316不锈钢包石墨 GB/T4622.2-2003耐高温1300℃","片",10,"按合同要求交货","炼铁厂"]
[366,7402700032,"金属包覆垫片","直径670/630*8","316不锈钢包石墨 GB/T4622.2-2003耐高温1302℃","片",10,"按合同要求交货","炼铁厂"]
[367,7402700035,"金属包覆垫片","直径 695/635*10","316不锈钢包石墨 GB/T4622.2-2003耐高温1305℃","片",10,"按合同要求交货","炼铁厂"]
[368,7402700066,"金属硬密封进出孔密封垫圈","HB2810-16K",null,"只",10,"按合同要求交货","炼铁厂"]
[369,7402700011,"金属包覆垫","直径800*直径880*5","316不锈钢包石墨 . 耐温250℃","片",10,"按合同要求交货","炼铁厂"]
[370,7402700065,"金属包覆垫片","直径915/直径820","厚度5mm 耐温1200度","片",10,"按合同要求交货","炼铁厂"]
[371,7402700028,"金属包式垫片","直径1290*30*10 304/石棉橡胶+石墨","304/石棉橡胶+石墨 GB/T15601-1995","片",10,"按合同要求交货","炼铁厂"]
[372,7402700069,"金属垫圈","1200*1290*厚度5mm","适用于加气出口金属碟形齿回阀;H47X-2.5;DN1200","只",10,"按合同要求交货","炼铁厂"]
[373,5500100029,"眼睛阀密封圈","直径345*直径16","氟硅橡胶 氟硅橡胶，耐高温400℃","只",10,"按合同要求交货","炼铁厂"]
[374,7402700068,"金属垫圈","1600*1690*厚度5mm","适用于煤气出口主管道电动扇形阀;D943P-2.5;DN1600","只",10,"按合同要求交货","炼铁厂"]
[375,7402500081,"弹性圈","∮90*∮22*30","材质:氟橡胶","只",10,"按合同要求交货","炼铁厂"]
[376,7402900062,"煤气阀凹形专用密封填条","16GJ15-9-13",null,"米",15,"按合同要求交货","炼铁厂"]
[377,7400700045,"活塞密封","RVE001400;140*155*34.0*6;NB83",null,"套",20,"按合同要求交货","炼铁厂"]
[378,7402900011,"密封填条","*","CSCL19R5-2FJ-26B 耐高温400度","米",30,"按合同要求交货","炼铁厂"]
[379,7402900012,"密封填条","*","CSCL13B-2GJ.13B耐高温400度","米",30,"按合同要求交货","炼铁厂"]
[380,7402600014,"视孔石墨成型环","直径35*20*5",null,"只",100,"按合同要求交货","炼铁厂"]
[381,7402500060,"橡胶平垫圈","直径65/直径48-5mm",null,"只",100,"按合同要求交货","炼铁厂"]
[382,7402700016,"金属包覆垫片","DN100，厚度4mm，外径154mm，内径100mm，耐温>500℃","碳钢 GB/T150601-1995","片",100,"按合同要求交货","炼铁厂"]
[383,7400100431,"硅胶O型密封条","直径7mm","Pg≥0.25MPa 温度≥300℃ 高炉煤气","米",80,"按合同要求交货","炼铁厂"]
[384,7402500006,"缠绕式密封垫圈","328*250*3.2",null,"只",15,"按合同要求交货","炼铁厂"]
[385,7402600015,"石墨垫片","CPS-316","不锈钢 直径180*140*3","片",65,"按合同要求交货","炼铁厂"]
[386,7402600036,"石墨垫片","CPS-316;不锈钢;直径670*600*3.5",null,"个",50,"按合同要求交货","炼铁厂"]
[387,4000800946,"金属包式垫片","直径1400","不锈钢","个",3,"按合同要求交货","炼铁厂"]
[388,5500100004,"二次均压阀密封圈","HJN0901-2J","DN150 氟硅橡胶 密封圈 HJN0901-2J 氟硅橡胶，耐高温400℃","只",3,"按合同要求交货","炼铁厂"]
[389,7401500064,"防尘圈","ES56151-0600-46-144-8307;60*68.8*6.3","60*68.8*6.3","只",5,"按合同要求交货","炼铁厂"]
[390,7402000026,"离心水泵 机械密封","KQSN600-N27/466","P206","套",1,"按合同要求交货","炼铁厂"]
[391,7402500064,"缠绕式密封垫圈","272*200*3.2",null,"只",30,"按合同要求交货","炼铁厂"]
[392,7402500082,"封阀板密封圈","670*790*38mm","耐高温500度，材质：硅橡胶","只",4,"按合同要求交货","炼铁厂"]
[393,7402600001,"缠绕式密封垫圈","465*400*3.2",null,"只",22,"按合同要求交货","炼铁厂"]
[394,7402700006,"金属包覆垫片","2790*1660*60 压实厚度8mm","不锈钢 耐温1200度 整体成型 外圆角半径90mm 内圆角半径36.5mm","片",5,"按合同要求交货","炼铁厂"]
[395,7402700042,"316不锈钢高温专用垫片","DN400","426/544 耐温>500℃","片",40,"按合同要求交货","炼铁厂"]
[396,7402700060,"316不锈钢高温专用垫片","DN350;377/476","耐温>500℃","个",25,"按合同要求交货","炼铁厂"]
[397,7402700077,"重力除尘放散阀密封圈","直径557*直径520","材质： 氟硅橡胶，耐高温400℃，厚度：13mm","个",1,"按合同要求交货","炼铁厂"]
[398,7402700080,"十字测温金属包覆垫片","直径503/直径445 压实厚度6mm","材质 :不锈钢 , 耐温1200度","片",5,"按合同要求交货","炼铁厂"]
[399,7402700083,"鹅颈管金属缠绕式垫片","直径540*直径620 压实厚度12mm","材质 :不锈钢 , 耐温1200度","片",5,"按合同要求交货","炼铁厂"]
[400,7402700085,"方形金属包覆垫片","1830*390*30*6","包覆垫片材质：904L不锈钢，填充料材质：陶瓷纤维，耐高温1300℃，方型金属垫包覆垫片应弧度圆角整体锻造，氩弧焊焊接，禁止直角锡焊，外圆角半径65mm，内圆角半径35mm","片",3,"按合同要求交货","炼铁厂"]
[401,7402700086,"方形金属包覆垫片","715*380*35*6","包覆垫片材质：904L不锈钢，填充料材质：陶瓷纤维，耐高温1400℃，方型金属垫包覆垫片应弧度圆角整体锻造，氩弧焊焊接，禁止直角锡焊，外圆角半径60mm，内圆角半径25mm","片",3,"按合同要求交货","炼铁厂"]
[402,7402700087,"金属包覆垫片","外径2340*内径2280*厚度6","包覆垫片材质：904L不锈钢，填充料材质：陶瓷纤维，耐高温1400℃","片",2,"按合同要求交货","炼铁厂"]
[403,7402800003,"盘根","CPS7510 16*16mm",null,"Kg",7,"按合同要求交货","炼铁厂"]
[404,7402800017,"石墨盘根","2101；20*20","石墨","Kg",5,"按合同要求交货","炼铁厂"]
[405,5100100038,"联轴器橡胶弹性体","80*150*230","新天然橡胶","只",20,"按合同要求交货","炼铁厂"]
[406,5100100039,"联轴器橡胶弹性体","*","120*170*60新天然橡胶","只",6,"按合同要求交货","炼铁厂"]
[407,7401900096,"骨架油封","SD300*340*18 NBR",null,"只",2,"按合同要求交货","炼铁厂"]
[408,7402000004,"机械密封","KL109-25","KL109-25","套",2,"按合同要求交货","炼铁厂"]
[409,7402000006,"机械密封","KL109-45","KL109-45","套",2,"按合同要求交货","炼铁厂"]
[410,7402700041,"金属包覆垫片","DN350",null,"片",35,"按合同要求交货","炼铁厂"]
[411,7402700067,"316不锈钢高温专用垫片","DN300;","325/416;耐温>500℃","片",60,"按合同要求交货","炼铁厂"]
[412,7402700084,"金属包覆垫片","760*860*8","不锈钢 耐高温500-600℃，压实厚度8mm","片",5,"按合同要求交货","炼铁厂"]
[413,7402800007,"石墨盘根","10*10","石墨","Kg",100,"按合同要求交货","炼铁厂"]
[414,7402900066,"硅橡胶密封圈","SF-X-360-05","耐高温硅橡胶（170-350℃）；φ365*18","只",2,"按合同要求交货","炼铁厂"]
[415,7402500008,"缠绕式密封垫圈","92*40*3.2",null,"只",30,"按合同要求交货","炼铁厂"]
[416,7402700024,"316不锈钢高温专用垫片","DN50 57/107 耐温>500℃",null,"片",50,"按合同要求交货","炼铁厂"]
[417,7402700025,"316不锈钢高温专用垫片","DN65 76/127 耐温>500℃",null,"片",50,"按合同要求交货","炼铁厂"]
[418,7402700031,"金属包覆垫片","直径1360/1290*10","316不锈钢包石墨 GB/T4622.2-2003耐高温1301℃","片",10,"按合同要求交货","炼铁厂"]
[419,7402700045,"316不锈钢垫片","直径65*直径35*3","16Kg/cm2","片",100,"按合同要求交货","炼铁厂"]
[420,5500200001,"风筒，直吹管含锆硅酸铝纤维棉垫","直径460*直径220mm,厚13mm","硅酸铝 耐高温1200℃","件",50,"按合同要求交货","炼铁厂"]
[421,7402900014,"含锆硅酸铝纤维棉垫","直径550*直径230mm,厚13mm",null,"件",100,"按合同要求交货","炼铁厂"]
[422,7001800116,"离心水泵 机械密封","SBS200-420E/415",null,"套",1,"按合同要求交货","能源厂"]
[423,7402000002,"离心水泵 机械密封","SBS125-230E",null,"套",1,"按合同要求交货","能源厂"]
[424,5400100046,"离心式空压机 中冷橡胶密封条","FS-ELLIOTT 260","铸造 氟橡胶，耐温大于250℃","只",1,"按合同要求交货","能源厂"]
[425,7001200277,"高压泵;高压密封组","L-NYL01.01.02","内径83；铜件+密封件","件",1,"按合同要求交货","能源厂"]
[426,7001800103,"离心水泵 机械密封","MTN-70",null,"套",1,"按合同要求交货","能源厂"]
[427,7402000007,"离心水泵 机械密封","SBS150-605F/523",null,"套",1,"按合同要求交货","能源厂"]
[428,5400100032,"离心式空压机 密封套件","FS-ELLIOTT 5件套","铸造 6\",8\"×2,10\",16\",氟橡胶，耐温大于250℃","套",1,"按合同要求交货","能源厂"]
[429,7402000052,"机械密封","MN206-110","100YTZX-560，硬质合金","套",1,"按合同要求交货","能源厂"]
[430,7402000015,"离心水泵 机械密封","SBL150-250IA","(内径：45mm)","套",2,"按合同要求交货","能源厂"]
[431,7402000016,"离心水泵 机械密封","SBL250-315A","（内径50）","套",2,"按合同要求交货","能源厂"]
[432,7402000036,"水泵机械密封","40ZW20-15","电机功率：15KW；电压：380V；流量22t/h;扬程40米;口径50mm","套",2,"按合同要求交货","能源厂"]
[433,7402000013,"离心水泵 机械密封","SBS350-360E/357",null,"套",2,"按合同要求交货","能源厂"]
[434,7402000010,"离心水泵 机械密封","SBS200-420E/415",null,"套",2,"按合同要求交货","能源厂"]
[435,7402500035,"电动盲板阀密封","F943X-1.6C","DN500","套",2,"按合同要求交货","能源厂"]
[436,7402000009,"离心水泵 机械密封","SBS200-320E/314",null,"套",2,"按合同要求交货","能源厂"]
[437,7402000029,"水泵机械密封","SLOW200-660C",null,"套",2,"按合同要求交货","能源厂"]
[438,7402000035,"机械密封","MTN-50","电机功率：15KW；电压：380V；流量22t/h;扬程40米;口径65mm","套",2,"按合同要求交货","能源厂"]
[439,7402000011,"离心水泵 机械密封","SBS300-435F/450",null,"套",2,"按合同要求交货","能源厂"]
[440,7402100040,"高压密封组件","A-36/20.02.01.02",null,"套",2,"按合同要求交货","能源厂"]
[441,7402000003,"离心水泵 机械密封","SBS150-360F",null,"套",2,"按合同要求交货","能源厂"]
[442,7402000001,"离心水泵 机械密封","KQSN250-M6/410","离心水泵 机械密封 KQSN250-M6/410 MG1/80-G60","套",2,"按合同要求交货","能源厂"]
[443,7001800301,"管道泵 机械密封","40GB-A",null,"套",5,"按合同要求交货","能源厂"]
[444,5100100456,"联轴器弹性圈","NUP285-130513","材质:聚氨酯;外径40mm,内径20mm,长度40mm;用于1#、2#、3#煤气加压机新弹性套柱销联轴器","只",20,"按合同要求交货","能源厂"]
[445,7402500037,"密封垫圈","BXGJS1103295","耐高温500℃；不锈钢","片",10,"按合同要求交货","能源厂"]
[446,7402500062,"密封垫","BJLM-100","DN100；硅橡胶；使用温度100度； 压力；PN10","只",5,"按合同要求交货","能源厂"]
[447,7402700053,"金属硬密封煤气除尘人孔密封垫圈","HZ60-180/B","规格890*800","只",5,"按合同要求交货","能源厂"]
[448,7402500038,"高压密封垫","GJLH20026045","耐高温500℃；不锈钢","片",10,"按合同要求交货","能源厂"]
[449,7402800019,"盘根","CPS2113F;8*8","石墨；耐高温500℃","Kg",10,"按合同要求交货","能源厂"]
[450,7402700054,"煤气管道金属硬密封垫圈","DN500","不锈钢;直径560*500*3.2","片",10,"按合同要求交货","能源厂"]
[451,7402500040,"下锅筒密封圈","2.95395E+12","耐高温500℃；不锈钢","片",10,"按合同要求交货","能源厂"]
[452,7402500039,"上锅筒密封圈","3.2542E+12","耐高温500℃；不锈钢","片",10,"按合同要求交货","能源厂"]
[453,7402600024,"高温高压石墨垫片","CSCLS3000","耐高温500℃；不锈钢;厚3mm","片",10,"按合同要求交货","能源厂"]
[454,7402500036,"高温密封圈","CLBF45420500","耐高温500℃；不锈钢;直径500*420*45*3.2","片",10,"按合同要求交货","能源厂"]
[455,7402900061,"耐压水密封组件","A550-V1521-2VING，","夹门密封，材质：聚氨酯组合不锈钢，长2.6米，可自由弯曲","套",10,"按合同要求交货","能源厂"]
[456,7402800038,"耐高温陶瓷钎维盘根","带不锈钢丝;12mm*12mm",null,"Kg",10,"按合同要求交货","能源厂"]
[457,5400300011,"煤气增压机 油封","AIS750.3-2","锻件 材质：铝","只",3,"按合同要求交货","能源厂"]
[458,7402600054,"316不锈钢椭圆石墨垫片","460/φ400*360/300*3.2",null,"片",4,"按合同要求交货","能源厂"]
["注：1、投标报价含税，税率13% ；                                                                                                 \n2、生产厂家要求全称填写准确无误 ；                                                                                       \n3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）"]
[]
["投标人：                         （盖单位公章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日  期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2023年10月-2024年9月密封年度采购项目            项目编号：HGJY-G2023161"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位公章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日  期：      年      月      日                "]