{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":24,"n_cols":13,"rows_kept":24,"merged":[[0,0,0,12],[1,0,1,12],[20,0,20,8],[21,0,21,8],[22,0,22,8],[23,0,23,8]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2023年10月电磁备件采购项目                     项目编号：HG JY-G2023164"]
["标包号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,4100400043,"电缆卷筒","JTA135-20-2 220V 135A","220V 135A 电缆长度20米双通道","台",1,null,"炼钢厂部","2023-11-10"]
[2,5800200027,"吸盘链条","MW929-165100L/G-75",null,"付",16,"GB5802-1986","炼钢厂部","2023-12-11"]
[3,5300101006,"吸盘链条","16t+16t;MW42-155110L/G吸盘专用","主环∮45;链环∮35;MW42-155110L/G吸盘专用","付",2,null,"340热轧","2023-12-11"]
[4,5300800011,"稀土永磁除铁器","YC12-110130-X","皮带宽度B=1000mm；驱动电机功率4KW,自重2100kg；标准架设高度300mm","台",1,"GB/T4307-2005","原料工段","2023-12-11"]
[5,6000400007,"电磁吸盘","MW929-420400L/G",null,"台",1,"JB/T10577-2006","720厂部","2023-12-11"]
[6,4100400042,"电缆卷筒","JTA100-25-2-Ⅱ","容量100A 电缆长度25米2通道 外置滑环","台",1,"JT/T806.4-2011","炼钢厂部","2023-12-11"]
[7,6100900165,"停电保磁控制柜","SH22058","额定输出电压DC220V;额定电流100A","台",1,"GB7251.1-2005","炼钢厂部","2023-12-11"]
[8,6100900162,"智能控制板","ZKDQ-EIectromagnet-Con-V1.0","15路输入;9路输出","块",1,"IPC-6012","炼钢厂部","2023-12-11"]
[9,6100900163,"保护板","ZKDQ-EIectromagnet-RC-V1.0","AC380/DC220V","块",1,"IPC-6012","炼钢厂部","2023-12-11"]
[10,6100900164,"电源板","ZKDQ-EIectromagnet-Power-V1.0","输入电压AC380V/DC220V;输出电压DC24V","块",2,"IPC-6012","炼钢厂部","2023-12-11"]
[11,6200200922,"整流模块","MDK135A/2200V","额定电流135A;耐压2200V","块",10,"GB/T17761-2018","炼钢厂部","2023-12-11"]
[12,6200200923,"整流模块","MFC(TD)90A/1800V","额定电流90A;耐压1800V","块",10,"GB/T17761-2018","炼钢厂部","2023-12-11"]
[13,6100900144,"数显板","QLWKV3016","AC220V","块",2,"JB/DQ4509-2003","炼钢厂部","2023-12-11"]
[14,4100700195,"晶闸管","QLKKTC20V20XP","电流200A;耐压2000V","个",2,"JB/DQ4509-2003","炼钢厂部","2023-12-11"]
[15,6100100220,"电磁吸盘变压器","ZSG-60","输入电压;AC380V;输出电压;DC230V;功率;60KVA;全铜绕线","台",2,"GB/T18494.1-2014","炼钢厂部","2023-12-11"]
[16,4100400042,"电缆卷筒","JTA100-25-2-Ⅱ","容量100A 电缆长度25米2通道 外置滑环","台",2,"JT/T806.4-2011","炼钢厂部","2023-12-11"]
[17,4100400047,"电缆卷筒弹簧","JTA100-25-2-Ⅱ","JTA100-25-2-Ⅱ型电缆卷筒用弹簧","只",4,"JT/T806.4-2011","340热轧","2023-12-11"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2023年10月电磁备件采购项目        项目编号：HG JY-G2023164"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}