{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表","Sheet1"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":18,"n_cols":13,"rows_kept":18,"merged":[[0,0,0,12],[1,0,1,12],[14,0,14,8],[15,0,15,8],[16,0,16,8],[17,0,17,8]],"flags":["formulas_cached_only"]}
["（一）开标一览表"]
["项目名称：2023年11月电磁备件采购项目              项目编号：HGJY-G2023183"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","生产厂家","备注"]
[1,5300600117,"电缆卷筒弹簧","1.6*40*22000","直径340mm，单层厚度1.6mm，宽度40mm，长度22m，合金弹簧钢","个",1,"Q/0100 ANY006—2019 GB/T 1222-2016","检验检测中心","2023-12-12"]
[2,6100900145,"多功能智能控制板","MFCHARGE","输入电压AC/DC110~245V;AO输出DC12V; 0~10V;DI输入;6输入;DO输出;6输出","块",1,"GB/T16261-1996","炼钢厂部","2023-12-12"]
[3,6100900146,"主控板","MFMC-200","输入电压AC/DC;110~245V;AO输出DC12V; 0~10V;DI输入;12输入;DO输出：8输出","块",1,"GB/T16261-1996","炼钢厂部","2023-12-12"]
[4,6100900147,"智能脉冲控制板","QLWKV3009","输入电压AC220V;输出;脉宽调制10路;AI输入;1路;DI输入;2路;DO输出;1路","块",1,"GB/T16261-1996","炼钢厂部","2023-12-12"]
[5,4100400047,"电缆卷筒弹簧","JTA100-25-2-Ⅱ","JTA100-25-2-Ⅱ型电缆卷筒用弹簧","只",4,"JT/T806.4-2011","340热轧","2024-01-11"]
[6,5601800021,"气管卷筒","QJDF-50/20","卷取长度20m;最大力矩252N*m;气压2MPa:重量380Kg;带力矩电机及减速机","台",1,"JT/T806.4-2011","炼钢厂部","2023-12-27"]
[7,5300100522,"吸盘链条","20t+20t",null,"条",4,"GB5802-1986","炼钢厂部","2024-01-11"]
[8,5300100523,"吸盘链条","7.5t+7.5t","1.1米/根","根",16,"GB5802-1986","炼钢厂部","2024-01-11"]
[9,6000400085,"起重电磁铁","MW42-140140YL/2-75","额定电流55A;额定电压DC220V;功率12.1Kw 重量5000Kg","台",2,"JB4315-86","炼钢厂部","2023-12-27"]
[10,6100900166,"吸盘控制设备","ZKBP1-B-120A/C-N","输入电源AC380V 输出电源DC220V 输出电流DC120A;停电保磁时间30min","台",1,"JB4315-86","炼钢厂部","2023-12-27"]
[11,4100400286,"电缆卷筒","JTA25-15/3","3通道，电流25A，3*6平方电缆，长度15米，水平地面安装，弹簧式收缩卷筒","台",2,"JB/T11864-2014","340管加工热处理","2023-12-28"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2023年11月电磁备件采购项目              项目编号：HGJY-G2023183"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"Sheet1","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}