{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":19,"n_cols":14,"rows_kept":19,"merged":[[0,0,0,8],[1,0,1,13],[15,0,15,8],[16,0,16,8],[17,0,17,8],[18,0,18,8]],"flags":["formulas_cached_only"]}
["                            （一）开标一览表"]
["项目名称：2024年1月机械备件采购项目Ⅱ              项目编号：HGJY-G2024015"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","执行标准","申请部门","交货期","含税单价（元）","标包合价（含税）","生产厂家","备注"]
[1,null,"炮雾机","射程60米","AC380;50HZPLC变频控制;","台",6,"详见技术规格书","炼钢厂6#连铸机铸坯质量保障性改造项目","2024-02-27"]
[2,6700400073,"制样粉碎机","F97-3",null,"台",1,"物流中心","DZ/T0015-1991","2024-03-12",null,null,"江西通用"]
[3,5500300122,"凿岩机钻杆连接套筒","LDJH400.01.05-GJ01","材质42CrMo锻件,整体调质处理，硬度HRC55-60，波型螺纹B62，凿岩机配套使用，带密封件及密封阀芯","套",4,"高炉","GB/T19001-2000","2024-03-13"]
[4,5500300123,"开口机挂钩装置","SLHG30.03-01","整体式挂钩材质Q355B，销轴材质45#钢调质处理，包含蝶形弹簧、紧固件等，底座焊接完成后上铣床加工，变形量小于1mm，重量253.5Kg","套",2,"高炉","JB/T12471-2015","2024-03-13"]
[5,7102300006,"磨机双阀板排渣阀","TJDF25","阀体：球墨铸铁QT450，密封面材质：硬质合金YG8，阀板材质：45#锻钢。 含气动执行机构，快排阀组件，机械式防爆限位开关，所有电气设备满足煤粉粉尘防爆要求。","台",1,"高辅工段","审核图纸","2024-03-13"]
[6,7502600008,"横流式冷却风机","GFDD570-220","电压：220V；电流1.4A；频率：50Hz；功率270W；风量：3200m3/h；重量12kg.","台",5,"炼铁厂部",null,"2024-03-13"]
[7,7102100010,"气动控制阀门","D376XE69",null,"只",5,"180热轧","ISO5211","2024-03-12"]
[8,7102100012,"气动控制阀门","D376XE71",null,"只",5,"180热轧","ISO5211","2024-03-12"]
[9,7102100013,"气动控制阀门","D376XE72",null,"只",5,"180热轧","ISO5211","2024-03-12"]
[10,5718600027,"直通叶轮视镜","SG-YL11-21内螺纹G3/8 ；     304不锈钢","304不锈钢","件",10,"340管加工热处理","HG501-86","2023-12-28"]
[11,7501300134,"吸振型膨胀节DN300","2.5XB300-F","不锈钢 50kg  PN2.5MPa","套",2,"89管加工热处理","审核图纸","2024-04-12"]
[12,5501800038,"块矿筛下层筛板","B=2038",null,"套",3,"原料工段","审核图纸","2024-03-13"]
["注：1、投标报价含税，税率13%                                                                                     2、生产厂家要求全称填写准确无误"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":22,"n_cols":4,"rows_kept":22,"merged":[[0,0,0,3],[1,0,1,3],[3,0,6,0],[3,3,6,3],[7,0,17,0],[7,3,17,3],[18,0,18,3],[19,0,19,3],[20,0,20,3],[21,0,21,3]],"flags":["formulas_cached_only"]}
["                   （二）商务/技术偏离表"]
["项目名称：2024年1月机械备件采购项目Ⅱ      项目编号：HGJY-G2024015"]
["偏离类型","序号","招标内容","偏离内容"]
["商务偏离"]
[]
[]
[]
["技术偏离"]
{"$rows_empty":10}
["注：1、如商务无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容有序对应填写，后在偏离内容栏中按序号顺序填写准确清楚。\n    2、如技术无偏离则在偏离内容填写”无”。如有偏离先按序号和招标内容（物料描述、标准、交货期等内容）有序对应填写，后在偏离内容栏中按对应序号顺序填写准确清楚。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]