{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Macro1","一、开标一览表","二、商务 技术偏离表"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Macro1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"一、开标一览表","index":1,"n_rows":25,"n_cols":12,"rows_kept":25,"merged":[[0,0,0,11],[1,0,1,11],[21,0,21,11],[22,0,22,11],[23,0,23,11],[24,0,24,11]],"flags":["formulas_cached_only"]}
["    （一）开标一览表"]
["项目名称：2024年2月电动机招标采购项目                      项目编号：HGJY-G2024022"]
["序号","资材编号","资材名称","规格描述","技术参数","单位","数量","交货时间","使用部门","含税单价(元)","生产厂家\n","备注   "]
[1,"6000201115","交流伺服电机","130SJT-M050D(A4II)","输入电压AC220V三相, 额定功率1.5Kw; 额定电流6A ; 额定转矩6NM ; 额定转速2500rpm ; 最高转速3000rpm","台","1","2024.4.25","检验检测中心"]
[2,"6000201169","液压内轴电机","C05-43BO 5HP","额定电压：380VAC   额定电流：8.6A     额定转速：1420rpm  额定功率：3.75KW","台","1","2024.4.25","检验检测中心"]
[3,"6000201170","三相交流异步电动机","M2BAX 112MA4","额定功率：4KW      额定电流：8.46A    额定转速1433rpm IP55 卧式","台","1","2024.4.25","检验检测中心"]
[4,"6000201203","变频调速三相异步电动机","YTSZ315M1-4","额定功率160KW,额定电压380V，额定电流294A,额定转速1485r/min,恒转矩范围0-50HZ，恒功率范围50-100HZ,绝缘等级F，IP54,","台","1","2024.4.25","89管加工热处理"]
[5,"6000201023","起重及冶金用绕线转子三相异步电动机","YZR355L1-10C;110Kw","定子电压380V;223A;转子电压362V;189A ;S3-40%;H级绝缘;IP54;接法Y;转速586r/min;带超速开关","台","1","2024.4.25","炼钢厂部"]
[6,"6000300276","变频调速三相异步电动机","YTSZ315M2-10","功率：90KW;196A;额定转速:585rpm;防护等级:IP55;绝缘等级：H级;频率:50HZ;接线方式:三角形;厂家:大连第二电机厂","台","1","2024.4.25","340热轧"]
[7,"6000201161","YD低速电动机","YD 90","额定功率0.3Kw;额定电压380V;额定电流1.3A;额定转速1.2r/min;额定转矩650N.m;防护等级IP54;绝缘等级F级;安装方式B5;带抱闸","台","1","2024.4.25","炼钢厂部"]
[8,"6000200250","交流电动机","YSPA90L4-1.5Kw","AC380V B级 IP44 IM B5 接线 Y 接线盒位置R(右) 3.7A 定额S1 1400r/min 标准编号 JB/T1009-2007","台","2","2024.4.25","340热轧"]
[9,"6000201116","交流异步电动机","BPYXKK500-6W","功率1250Kw;额定电压6000V;额定电流146A;额定频率50Hz;绝缘等级F级;防护等级IP54;转速990r/min;S1工作制;Y型接法;冷却方式IC616","台","1","2024.4.25","炼钢厂部"]
[10,"6000201167","三相异步电动机","1TL0001-3AD63-3AA4-Z;315L","额定功率110Kw;额定电压380/660V;额定电流220/127A;额定转速741r/min;绝缘等级:F级;防护等级IP55;安装方式B3;三角型接法","台","1","2024.4.25","炼钢厂部"]
[11,"6000201172","冷却塔三相异步电动机","YLT225M-10","额定功率15Kw;额定电压380V;额定频率50Hz;额定电流35.1A;防护等级IP55;S1工作制;绝缘等级F级;额定转速580r/min;三角接法;安装方式B5","台","2","2024.4.25","炼钢厂部"]
[12,"6000201194","三相异步电动机","1TL0001-1EA23-3JB4-Z","功率22Kw;IM;B35;额定电压380/660V;电流42.0/24.0A;频率50Hz;EFF91.6%;COSφ0.87;Th.CL;155（F）;转数2935r/min;IP55;配G-180A型独立风扇","台","1","2024.4.25","炼钢厂部"]
[13,"6000201193","变频调速三相异步电动机","YPG132S-4-M1-R;4KW;带小齿轮","额定电压380V;额定电流9.7A;50HZ;额定转速1455r/min;H级; IP55;Δ型接线方式 ;S4;恒转矩3-50HZ;恒功率50-100HZ;出厂序列号1100078341/1:；小齿轮安装方式采用止动垫圈加锁紧螺母方式。","台","4","2024.4.25","180热轧"]
[14,"6000201191","异步交流电动机","YGM2-180L-4; 22KW","额定电压380V ; F级 IP54 安装方式B5; △型接线方式 ;42.9A 1470r/min ;接线盒在电机左侧线洞朝下.","台","1","2024.4.25","180热轧"]
[15,"6000201192","三相异步电动机","YE3-132M1-6；4KW","额定电压380V;额定电流9.46A;额定转速970r/min;F级 IP55 ; 50HZ;Δ型接线方式 ;功率因数0.74;效率85.8%","台","1","2024.4.25","180热轧"]
[16,"6000201214","三相异步电动机","YE4-200L-4；安装方式:B35","30KW 安装方式:B35 额定转速1470r/mi;三角型接法;电压380V;防护等级IP55;功率因素0.85;绝缘等级:F S1工作制","台","1","2024.4.25","炼铁厂部"]
[17,"6000201208","三相异步电动机","YE4-315L1-4；安装方式:B3","安装方式:B3额定功率:160KW;额定电压:380V;额定电流:288A;额定转速:1470rpm;绝缘等级:H级;防护等级:IP44;;频率:50HZ","台","1","2024.4.25","炼铁厂部"]
[18,"6000201219","防爆电动机","YB2-90S-4","1.1KW  B5  1390r/min  2.9A 380V 50Hz 0.77 Y型接线","台","1","2024.4.25","炼铁厂部"]
["注：1、投标报价含税，税率13% ；                                                                                                                2、生产厂家要求全称填写准确无误 ；                                                                                                               3、每个单项只允许一个有效报价，须按此表顺序与格式填报，不得打乱报价顺序（未报价的行、列不得删除）；"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]

{"sheet":"二、商务 技术偏离表","index":2,"n_rows":18,"n_cols":4,"rows_kept":18,"merged":[[0,0,0,3],[1,0,1,3],[3,0,5,0],[3,3,5,3],[6,0,13,0],[6,3,13,3],[14,0,14,3],[15,0,15,3],[16,0,16,3],[17,0,17,3]],"flags":["formulas_cached_only"]}
["   （二）商务/技术偏离表"]
["项目名称：2024年2月电动机招标采购项目                      项目编号：HGJY-G2024022"]
["偏离类型","序号","招标方要求内容","投标方偏离内容"]
["商务偏离"]
[]
[]
["技术偏离"]
{"$rows_empty":7}
["注：1、如商务无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标方要求内容有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n    2、如技术无偏离则在偏离内容单元格中填写”无”。如有偏离按序号和招标内容（规格描述、技术要求及标准、交货期等内容）有序对应填写，后将本单位偏离内容按序号顺序填写在一个单元格中。\n"]
["投标人：                         （盖单位章）                    "]
["法定代表人或其委托代理人：        （签字或盖章）              "]
["日    期：      年      月      日                "]